Aero Vodochody L-29 Delfin — l-29shortchecklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

PARTIAL POWER FAILURE < 500 Ft.:-  [EMERGENCY]
[ ]  1. Isolation Switch .... ON
[ ]  2. Throttle to RPM .... SLOW

PARTIAL POWER FAILURE 500 - 12,000 Ft.:-  [EMERGENCY]
[ ]  1. Throttle .... IDLE
[ ]  2. Isolation Switch .... ON
[ ]  3. Power .... SET

PARTIAL POWER FAILURE >12,000 Ft.:-  [EMERGENCY]
[ ]  1. Throttle .... IDLE
[ ]  2. Isolation Switch .... ON
[ ]  3. INCREASE Power IMMEDIATELY To:-
NOTE: (a) 60% 12,000 - 18,000 Ft.
NOTE: (b) 80% > 18,000 Ft
NOTE: N.B. WITH AFRCU ISOLATED, MAKE ALL CHANGES VERY SLOWLY (NO RPM LIMITER).

LOW PRESSURE FUEL or OIL:-  [EMERGENCY]
[ ]  1. Engine Switch & C.Bs .... CHECK
[ ]  2. SEC ‘B’ switch .... Cycle
[ ]  3. Power .... 85% (Max Oil) 94% (Max Fuel)
[ ]  4. Once Set AVOID Throttle Movement & RTB..
NOTE: N.B. Oil Pressure BELOW 1.2kg/cm for 2 Mins., RTB as Above.

EMERGENCY UNDERCARRIAGE LOWERING:-  [EMERGENCY]
(A)
[ ]  1. Hydraulic Circuit .... BLEED (Cock on LEFT)
[ ]  2. Gear & Flaps Normally .... LOWER
NOTE: IF This FAILs Then do (b).
(B)
[ ]  1. BELOW 250 K., 100 bar .... CHECK
[ ]  2. SEC ‘B’ switch Cycle & C.Bs.
[ ]  3. Emg. Hand Valve .... OPEN
[ ]  4. LEAVE U/C DOWN

EMERGENCY FLAP LOWERING:-  [EMERGENCY]
[ ]  1. C.Bs. & SEC. ‘B’ .... CHECK
[ ]  2. 250 K, Hand Valve .... OPEN

RELIGHT - HOT START:-  [EMERGENCY]
[ ]  1. Throttle .... CLOSE
[ ]  2. Air Start .... PRESS
IF NO GO:-
[ ]  3. HP Cock - OFF, Air Start .... OFF
[ ]  4. 30 - 40 Seconds .... WAIT
[ ]  5. N.E. Electrics .... OFF

RELIGHT - COLD START:-  [EMERGENCY]
[ ]  1. Throttle .... CLOSED
[ ]  2. 250 K - NE Electrics .... OFF
[ ]  3. C.Bs - LIVE - 10-15% WINDMILL.
[ ]  4. AirStart .... PUSH
[ ]  5. HP Cock - ON - AirStart .... OFF
NOTE: N.B. IF Windmilling BELOW 10% USE Ground Start.

ENGINE FIRE:-  [EMERGENCY]
[ ]  1. Throttle .... CLOSED
[ ]  2. HP Cock .... OFF
[ ]  3. SPEED to HEIGHT.
[ ]  4. BELOW 240 K - Fire Button .... PRESS
[ ]  5. NO RELIGHT.

GENERATOR FAILURE:-  [ABNORMAL]
[ ]  1. Switches & C.Bs .... CHECK
[ ]  2. Load .... REDUCE & RTB
NOTE: N.B. After 20 Minutes EXPECT EMG. U/C & FLAPS

Warning lights panel
WARNING LIGHTS PANEL
NOTE: FIRE- -----LOW FUEL------
NOTE: GENERATOR
NOTE: U/C----FUEL PUMP (LP PUMP) ---
NOTE: RELIGHT
NOTE: EXT. TANKs -- ISOL V. ---LOW CAB.PR.
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