Aero Vodochody L-29 Delfin — L29CHECKLIST
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "AFTER ENTERING THE COCKPIT" item count differs between passes (44 vs 21); verify nothing was dropped.
content_gap: Section "LANDING" item count differs between passes (21 vs 2); verify nothing was dropped.

INTERIOR INSPECTION R/C (for solo flight)
[ ]  Ejection seat .... secured
[ ]  Safety pins .... installed
[ ]  Parachute .... removed or secure
[ ]  Harness and lap belt .... secure
[ ]  ISOLATION VALVE Switch .... off
[ ]  FIRE EXT cover .... safety wired
[ ]  F/C STAT PRESS Lever .... NORMAL safety wired
[ ]  F/C DYN PRESS Lever .... NORMAL safety wired
[ ]  F/C ATT IND BANK Switch .... NORMAL
[ ]  F/C ATT IND PITCH Switch .... NORMAL
[ ]  LANDING LIGHT Switch .... NORMAL
[ ]  F/C LDG GEAR LOCK OUT .... OFF
[ ]  RAM AIR shut off lever .... CLOSED
ENGINE+FUEL GAGES
[ ]  Priority switch .... F/C
[ ]  EXT STORES JETTISON .... safety wired
[ ]  SEC B switch .... ON
[ ]  MASTER switch .... ON
[ ]  ICS switches--(avionics--) .... AS REQUIRED
[ ]  EMERG BRAKE .... OFF, safety wired
[ ]  Pressure gauges .... proper reading
[ ]  Hand valves .... closed, safety wired
[ ]  Canopy .... closed
[ ]  External CABIN SEAL lever .... INFLATE

AFTER ENTERING THE COCKPIT
[ ]  Parachute and harness .... tight and secure
[ ]  Shoulder harness lock .... as required
[ ]  Rudder pedals .... as required
[ ]  Oxygen equipment .... connect and hooked to
LEFT CONSOLE CHAIN
[ ]  Oxygen panel .... check pressure
[ ]  Emergency lever (RED) .... NORMAL
[ ]  Diluter demand lever (WHITE) .... NORMAL OXYGEN
[ ]  Supply lever (GREEN) .... ON
[ ]  CAB PRESS DUMP valve .... closed (CW)
[ ]  FIRE COCK LEVER .... OPEN, safety wired
[ ]  HYD DUMP VALVE lever .... CLOSED safety wired
[ ]  Throttle position .... idle
[ ]  Throttle friction .... as required
[ ]  FUEL SHUT OFF lever .... CLOSED
[ ]  DE-ICING lever .... OFF
[ ]  PNEU FILL DE -PRESS .... CLOSED (CW)
[ ]  ISOLATION VALVE switch .... OFF
[ ]  AIR START button .... covered, safety wired
[ ]  FIRE EXT COVER .... safety wired
[ ]  PITOT BOOM .... RIGHT safety wired
[ ]  PARACHUTE .... NO DELAY LANYARD ATT
INSTRUMENT PANEL
[ ]  TAXI LIGHT switch .... OFF
[ ]  LANDING LIGHT switch .... OFF
[ ]  HP OXYGEN indication .... check min 100 kg's
[ ]  LDG GEAR buttons .... check out
[ ]  All instrument readings .... normal
[ ]  EXT STORES switch .... SAFE, safety wired
[ ]  EXT TANKS switch .... OFF
[ ]  Arming switch .... BLANK
[ ]  RAM AIR shut off lever .... as required
RIGHT CONSOLE
[ ]  Electrical switches .... OFF
[ ]  EMERG BRAKE lever .... OFF, safety wired
[ ]  VHF & AVIONICS .... ALL OFF
[ ]  ICS panel --(avionics--) .... as required
[ ]  EMERG GEAR EXTENSION valve .... Closed, safety wired
[ ]  EMERG FLAP EXTENSION valve .... Closed, safety wired
[ ]  CABIN PRESS/ HEATING .... OFF
[ ]  CABIN HEAT .... AUTOMATIC
[ ]  Inverter select switch .... MAIN INV (down)
[ ]  All C/B's .... ON (in)
[ ]  Ejection pins .... in sockets

BEFORE STARTING ENGINE
[ ]  Helmet .... on
[ ]  Oxygen hose .... connect
[ ]  Radio cable .... connect
[ ]  Oxygen check .... complete
[ ]  Brake check .... 4kg/cm2
[ ]  Control stick and rudder .... free and correct movement
[ ]  BATT switch .... ON
[ ]  VOLT/AM METER check button .... depress, 24v
[ ]  COMMS switch .... master on
[ ]  Intercome .... check
[ ]  External power unit .... connect
[ ]  APU ON light (green) .... illuminated
[ ]  VHF radio .... ON
[ ]  Start up clearance .... request
[ ]  GEN switch .... ON
[ ]  ENG switch .... ON
[ ]  C&W panel .... push to test, all lights
[ ]  Electrical gear position indicators .... push to test, all red lights illuminated

ENGINE START
CAUTION: Be sure that the danger areas are clear before starting.
[ ]  GENERATOR light .... blinking
[ ]  DO NOT START light .... OUT
[ ]  GND START button .... depress for 3 sec
[ ]  Spark plugs igniting .... listen for sparking
[ ]  Throttle .... idle
[ ]  FUEL SHUT-OFF lever .... fully OPEN
[ ]  EGT (APU 700 degrees
BATT 750 degrees) .... keep manually within
[ ]  Fuel/ oil pressure .... rising limits
[ ]  Idle RPM .... 35% within 60 sec's
[ ]  APU .... disconnect
[ ]  Fuel pressure .... 12 kg's
[ ]  Oil pressure .... 0.5 kgs
[ ]  EGT (idle) .... 550'c MAX
[ ]  GENERATOR light .... out

FALSE START/ HOT START  [ABNORMAL]
CAUTION: Stop the engine immediately if one of the following occurs
NOTE: - no sparking of spark plugs
NOTE: - No oil pressure indication
NOTE: - EGT exceeds 750’c
NOTE: The engine must be stopped if there is;
NOTE: - no RPM rise
NOTE: - Idle RPM 35% is not reached after 60 sec’s
NOTE: - Oil pressure stays below 0.5 kg’s
TO STOP THE ENGINE
[ ]  Throttle idle
[ ]  FUEL SHUT OFF lever .... CLOSED
IN CASE OF FIRE CONTINUE WITH THE FOLLOWING STEPS;
[ ]  FIRE COCK lever .... SHUT
[ ]  FIRE EXT button .... DEPRESS
[ ]  All electric's switches .... OFF
[ ]  Aircraft .... Abandon

AFTER ENGINE START
[ ]  SEC B switch .... ON
[ ]  INV switch (PO-250) .... ON
[ ]  ICS panel .... recheck
[ ]  VHF/ AVIONICS .... ON
[ ]  Ext tank switch .... ON

ENGINE RUN-UP (first flight of day)
[ ]  Brakes .... apply
[ ]  Throttle .... idle 35%
[ ]  EGT .... 550’c MAX
[ ]  Fuel pressure .... 12 kg’s
[ ]  Oil pressure .... 0.5 kg’s
[ ]  Oil temperature .... 20’c MIN
[ ]  Throttle .... 52% (EGT, OP, OT, FP)
[ ]  C+W panel (T-9) .... check
[ ]  Attitude indicator (horizon) .... Erect
[ ]  RMI Compass .... synchronise with standby
[ ]  Fire warning .... check
[ ]  VOLTS/AMPS .... check 28V
[ ]  Throttle .... 65% (EGT, OP, OT,
[ ]  Flaps/ stabiliser .... check operation ,FP)
[ ]  Speed brakes .... check operation
[ ]  HYD PRESS gage .... check pressure
[ ]  EXT TANKS light (C+W) .... out
[ ]  Throttle .... 94% (EGT, OP, OT, FP)
[ ]  ISOLATION VALVE switch .... on (check light)
[ ]  RPM rise .... 1 to 3% RPM
[ ]  Throttle .... 97% (EGT, OP, OT, FP)
[ ]  Throttle .... 100%(EGT, OP, OT, FP)
[ ]  EGT .... 700'c max
[ ]  Fuel pressure .... 79 kgs max
[ ]  Oil pressure .... 1.8 to 2.5 kg's
[ ]  Oil temperature .... 110'c max
[ ]  Throttle .... idle (RPM stabilised)
[ ]  Throttle slam in 2 secs .... 12 to 14 sec's
[ ]  RPM swing .... 2% RPM max (5 times)
[ ]  EGT .... 730'c peak
[ ]  Throttle .... idle
[ ]  Flight controls .... recheck
[ ]  Taxi clearance .... request

ENGINE RUN UP (subsequent flight)
[ ]  Brakes .... apply
[ ]  Throttle .... idle 35%
[ ]  EGT .... 550'c max
[ ]  Fuel pressure .... 12 kg's
[ ]  Oil pressure .... 0.5 kg's
[ ]  Oil temperature .... 20'c min
[ ]  Throttle .... 52% (EGT, OP, OT, FP)
[ ]  C+W panel (T-9) .... check
[ ]  Attitude indicator .... erect
[ ]  Compass .... sycronize check standby
[ ]  Fire warning .... check
[ ]  VOLTS/ AMPS .... check 28V
[ ]  Throttle .... 65% (EGT, OP, OT, FP)
[ ]  Flaps/ stabiliser .... check operation (elc+mech
[ ]  Speed brake .... check operation ind)
[ ]  HYD PRESS gage .... check pressure
[ ]  EXT TANKS light (C+W) .... out
[ ]  Throttle .... idle
[ ]  Flight controls .... full & free
[ ]  Taxi clearance .... request

BEFORE TAXI
[ ]  Altimeter .... set
[ ]  Engine instruments .... in green
[ ]  All safety pins .... removed and stowed
[ ]  Canopy .... closed
[ ]  Pressurisation .... as required

TAXING
[ ]  Brakes .... apply
[ ]  Chocks .... removed
[ ]  Throttle .... 80%
[ ]  Brakes .... release and test
[ ]  Turn check left/ right .... perform

PRE TAKEOFF
[ ]  Trim .... 2' rear
[ ]  Speed brakes .... check in
[ ]  Flaps .... 15' set
[ ]  Fuel quantity .... check
[ ]  Engine and flight instruments .... T's & P's check
[ ]  Oxygen .... check
[ ]  Canopy .... locked
[ ]  Harness .... secure
[ ]  Hydraulic pressure .... check
[ ]  C+W panel .... check
[ ]  Flight controls .... full & free
[ ]  All pins .... removed and stowed
[ ]  Cockpit pressurisation .... check (both cockpits)

TAKEOFF
[ ]  Brakes .... apply
[ ]  Altimeter .... recheck
[ ]  Attitude indicator .... reset
[ ]  Compass .... RWY heading
[ ]  Radio compass needle .... check direction
[ ]  Throttle .... 90% RPM
[ ]  Engine instruments .... check
[ ]  Brakes .... release
[ ]  Throttle .... 100% max power
[ ]  Nose wheel lift off .... 140km/h
[ ]  Lift off .... 180km/h

AFTER TAKEOFF
[ ]  LANDING GEAR UP button .... push (min 50ft AGL)
[ ]  FLAPS 0' button .... push (min 150ft AGL)
[ ]  Throttle .... 97% upon reaching 250
[ ]  ELEV TRIM lever .... set km/hr
[ ]  Engine instruments .... check
[ ]  All warning lights .... out

CLIMB
[ ]  100% RPM max of 6 mins, then reduce to 97%
[ ]  initial climb speed 350 kph
[ ]  CABIN ALT PRESSURE .... CHECK
[ ]  Oxygen .... check
[ ]  Engine instruments .... check (EGT, OP, OT, FP)

CRUISE
[ ]  Level of maintain CAS or MACH number power about 90%
[ ]  Fuel quantity .... check
[ ]  Oxygen .... check
[ ]  Engine instruments .... check (EGT, OP, OT, FP)
[ ]  Location .... identify

DESCENT
NOTE: Normal decent is at 65% AT 300 KPH
[ ]  Fuel quantity .... check
[ ]  Engine & flight instruments .... check (EGT, OP, OT, FP)
[ ]  Approach .... request
[ ]  Altimeter .... set QFE
[ ]  De-mist .... as required

BEFORE LANDING
[ ]  Fuel quantity .... check
[ ]  All warning lights .... out
[ ]  Pneumatic & hydraulic gages .... check

LANDING
[ ]  Check speed/ distance for particular weight
[ ]  Approach .... 300 kph
DOWN WIND LEG
[ ]  Airspeed .... 290 kph
[ ]  LANDING GEAR .... select down
[ ]  Landing gear .... check indicators
[ ]  Airspeed .... 270 kph
[ ]  FLAPS 15' button .... select 15'
[ ]  Flaps indicator .... check
[ ]  Airspeed .... 250 kph
[ ]  Throttle .... 90-94%
BASE LEG
[ ]  Airspeed .... 240 kph
[ ]  Throttle .... 80-85%
[ ]  FLAPS 30' button .... select 30'
[ ]  Flaps indicator .... check
[ ]  Airspeed in turn .... 220 kph
FINAL APPROACH
[ ]  Landing gear + flaps .... check indicators
[ ]  Airspeed .... 200 kph
[ ]  Throttle .... as required

AFTER TOUCH DOWN
NOTE: Max braking speed 1300 lts 140 kph
NOTE: 1000 lts 145 kph
NOTE: 700 lts 150 kph
NOTE: 400 lts 160 kph

AFTER LANDING
[ ]  Trim .... neutral
[ ]  Speed brakes .... in
[ ]  Pitot heat .... off
[ ]  Flaps .... up
[ ]  Pressurisation .... off

ENGINE SHUT DOWN
[ ]  Chocks .... in place
[ ]  Canopies .... open
[ ]  Ejector seat pins .... install
[ ]  Throttle .... idle for 30 sec's
[ ]  FUEL SHUT OFF lever .... closed
[ ]  SEC B switch .... off
[ ]  INV switch .... off
[ ]  Engine run down time .... check min 50 sec's
AFTER ENGINE STOP
[ ]  ENG switch .... off
[ ]  GEN switch .... off
[ ]  BATT switch .... off
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