American Champion Aircraft 8KCAB Decathlon — Paul_Yust_8KCAB_Decathlon_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

PREFLIGHT
[ ]  Gust Lock .... REMOVE
[ ]  If Empty Rear Seat .... FASTEN BELT
[ ]  Fuel Gauges .... CHECK
[ ]  ELT and Lights for Night .... CHECK
[ ]  Tie Downs & Chocks .... REMOVED
[ ]  Right Wing & Strut .... CHECK
[ ]  Right Wheel & Brake (24 PSI) .... CHECK
[ ]  Right Fuel Qty .... CHECK & SECURE
[ ]  Gascolator (1st Flight) .... DRAIN
[ ]  Oil Level .... 6-8 QTS
[ ]  Windshield .... CLEAN
[ ]  Prop/Spinner/Filter/Light .... CHECK
[ ]  Left Wing-same as right .... CHECK
[ ]  Pitot Tube/Stall Warning .... CHECK
[ ]  Static Port/Antennas .... CHECK
[ ]  Aft Belly Sump (1st Flight) .... SAMPLE
[ ]  Rudder & Elevator .... CHECK
[ ]  Tail Wheel (40 PSI) .... CHECK
[ ]  Tach. Time .... RECORD

ENGINE START
[ ]  Passenger Brief .... COMPLETE
[ ]  Seats, Harness, Door .... SECURE
[ ]  Fuel Shut-Off Valve .... ON
[ ]  Brakes .... TEST & SET
[ ]  Electrics/Avionics .... OFF
[ ]  Beacon (Always On) .... ON
[ ]  Alternate Air .... COLD
[ ]  Throttle .... 1/2” OPEN
[ ]  Prop .... FULL FORWARD
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Master .... ON
[ ]  Prime (*details below) .... AS REQ
[ ]  Prop Area .... CLEAR
[ ]  Control Stick .... FULL AFT
[ ]  Mags .... BOTH ON
[ ]  Starter (15 sec limit) .... ENGAGE
[ ]  Mixture (as engine starts) .... FULL RICH
[ ]  Throttle .... 1000 RPM
[ ]  Oil pressure .... CHECK
[ ]  Mixture (for taxi) .... LEAN
[ ]  Avionics .... ON & SET
[ ]  Brakes .... RELEASE
NOTE: * Cold Start Prime: Turn on fuel pump and push mixture to full rich. Hold
for 3 seconds then return mixture to idle cut-ff and turn off fuel pump.
NOTE: * Hot Start Prime: Not usually required.
NOTE: * Flooded Start: With throttle full open and mixture idle cut-off turn prop
10 revs then do half prime and try start again.

RUN-UP
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Elevator Trim Position .... TAKEOFF
[ ]  Flight Instruments .... SET
[ ]  Fuel Shut-Off Valve .... ON
[ ]  Mixture (<3000’) .... RICH
[ ]  Throttle .... 1800 RPM
[ ]  - Mags L/R (175/50) .... CHECK
[ ]  - Prop .... CYCLE TWICE
[ ]  - Alternate Air .... CYCLE
[ ]  - Engine Gauges .... GREEN
[ ]  - Throttle .... 1000 RPM

TAKE-OFF
[ ]  Doors/Windows/Belts .... SECURE
[ ]  Transponder/Strobes/Lights .... ON
[ ]  Fuel Pump (optional) .... ON
[ ]  Throttle/Prop/Mixture .... FULL FORWARD
[ ]  Rotate .... 56 RPM
[ ]  Climb Speed .... 80-90 MPH
[ ]  Fuel Pump (at 1000’) .... OFF
[ ]  Landing Light .... OFF

CRUISE
[ ]  Power .... 23”/2400 OR AS REQ
[ ]  Mixture .... LEAN BELOW 75% PWR

AEROBATICS
[ ]  Altitude .... FINISH ABOVE 3000’ AGL
[ ]  Clear Area .... COMPLETE
[ ]  Engine .... 24” /2500 & GREEN
[ ]  Mixture .... RICH
ENTRY SPEED
[ ]  - Acrobatic VA .... 130 MPH
[ ]  - Aileron or Barrel Roll .... 120 MPH
[ ]  - Loop .... 140 MPH
[ ]  - Immelmann .... 145 MPH
[ ]  - Hammerhead .... 145 MPH
[ ]  - Snap Roll .... 90 MPH

LANDING
[ ]  Brakes .... CHECK FIRM
[ ]  Parking Brake .... OFF
[ ]  Fuel Pump (optional) .... ON
[ ]  GUMPS Check .... COMPLETE
[ ]  Final Approach .... 70-80 MPH

SHUTDOWN
[ ]  S  Avionics/Electrics .... OFF
[ ]  L  Mixture .... IDLE-CUTOFF
[ ]  I   Mags .... OFF
[ ]  M Master .... OFF
[ ]  Tach Time .... RECORD
[ ]  Gust Lock (Seat Belt) .... SECURE
[ ]  Flight Plan .... CLOSED

ENGINE FAILURE AT TAKEOFF
[ ]  Throttle .... CLOSED
[ ]  Land .... ASAP

EMERGENCY LANDING
[ ]  Best Glide Speed .... 75 MPH
[ ]  Landing field .... SELECTED
[ ]  Seats & Belts .... READY
[ ]  Door .... AJAR
TIME PERMITTING:
[ ]  - Engine (details below) .... AIR START
[ ]  - Radio (121.5) .... MAYDAY
[ ]  - Transponder .... 7700
[ ]  - ELT .... ON
IF NO LUCK RESTARTING ENGINE THEN
[ ]  - Mixture .... IDLE CUTOFF
[ ]  - Fuel Shut-Off Valve .... OFF
[ ]  - Master & Mags .... OFF
[ ]  Final Approach .... 75 MPH
[ ]  Before Touchdown .... DO NOT STALL

DITCHING OVER WATER
[ ]  Cabin Side Door .... JETTISON
[ ]  If High Swells .... LAND PARALLEL
[ ]  Else .... LAND INTO WIND
[ ]  Before Touchdown .... DO NOT STALL

EMERGENCY EXIT/BAIL OUT
[ ]  Throttle .... CLOSED
[ ]  Door .... JETTISON
[ ]  Dive .... OUT & SLIGHTLY AFT
[ ]  Parachute .... OPEN WHEN CLEAR

ENGINE AIR START
[ ]  Airspeed .... 80+ MPH
[ ]  Mags .... BOTH ON
[ ]  Throttle .... 3/4 FORWARD
[ ]  Mixture (<5000) .... FULL FORWARD
[ ]  Prop .... FULL FORWARD
[ ]  Fuel Shut-Off Valve .... CHECK ON
[ ]  Alternate Air .... FULL HOT
[ ]  Fuel Pump .... ON
IF NO RESTART    THEN
[ ]  - Mixture .... IDLE THEN RICH
IF PROP STOPS WINDMILLING    THEN
[ ]  - Starter .... ENGAGE

V-SPEEDS (MPH @ Max Wt)
NOTE: |VS 53   |VR 56   |VA 121  |
NOTE: |VFINAL  |VX   64 |VNO 160?|
NOTE: |75      |        |        |
NOTE: |VGLIDE  |VY 76   |VNE 180 |
NOTE: |75      |        |        |

ENGINE FIRE – GROUND
[ ]  Starter .... CONTINUE CRANKING
[ ]  Mixture .... IDLE CUTOFF
[ ]  Throttle .... FULL OPEN
IF FIRE PERSIST  THEN
[ ]  - Fuel Shut-Off Valve .... OFF
[ ]  - Mags & Electrics .... OFF
[ ]  Exit Plane .... ASAP
[ ]  Fire Extinguisher .... AS REQ

ENGINE FIRE – IN FLIGHT
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Shut-off Valve .... OFF
[ ]  Mags & Electrics .... OFF
[ ]  Cabin Heat .... OFF
[ ]  Fire Extinguisher .... AS REQ
[ ]  Land .... ASAP

ELECTRICAL FIRE
[ ]  Mags .... REMAIN ON
[ ]  Master & All Other Electrics .... OFF
[ ]  Cabin Vents/Window .... OPEN IF REQ
[ ]  Fire Extinguisher .... AS REQ
[ ]  Master (if power required) .... ON
[ ]  - Electric Switches .... 1 AT TIME
[ ]  Land .... ASAP

ALTERNATOR/ELECTIC FAILURE
[ ]  Master .... OFF, then ON
IF DISCHARGE CONTINUES THEN
[ ]  - All Non-Essential Electric .... OFF
[ ]  - Fuses .... CHECK
[ ]  Land .... ASAP

ABNORMAL OIL PRESS/TEMP
[ ]  Throttle .... REDUCE POWER
[ ]  Land .... ASAP

ICING CONDITIONS
[ ]  Pitot Heat .... ON
[ ]  Cabin Heat .... OFF
[ ]  Direction and/or Altitude .... CHANGE

WEIGHT & BALANCE (LBS)
[ ]  Empty Weight .... 1326
[ ]  Normal Max Gross Weight .... 1950
[ ]  - Half Fuel Payload (19.5 gals) .... 504
[ ]  - Full Fuel Payload (39 gals) .... 384
[ ]  Acrobatic Max Gross Weight .... 1800
[ ]  - Half Fuel Payload (19.5 gals) .... 354
[ ]  - Full Fuel Payload (39 gals) .... 234
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