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Pre-Start Checklist
[ ]  Parking Brakes .... SET
[ ]  Battery Switch .... OFF
[ ]  Generator Switches .... OFF
[ ]  Power Management Switch .... CHECK SET TO (take off)
[ ]  Automatic Torque Switches .... CHECK OFF !!!
[ ]  Throttle .... IDLE
[ ]  Landing Gear Lever .... CHECK DOWN
[ ]  Propeller .... HIGH RPM
[ ]  Fuel Cond. Lever .... FUEL CUTOFF
[ ]  Idle Gate Lever .... GROUND IDLE
[ ]  Flaps .... UP
[ ]  Battery Switch .... ON
[ ]  Panel Lights .... ON if required
[ ]  Fuel Quantity .... CHECK
[ ]  Flight controls .... CHECK
[ ]  Avionics Master Switch .... ON
[ ]  Check Weather .... (ATIS, Flight Services)
[ ]  Anti-ice .... TEST/CHECK
[ ]  Request Clearance
[ ]  Transponder .... STANDBY
[ ]  Beacon .... ON

Startup Checklist
[ ]  Engine and Propeller Area Throttle .... CLEAR
[ ]  Throttle .... IDLE
[ ]  Fuel Valves .... OPEN
[ ]  Fuel Cond. Lever .... AUTO
[ ]  Idle Gate Lever .... FLIGHT IDLE
[ ]  Prop Brake .... OFF
[ ]  Engine Start Selection Switch .... CRANK few seconds
[ ]  Engine Start Selection Switch .... START A+B
[ ]  Start Button Engine 2 .... START (hold until engine starts)
[ ]  Generator 2 .... ON
[ ]  Start Button Engine 1 .... START (hold until engine starts)
[ ]  Generator 1 .... ON
[ ]  Loadmeter+Voltmeter .... CHECK for CHARGE
[ ]  Engine Start Selection Switch .... OFF

Before Taxi Checklist
[ ]  Nav Lights .... ON
[ ]  Taxi Lights / Logo Lights / Wing Lights .... ON
[ ]  Heading Indicator / Altimeter .... SET
[ ]  Instruments .... NORMAL OPERATION
[ ]  Radios and Avionics .... ON, CHECKED and SET
[ ]  Autopilot .... SET and OFF
[ ]  F/D .... ON
[ ]  Request Taxi Clearance

Taxi Checklist
[ ]  Parking Brake .... RELEASE
[ ]  Brakes .... CHECK during taxi
[ ]  Directional Gyro .... PROPER IND. during turns
[ ]  Turn Coordinator .... PROPER IND. during turns
[ ]  Artificial Horizon .... ERECT during turns
[ ]  Taxi to assigned runway .... SPEED Max. 20 knots

Before Take-off Checklist
[ ]  Parking Brake .... SET
[ ]  Fuel Quantity .... CHECK
[ ]  Throttle .... IDLE
[ ]  Elevator Trim .... SET for takeoff
[ ]  Flaps .... 15 deg
[ ]  Flight Controls .... FREE AND CORRECT
[ ]  Engine / Flight Instruments .... CHECK
[ ]  Radios and Avionics .... SET
[ ]  Landing Lights .... ON
[ ]  Taxi Lights .... OFF
[ ]  Strobe Light .... ON
[ ]  Pitot Heat .... ON
[ ]  Anti-Ice .... AS REQUIRED
[ ]  Power Management Switch .... SET TO (take off)
[ ]  Annunciator Lights .... CHECK
[ ]  Transponder .... ON
[ ]  Request Takeoff Clearance

Take-off Checklist
[ ]  Automatic Torque Switches .... BOTH ON
[ ]  Brakes .... RELEASE
[ ]  V1 = Vr = .... 110 KIAS
[ ]  Pitch .... 10 degrees
[ ]  V2 = .... 115 KIAS
[ ]  At Positive Climb Rate .... Touch Brakes
[ ]  Landing Gear .... RETRACT
[ ]  Power Management Switch .... SET CLB (climb)
[ ]  At 130 KIAS .... RETRACT FLAPS
[ ]  Annunciator Lights / Eng. Instruments .... CHECK

Climb-out Checklist
[ ]  Power Management Switch .... CHECK CLB
[ ]  Autopilot .... CHECK and SET
[ ]  Yaw Damper .... ON
[ ]  Landing Lights .... OFF
[ ]  Airspeed .... 190 KIAS / 1800 fpm / 89%
[ ]  above 12’000 ft .... 180 KIAS / 1500 fpm / 77%
[ ]  Engine Instruments .... MONITOR
[ ]  ATC .... AS REQUIRED
[ ]  At Transition Altitude (FL180) set Altimeter to 29,92" (1013mb)

Cruise Checklist
[ ]  Accelerate to cruise speed
[ ]  Power Management Switch .... SET CRZ (cruise)
[ ]  at 6’000 ft .... 245 KIAS / 78%
[ ]  at 9’000 ft .... 240 KIAS / 76%
[ ]  at 12’000 ft .... 235 KIAS / 73%
[ ]  at 18’000 ft .... 220 KIAS / 68%
[ ]  at 24’000 ft .... 205 KIAS / 63%
[ ]  Service Ceiling .... 25’000 ft
[ ]  Engine+Instruments .... CHECK
[ ]  Fuel Quantity .... CHECK
[ ]  Radios .... TUNED and SET
[ ]  Autopilot .... CHECK and SET

Descent Checklist
[ ]  Atis / Airport Information .... CHECK
[ ]  Altimeter .... CHECK
[ ]  Radios .... SET
[ ]  Automatic Torque Switches .... OFF !!!
[ ]  Descent Speed .... 200 - 240 KIAS / ~15%
[ ]  Descent Rate .... -1500 fpm
[ ]  Flaps / Landing Gear .... CHECK UP
[ ]  At Transition Altitude (FL180) reset Altimeter to local
[ ]  Check Weather .... (ATIS, Flight Services)

Approach Checklist
LOCALIZER LEVEL FLIGHT :
[ ]  Speed: Establish .... 160 KIAS / 28%
[ ]  Landing Lights .... ON
[ ]  Flaps .... 15 deg
[ ]  Speed: Establish .... 145 KIAS / 41%
[ ]  Turning towards runway set flaps .... 30 deg
[ ]  Speed: Establish .... 130 KIAS / 44%
[ ]  Landing Gear .... DOWN
FINAL GLIDESLOPE DESCENT :
[ ]  Speed: Establish .... 120 KIAS / 28%
[ ]  Descent Rate .... -600 fpm
[ ]  Elevator Trim .... AS DESIRED
[ ]  Parking Brake .... VERIFY OFF
[ ]  Anti-Ice .... AS REQUIRED
[ ]  Yaw Damper .... OFF

Landing Checklist
[ ]  Landing Gear .... CHECK DOWN, 3 GREEN
[ ]  Autopilot .... OFF
[ ]  Landing Speed .... 115 KIAS
[ ]  Touchdown .... MAIN WHEELS FIRST
[ ]  Landing Roll .... LOWER NOSE WHEEL
[ ]  After touchdown .... Apply Reverse Thrust, at 60 kts: Cancel Reverse Thrust

Taxi To Ramp
[ ]  Strobe Light .... OFF
[ ]  Taxi Lights .... ON
[ ]  Landing Lights .... OFF
[ ]  Flaps .... RETRACT
[ ]  Anti-Ice .... OFF
[ ]  Transponder .... 1200
[ ]  Speed .... Max. 20 knots
[ ]  Elevator Trim .... TAKEOFF SETTING
[ ]  Avionics/Radios .... AS REQUIRED

Shutdown Checklist
[ ]  Parking Brake .... SET
[ ]  Throttle .... IDLE
[ ]  Pitot Heat .... OFF
[ ]  F/D .... OFF
[ ]  Avionics .... OFF
[ ]  Taxi Lights .... OFF
[ ]  Logo Lights / Wing Lights .... OFF
[ ]  Nav Lights .... OFF
[ ]  Fuel Cond. Lever .... FUEL CUTOFF
[ ]  Idle Gate Lever .... GROUND IDLE
[ ]  Fuel Valves .... CLOSE
[ ]  Power Management Switch .... SET TO (take off)
[ ]  Beacon .... OFF
[ ]  Generators .... OFF
[ ]  Prop Brake .... ON
[ ]  Panel Light .... OFF
[ ]  Battery Switch .... OFF

Securing Aircraft
[ ]  Parking Brake .... Verify SET
[ ]  Throttle .... Verify IDLE
[ ]  All Switches .... Verify OFF
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