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AIRSPEEDS FOR SAFE OPERATION
NOTE: All airspeeds quoted in this section are indicated airspeeds (IAS)
TAKE-OFF
[ ]  Lift-off .... 65 KTS / 75 MPH
[ ]  50 Ft. .... 73 KTS / 84 MPH
MAXIMUM CLIMB
[ ]  Best Rate (VY) .... 75 KTS / 86 MPH
[ ]  Best Angle (VX) .... 68 KTS / 78 MPH

[ ]  Cruise Climb .... 87 KTS / 100 MPH
MAXIMUM TURBULENT AIR PENETRATION
[ ]  Balked Landing .... 114 KTS / 131 MPH
[ ]  Landing Approach .... 64 KTS / 74 MPH
[ ]   .... 69 KTS / 79 MPH
[ ]  Emergency Glide speed .... 78 KTS / 90 MPH

[ ]  Maximum Demonstrated Crosswind .... 13 KTS / 15 MPH

Preflight Inspection
[ ]  Emergency Locator Transmitter .... ARMED
1. CABIN
[ ]  Parking Brake .... SET
[ ]  Control Lock .... REMOVED
[ ]  All Switches .... OFF
[ ]  Flaps .... DOWN
2. RIGHT FUSELAGE
[ ]  Baggage Door .... CLOSED
[ ]  Static Pressure Button .... UNOBSTRUCTED
3. EMPENNAGE
[ ]  Control Surfaces .... CHECK
[ ]  Position Light .... CHECK
[ ]  Tie Down .... REMOVED
4. LEFT FUSELAGE
[ ]  All Antennas .... CHECK
[ ]  Static Pressure Button .... UNOBSTRUCTED
5. LEFT WING TRAILING EDGE
[ ]  Flap .... CHECK
[ ]  Fuel Vent line .... UNOBSTRUCTED
[ ]  Aileron .... CHECK
[ ]  Wing Tip .... CHECK
[ ]  Position Light .... CHECK
6. LEFT WING LEADING EDGE
[ ]  Pitot Tube .... CHECK
[ ]  Landing Light .... CHECK
[ ]  Tie Down and Chocks .... REMOVED
[ ]  Stall Warning .... CHECK
[ ]  Fuel Tank .... CHECK QUANTITY
[ ]  Filler Cap .... SECURE
7. LEFT LANDING GEAR
[ ]  Tire and Brake .... CHECK
[ ]  Fuel Sump .... DRAIN
8. NOSE SECTION
[ ]  Left Cowl .... SECURE
[ ]  Engine Oil .... CHECK
[ ]  Cap and Dipstick .... SECURE
[ ]  Induction Air Intake .... CHECK
[ ]  Filter .... CHECK
[ ]  Propeller .... CHECK
[ ]  Tire and Nose Gear .... CHECK
[ ]  Right Cowl .... SECURE
[ ]  Chocks and Tow Bar .... REMOVED
[ ]  Fuel Strainer .... DRAIN
9. RIGHT LANDING GEAR
[ ]  Fuel Sump .... DRAIN
[ ]  Tire and Brake .... CHECK
10. RIGHT WING LEADING EDGE
[ ]  Fuel Tank .... CHECK QUANTITY
[ ]  Filler Cap .... SECURE
[ ]  Tie Down and Chocks .... REMOVED
[ ]  Wing Tip .... CHECK
[ ]  Position Light .... CHECK
11. RIGHT WING TRAILING EDGE
[ ]  Aileron .... CHECK
[ ]  Flap .... CHECK
[ ]  Fuel Vent line .... UNOBSTRUCTED

BEFORE STARTING ENGINE
[ ]  Seats .... POSITION AND LOCK
[ ]  Seat Belts .... FASTEN
[ ]  Parking Brake .... SET
[ ]  All Avionics .... OFF
[ ]  Circuit Breakers .... IN
[ ]  Flaps .... UP
[ ]  Clock .... SET
[ ]  Fuel Selector .... ROTATE thru 360 o check for freedom and movement
[ ]  Fuel Selector .... LEFT TANK
[ ]  Light Switches .... AS REQUIRED
[ ]  Battery Switch .... ON
[ ]  ALT Switch .... ON
[ ]  If external power is used .... OFF
[ ]  Horizontal Indicator .... SET
WARNING: Do not take off if gages indicate in yellow arc on either gage (airplanes after compliance with BEECHCRAFT S.I. No. 0624-281).

STARTING ENGINE
CAUTION: Starter cranking period should be limited to a maximum of 30 seconds, with at least 3 to 5 minutes between cranking periods.
NORMAL START:
[ ]  Mixture .... FULL RICH
[ ]  Throttle .... IDLE position
[ ]  Fuel Boost Pump .... ON (until fuel pressure stabilizes at 2.5 psi)
[ ]  Start Switch .... START position (release to BOTH position when engine fires)
[ ]  Fuel Boost Pump .... OFF (After engine is running smoothly)
[ ]  Oil Pressure .... IN YELLOW position within 30 seconds
[ ]  Engine Instruments .... CHECK
[ ]  Warm-up .... 800 to 1200 RPM
HOT START:
[ ]  Mixture .... FULL RICH
[ ]  Throttle .... IDLE position
[ ]  Starter Switch .... START position (release to BOTH position when engine fires)
[ ]  Fuel Boost Pump .... ON
[ ]  Fuel Boost Pump .... OFF (After engine is running smoothly)
[ ]  Oil Pressure .... IN YELLOW position within 30 seconds
[ ]  Engine Instruments .... CHECK
[ ]  Warm-up .... 800 to 1200 RPM

BEFORE TAXI
[ ]  Avionics Equipment .... ON, AS REQUIRED
[ ]  Anti-Collision Light .... ON
[ ]  Lights .... AS REQUIRED
[ ]  Radio .... SET

BEFORE TAKEOFF
[ ]  Parking Brake .... SET
[ ]  Seat Belts .... CHECK
NOTE: All reclining seats must be in the upright position during take-off.
[ ]  Flight Instruments .... CHECK AND SET
[ ]  Throttle .... 1700 RPM
[ ]  Magnetos .... CHECK at 1700 RPM, maximum drop of 150 RPM on each magneto, variance between individual magnetos should not exceed 50 RPM
[ ]  Vacuum .... CHECK
[ ]  Throttle .... 1500 RPM
[ ]  Ammeter .... CHECK stabilized indication within 1/4 scale of zero
[ ]  Throttle .... FAST IDLE
[ ]  Trim .... TAKEOFF
[ ]  Flaps .... CHECK AND SET 10 0
[ ]  Controls .... CHECK
[ ]  Doors .... SECURE
[ ]  Fuel Boost Pump .... OFF
[ ]  Mixture .... FULL RICH
[ ]  Oil Temperature .... CHECK
[ ]  Parking Brake .... RELEASE

TAKEOFF
[ ]  Power .... FULL THROTTLE
[ ]  Airspeed .... ACCELERATE 65 KTS
[ ]  Climb Speed .... CLEARED OBSTACLES

BEFORE LANDING
[ ]  Seat Belts .... SECURE
NOTE: All reclining seats must be in the upright position during landing.
[ ]  Mixture .... FULL RICH
[ ]  Landing Light .... ON
[ ]  Flaps .... DOWN
[ ]  Airspeed .... 69 KTS

AFTER LANDING
[ ]  Flaps .... UP
[ ]  Trim Tab .... SET to O0

SHUTDOWN
[ ]  Electrical and Avionics .... OFF
[ ]  GPS .... OFF
[ ]  Throttle .... CLOSE
[ ]  Mixture .... IDLE CUT OFF
[ ]  Magneto/Start Switch .... OFF
[ ]  Battery & ALT Switch .... OFF
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