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Pre-Start Checklist
WARNING: CHECKLIST FOR MICROSOFT FLIGHT SIMULATOR ONLY. NOT FOR REAL WORLD FLIGHT!
[ ]  Parking Brakes .... SET
[ ]  Throttle .... IDLE
[ ]  Battery Switch .... OFF
[ ]  Avionics Master Switch .... OFF
[ ]  Master Caution Display .... ON
[ ]  Flaps .... UP
[ ]  Propeller .... HIGH RPM
[ ]  Fuel Cond. Lever .... FUEL CUTOFF (Ctrl-Shift-F1)
[ ]  Landing Gear Lever .... CHECK DOWN
[ ]  Battery Switch .... ON
[ ]  Panel Lights .... ON if required
[ ]  Fuel Quantity .... CHECK
[ ]  Flight controls .... CHECK
[ ]  Avionics Master Switch .... ON
[ ]  Check Weather .... (ATIS, Flight Services)
[ ]  Anti-ice Switch .... TEST/CHECK
[ ]  Anti-ice Annunciators .... ILLUMINATED
[ ]  Request Clearance
[ ]  Transponder .... STANDBY
[ ]  Beacon .... ON

Startup Checklist
[ ]  Engine and Propeller Area .... CLEAR
[ ]  Throttle .... IDLE
[ ]  Fuel Flow / Fuel Cond. Lever .... ON
[ ]  Right Ignition and Engine Start Switch .... ON (hold until engine starts)
[ ]  Right ITT and N1 Turbine RPM .... MONITOR
[ ]  Right FUEL PRESS LO Annunciator .... EXTINGUISHED
[ ]  Right OIL PRESS LO Annunciator .... EXTINGUISHED
[ ]  Right Oil Pressure .... CHECK
[ ]  Right Generator .... ON
==> REPEAT FOR LEFT ENGINE
[ ]  Feather/Unfeather Props .... CHECK once
[ ]  Master Warning Display .... OFF
[ ]  Master Caution Display .... OFF
[ ]  Throttle Quadrant Display .... OFF
[ ]  Engine Instruments .... CHECK

Before Taxi Checklist
[ ]  Nav Lights .... ON
[ ]  Taxi Lights .... ON
[ ]  Heading Indicator / Altimeter .... SET
[ ]  Instruments .... NORMAL OPERATION
[ ]  Radios and Avionics .... CHECKED and SET
[ ]  Autopilot .... SET and OFF
[ ]  F/D .... ON
[ ]  Yaw Damper .... ON AS REQUIRED
[ ]  Autofeather .... ARM
[ ]  Anti-ice .... AS REQUIRED
[ ]  Request Taxi Clearance

Taxi Checklist
[ ]  Parking Brake .... RELEASE
[ ]  Taxi to assigned runway .... SPEED Max. 20 knots
[ ]  Brakes .... CHECK during taxi
[ ]  Directional Gyro .... PROPER IND. during turns
[ ]  Turn Coordinator .... PROPER IND. during turns
[ ]  Artificial Horizon .... ERECT during turns

Before Take-off Checklist
[ ]  Parking Brake .... SET
[ ]  Fuel Quantity .... CHECK
[ ]  Throttle .... IDLE
[ ]  Propeller .... HIGH RPM
[ ]  Elevator Trim .... SET for takeoff
[ ]  Flight Controls .... FREE AND CORRECT
[ ]  Radios and Avionics .... SET
[ ]  Landing Lights .... ON
[ ]  Taxi Lights .... OFF
[ ]  Engine Instruments .... CHECK
[ ]  Annunciator Lights .... CHECK
[ ]  Strobe Light .... ON
[ ]  Pitot Heat .... ON
[ ]  Anti-ice .... AS REQUIRED
[ ]  Transponder .... ON
[ ]  Request Takeoff Clearance

Take-off Checklist
[ ]  Smoothly increase thrust to .... FULL
[ ]  Brakes .... RELEASE
[ ]  V1 = .... 105 KIAS (descision)
[ ]  Vr = .... 110 KIAS (rotate)
[ ]  V2 = .... 115 KIAS
[ ]  Pitch .... 10-15 degrees
[ ]  At Positive Climb Rate .... Touch Brakes
[ ]  Landing Gear .... RETRACT
[ ]  Trim for climb to maintain .... 140 KIAS Torque 65
[ ]  Annunciator Lights .... CHECK
[ ]  Engine Instruments .... CHECK

Climb-out Checklist
[ ]  Propeller Synchrophaser .... ON
[ ]  Autopilot .... CHECK and SET
[ ]  Landing Lights .... OFF
[ ]  Airspeed .... 160 KIAS Torque 80
[ ]  Engine Instruments .... MONITOR
[ ]  ATC .... AS REQUIRED
[ ]  At Transition Altitude (FL180) set Altimeter to 29,92" (1013mb)

Cruise Checklist
[ ]  Accelerate to cruise speed .... 220-240 KIAS Torque 80
[ ]  Autofeather .... OFF
[ ]  Service Ceiling .... 35’000 ft
[ ]  Engine+Instruments .... CHECK
[ ]  Engine Temperatures .... STABILIZE at cruise cond.
[ ]  Anti-ice .... AS REQUIRED
[ ]  Fuel Quantity .... CHECK
[ ]  Radios .... TUNED and SET
[ ]  Autopilot .... CHECK and SET
[ ]  Lights .... as required
[ ]  Engine Instruments .... CHECK

Descent Checklist
[ ]  Atis/Airport Information .... CHECK
[ ]  Altimeter .... CHECK
[ ]  Radios .... SET
[ ]  Autofeather .... ARM
[ ]  Descent Speed .... 180 KIAS Torque 10
[ ]  Flaps .... CHECK UP
[ ]  Landing Gear .... CHECK UP
[ ]  Fuel Balance .... CHECK
[ ]  At Transition Altitude (FL180) reset Altimeter to local
[ ]  Check Weather .... (ATIS, Flight Services)

Approach Checklist
LOCALIZER LEVEL FLIGHT :
[ ]  Landing Lights .... ON
[ ]  Autofeather .... VERIFY ARMED
[ ]  Propeller .... HIGH RPM
[ ]  Fuel Cond. Lever .... FULL
[ ]  Anti-ice .... AS REQUIRED
[ ]  Speed: Establish .... 150 KIAS Torque 30
[ ]  Flaps .... SET APPR
[ ]  Speed: Establish .... 130 KIAS Torque 40
[ ]  Landing Gear .... DOWN
[ ]  Turning toward runway: set flaps .... FULL DOWN
FINAL GLIDESLOPE DESCENT :
[ ]  Speed: Establish .... 110 KIAS Torque 25
[ ]  Elevator Trim .... AS DESIRED
[ ]  Parking Brake .... VERIFY OFF

Landing Checklist
[ ]  Landing Gear .... CHECK DOWN, 3 GREEN
[ ]  Autopilot .... OFF
[ ]  Landing Speed .... 100 KIAS
[ ]  Touchdown .... MAIN WHEELS FIRST
[ ]  Landing Roll .... LOWER NOSE WHEEL
[ ]  After touchdown .... Apply Reverse Thrust, at 50 kts: Cancel Reverse Thrust

Taxi To Ramp
[ ]  Strobe Light .... OFF
[ ]  Flaps .... RETRACT
[ ]  Taxi Lights .... ON
[ ]  Landing Lights .... OFF
[ ]  Anti-ice .... OFF
[ ]  Speed .... Max. 20 knots
[ ]  Elevator Trim .... TAKEOFF SETTING
[ ]  Avionics/Radios .... AS REQUIRED
[ ]  Transponder .... 1200

Shutdown Checklist
[ ]  Parking .... SET
[ ]  Brake Throttle .... IDLE
[ ]  Autofeather .... OFF
[ ]  F/D .... OFF
[ ]  Avionics Switch .... OFF
[ ]  Taxi Lights .... OFF
[ ]  Nav Lights .... OFF
[ ]  Pitot Heat .... OFF
[ ]  Fuel Cond. Lever .... CUTOFF (Ctrl-Shift-F1)
[ ]  Propeller .... FEATHER
[ ]  Beacon .... OFF
[ ]  Panel Light .... OFF
[ ]  Battery Switch .... OFF when N1<15%
[ ]  Generator Switches .... OFF

Securing Aircraft
[ ]  Parking Brake .... Verify SET
[ ]  Throttle .... Verify IDLE
[ ]  All Switches .... Verify OFF
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