Beechcraft BE-55 _ BE-58 Baron — Baron_eps_cklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Ditching" item count differs between passes (12 vs 14); verify nothing was dropped.
content_gap: Section "Gear-Up Landing" item count differs between passes (8 vs 9); verify nothing was dropped.
content_gap: Section "Landing With One Main Gear Up or Unsafe" item count differs between passes (10 vs 9); verify nothing was dropped.
content_gap: Section "Landing With Only One Main Gear Extended" item count differs between passes (12 vs 11); verify nothing was dropped.
content_gap: Section "Radio Failure" item count differs between passes (18 vs 10); verify nothing was dropped.

Notes
NOTE: This emergency procedures checklist is intended to supplement the information contained in the Pilot’s Operating Handbook (POH) and serve as a handy inflight reference and instructional tool. Whenever time permits in an emergency situation, pilots should make use of all sources of information including the expanded text in the POH.
NOTE: In any emergency situation the pilot’s priorities should be 1. Maintain aircraft control. 2. Analyze the situation. 3. Take corrective action.
NOTE: Items in Bold Print are time critical steps that should be committed to memory so that they can be accomplished without referring to the checklist. As time permits during the handling of an emergency the pilot should then use the checklist to confirm that all Bold Print items have been accomplished.
NOTE: “Land as soon as practicable” as used in this checklist means that the pilot should land at the nearest airfield that has a suitable runway (length, type surface, etc.) and weather appropriate for the pilot’s proficiency and the type aircraft flown.
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Engine Failure During Takeoff Roll  [EMERGENCY]
Engine failure during takeoff roll
[ ]  Throttles [MEMORY] .... IDLE
[ ]  Brakes [MEMORY] .... As Required
[ ]  Complete SECURING SHUTDOWN ENGINE [E - 4] .... COMPLETE
NOTE: It is not normally possible to taxi with only one engine operating.

Engine Failure Immediately After Takeoff  [EMERGENCY]
Engine failure immediately after takeoff
IF SUFFICIENT RUNWAY AHEAD
[ ]  Throttles [MEMORY] .... Reduce
[ ]  Land Straight Ahead [MEMORY] .... LAND
IF TAKEOFF IS CONTINUED
[ ]  Airspeed [MEMORY] .... 100 KIAS (90 KIAS to Clear Obstacles)
[ ]  Mixtures [MEMORY] .... Full RICH (Forward)
[ ]  Propellers [MEMORY] .... Full HIGH RPM (Forward)
[ ]  Throttles [MEMORY] .... Full OPEN (Forward)
[ ]  Gear [MEMORY] .... UP
[ ]  Flaps [MEMORY] .... UP
[ ]  Dead Engine [MEMORY] .... Identify
[ ]  Throttle (Dead Engine) [MEMORY] .... Retard (Verify)
[ ]  Propeller (Dead Engine) [MEMORY] .... FEATHER
[ ]  Cowl Flap (Good Engine) .... Check OPEN
[ ]  Complete SECURING SHUTDOWN ENGINE [E - 4] .... COMPLETE

Engine Failure / Power Loss During Flight  [EMERGENCY]
Engine failure or power loss during flight
[ ]  Airspeed [MEMORY] .... 100 KIAS Minimum
[ ]  Mixtures [MEMORY] .... Full RICH (Forward)
[ ]  Propellers [MEMORY] .... Full HIGH RPM (Forward)
[ ]  Throttles [MEMORY] .... Full OPEN (Forward)
[ ]  Gear [MEMORY] .... UP
[ ]  Flaps [MEMORY] .... UP
[ ]  Affected Engine [MEMORY] .... Identify
[ ]  Throttle (Affected Engine) [MEMORY] .... Retard (Verify)
IF CONDITIONS PERMIT
[ ]  Engine Instruments .... Check
[ ]  Fuel Selector .... Switch to Another Tank
[ ]  Boost Pump .... ON; If No Start, OFF
[ ]  Ignition Switch .... Check L, R, BOTH
[ ]  Throttle & Mixture .... Try Different Settings
IF ENGINE POWER IS NOT RESTORED OR CONDITIONS DO NOT WARRANT A RESTART ATTEMPT
[ ]  Propeller (Dead Engine) .... FEATHER
[ ]  Throttle / Propeller (Good Engine) .... Power As Required
[ ]  Cowl Flap (Good Engine) .... As Required
[ ]  Complete SECURING SHUTDOWN ENGINE [E - 4] .... COMPLETE

Securing Shutdown Engine  [EMERGENCY]
Securing a shutdown engine
[ ]  Fuel Selector .... OFF
[ ]  Boost Pump .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Ignition Switch .... OFF
[ ]  Alternator .... OFF
[ ]  Electrical Load .... Minimize
[ ]  Gear Warning Horn .... Reset (Throttle Midrange)
[ ]  Cowl Flap .... CLOSED

Restarting Secured Engine  [EMERGENCY]
Restarting a secured engine
[ ]  Ignition Switch .... BOTH
[ ]  Fuel Selector .... MAIN
[ ]  Mixture .... As Required for Altitude (Full RICH < 3000’ Dens Alt)
[ ]  Throttle .... Open ½”
[ ]  Propeller .... Full HIGH RPM Then Retard to Detent @ 1000 RPM
IF PROP DOES NOT WINDMILL WHEN PROP LEVER IS ADVANCED
[ ]  Propeller .... Retard to Detent
[ ]  Starter .... Engage Until Engine Starts or Windmills *
IF ENGINE DOES NOT START
[ ]  Boost Pump .... ON
IF START IS STILL UNSUCCESSFUL
[ ]  Boost Pump .... OFF
[ ]  Throttle .... Full OPEN (Forward)
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Mixture .... Full RICH Once Engine Starts
AFTER ENGINE STARTS
[ ]  Throttle .... 15" MP Until Cylinder Head Temperature > 200°F
[ ]  Engine Instruments .... Check
[ ]  Boost Pump .... OFF
[ ]  Alternator .... ON
[ ]  Cowl Flap .... As Required
NOTE: If Starter Fails to Crank the Engine, Possible Internal Failure is Indicated; Make No Further Attempt to Restart

Engine Failure During Final Approach  [EMERGENCY]
Engine failure during final approach
[ ]  Throttle / Propeller .... Power As Required
[ ]  Gear .... Check DOWN
[ ]  Flaps .... UP Slowly Unless Landing Assured

Single Engine Approach and Landing  [EMERGENCY]
Single engine approach and landing
[ ]  Final Approach Speed .... 100 KIAS Minimum
[ ]  Gear .... Delay till Landing Assured
[ ]  Flaps .... UP till Landing Assured

Single Engine Go Around  [EMERGENCY]
Single engine go around
[ ]  Airspeed [MEMORY] .... 100 KIAS (90 KIAS to Clear Obstacles)
[ ]  Throttle [MEMORY] .... Full OPEN (Forward)
[ ]  Propeller [MEMORY] .... Full HIGH RPM (Forward)
[ ]  Gear [MEMORY] .... UP
[ ]  Flaps [MEMORY] .... UP

Emergency Landing Without Engine Power  [EMERGENCY]
Emergency landing without engine power
[ ]  Airspeed [MEMORY] .... 110 KIAS (2.5 NM/1000')
[ ]  Gear [MEMORY] .... UP
[ ]  Flaps [MEMORY] .... UP
[ ]  Propellers [MEMORY] .... FEATHER
[ ]  Cowl Flaps [MEMORY] .... CLOSED
[ ]  Fuel Selectors [MEMORY] .... OFF
[ ]  Boost Pumps [MEMORY] .... OFF
[ ]  Mixtures [MEMORY] .... IDLE CUT-OFF
[ ]  Ignition Switches [MEMORY] .... OFF
[ ]  Seat Belts & Harnesses .... Tighten
[ ]  Cabin Door .... Unlatch Prior to Touchdown
[ ]  Squawk 7700 and Make a MAYDAY Call if Time Permits .... SQUAWK 7700
[ ]  ELT Remote Switch .... ON
[ ]  Gear .... As Situation Dictates
[ ]  Flaps .... 28° (Full Down) Once Landing Assured *
[ ]  Final Approach Speed .... 90 KIAS
[ ]  Battery & Alternators .... OFF Prior to Touchdown
[ ]  Emergency Exit Windows .... Jettison As Appropriate
NOTE: The gliding distance during flare will be significantly increased due to the feathered propellers

Ditching  [EMERGENCY]
Ditching
[ ]  Squawk 7700 and Make a MAYDAY Call if Time Permits .... SQUAWK 7700
[ ]  ELT Remote Switch .... ON
[ ]  Loose Objects .... Secure or Jettison
[ ]  Seat Belts & Harnesses .... Tighten
[ ]  Cabin Door .... Unlatch Prior to Touchdown
[ ]  Approach .... High Winds, Heavy Seas — Into the Wind; Light Winds, Heavy Swells — Parallel to Swells
[ ]  Gear .... UP
[ ]  Flaps .... 28° (Full Down)
[ ]  Throttles / Propellers .... Establish 300 Ft/Min Descent at 90 KIAS *
[ ]  Touchdown .... Level Attitude at 300 Ft/Min Descent
[ ]  Mixtures .... IDLE CUTOFF at Touchdown
NOTE: If no power available, approach at 98 KIAS with flaps up or 90 KIAS with 10° flaps

Engine Fire During Start on Ground  [EMERGENCY]
Engine fire during start on ground
[ ]  Starter [MEMORY] .... Continue Cranking
[ ]  Throttle [MEMORY] .... OPEN
IF FIRE CONTINUES OR ENGINE FAILS TO START
[ ]  Fuel Selectors .... OFF
[ ]  Mixtures .... IDLE CUT-OFF
[ ]  Ignition Switches .... OFF
[ ]  Battery & Alternators .... OFF
[ ]  Abandon Aircraft and Use Fire Extinguisher .... ABANDON
IF ENGINE STARTS
[ ]  Throttle .... 1700 RPM for 1 Minute
[ ]  Engine .... Shutdown and Inspect

Engine Fire on Ground  [EMERGENCY]
Engine fire on ground
[ ]  Fuel Selectors [MEMORY] .... OFF
[ ]  Mixtures [MEMORY] .... IDLE CUT-OFF
[ ]  Ignition Switches [MEMORY] .... OFF
[ ]  Battery & Alternators [MEMORY] .... OFF
[ ]  Abandon Aircraft and Use Fire Extinguisher [MEMORY] .... ABANDON

Engine Fire in Flight  [EMERGENCY]
Engine fire in flight
[ ]  Fuel Selector [MEMORY] .... OFF
[ ]  Boost Pump [MEMORY] .... OFF
[ ]  Mixture [MEMORY] .... IDLE CUT-OFF
[ ]  Propeller [MEMORY] .... FEATHER
[ ]  Ignition Switch [MEMORY] .... OFF
[ ]  Alternator [MEMORY] .... OFF
[ ]  Airspeed [MEMORY] .... Increase to Extinguish Fire
[ ]  Complete SECURING SHUTDOWN ENGINE [E - 4] .... COMPLETE

Wing Fire  [EMERGENCY]
Wing fire
[ ]  Battery & Alternators [MEMORY] .... OFF
[ ]  Airspeed [MEMORY] .... Increase to Extinguish Fire
[ ]  Slip to Keep Flames Away From Fuel Tanks and Cabin [MEMORY] .... SLIP
IF FIRE IS OUT AND ELECTRICAL POWER IS REQUIRED FOR FLIGHT
[ ]  Nav Lights .... OFF
[ ]  Landing Light .... OFF
[ ]  Strobe Lights .... OFF
[ ]  Pitot Heat .... OFF If Left Wing Affected
[ ]  Boost Pump .... OFF
[ ]  Battery & Alternators .... ON

Cabin or Electrical Fire in Flight  [EMERGENCY]
Cabin or electrical fire in flight
[ ]  Battery & Alternators [MEMORY] .... OFF
[ ]  Storm Window [MEMORY] .... CLOSED
[ ]  Defrost [MEMORY] .... OFF (Pull Out)
[ ]  Pilot & Copilot Air [MEMORY] .... CLOSED (Push In)
[ ]  Cabin Heater [MEMORY] .... OFF
[ ]  Fire Extinguisher .... As Required **
[ ]  Air Vents .... OPEN Once Fire is Out
IF FIRE IS OUT AND ELECTRICAL POWER IS REQUIRED FOR FLIGHT
[ ]  All Switches But Ignition .... OFF
[ ]  Circuit Breakers .... Check (DO NOT Reset)
[ ]  Battery .... ON
[ ]  Alternators .... ON Individually
[ ]  Electrical Switches .... ON, One at a Time
WARNING: Use caution when discharging fire extinguisher. HALON is extremely toxic. After discharging an extinguisher within a closed cabin, ventilate the cabin.

Fuel Pressure Drop or Nacelle Fuel Leak  [EMERGENCY]
Fuel pressure drop or nacelle fuel leak
ON THE GROUND
[ ]  Shutdown and Investigate .... SHUTDOWN
IN FLIGHT, IF A FUEL LEAK IS SUSPECTED
[ ]  Throttle .... Do Not Retard
[ ]  Fuel Selector .... OFF
[ ]  Propeller .... FEATHER (When Engine Quits)
[ ]  Complete SECURING SHUTDOWN ENGINE [E - 4] .... COMPLETE
IN FLIGHT, IF NO FUEL LEAK IS SUSPECTED (ENGINE DRIVEN FUEL PUMP FAILURE)
[ ]  Boost Pump .... ON
[ ]  Mixture .... As Required
[ ]  Land as Soon as Practicable .... LAND
IF FUEL PRESSURE OR NORMAL ENGINE OPERATION NOT RESTORED
[ ]  Engine With Inop Pump .... Switch Tanks or Crossfeed

Fluctuating Fuel Pressure  [EMERGENCY]
Fluctuating fuel pressure
[ ]  Mixture .... Full RICH
[ ]  Boost Pump .... ON
[ ]  Mixture .... As Required

Crossfeed  [EMERGENCY]
Crossfeed
[ ]  Fuel Selector (Supply Side) .... MAIN or AUX
[ ]  Fuel Selector (Receive Side) .... CROSSFEED
[ ]  Fuel Pressure .... Check

Low Oil Pressure With Normal Oil Temperature  [EMERGENCY]
Low oil pressure with normal oil temperature
[ ]  Reduce Power on Affected Engine .... REDUCE
[ ]  Conserve Altitude Until Landing is Assured .... CONSERVE
[ ]  Land as Soon as Practicable .... LAND

Low Oil Pressure With High Oil Temperature  [EMERGENCY]
Low oil pressure with high oil temperature (engine failure is imminent)
[ ]  Throttle .... Reduce
[ ]  Propeller .... Minimum RPM
[ ]  Consider Shutting Down Affected Engine Once Landing is Assured .... CONSIDER

Chip Detector Warning Light  [EMERGENCY]
Chip detector warning light
[ ]  Engine Instruments .... Monitor
[ ]  Land as Soon as Practicable .... LAND
[ ]  Consider Shutting Down Affected Engine Once Landing is Assured .... CONSIDER

Single Alternator Failure  [EMERGENCY]
Single alternator failure (ammeter reads zero)
[ ]  Alternator .... OFF
[ ]  Electrical Load .... Minimize
[ ]  Land as Soon as Practicable .... LAND

Dual Alternator Failure  [EMERGENCY]
Dual alternator failure (both ammeters read zero)
IF OVERVOLTAGE WARNING LIGHT IS NOT ON
[ ]  Alternator Field Circuit Breaker .... Check (Lower Pilot Console)
[ ]  Alternator Circuit Breakers .... Check (Left Pilot Console)
[ ]  Alternators .... RE - EXC (Down) Then ON
IF OVERVOLTAGE WARNING LIGHT IS ON
[ ]  Voltage Regulator Switch .... Opposite Regulator
IF OVERVOLTAGE WARNING LIGHT DOES NOT GO OUT
[ ]  Alternator Field Circuit Breaker .... Pull (Lower Pilot Console)

Battery Charge Warning Light On in Flight  [EMERGENCY]
Battery charge warning light on in flight
[ ]  Voltage Regulator Switch .... Opposite Regulator
IF BATTERY CHARGE WARNING LIGHT DOES NOT GO OUT
[ ]  Battery .... OFF till Final Approach Then ON

Landing Gear Fails to Retract  [EMERGENCY]
Landing gear fails to retract
[ ]  DO NOT try to Retract Manually .... DO NOT
[ ]  Gear Switch .... DOWN
[ ]  Gear Indicator Light .... Check
[ ]  Gear Warning Horn .... Check (< 11” MP)

Landing Gear Fails to Extend  [EMERGENCY]
Landing gear fails to extend
[ ]  Gear Switch .... Check DOWN
[ ]  Gear Relay and Motor Circuit Breakers .... Check (Right Console) *
[ ]  Indicator Bulb .... Check
[ ]  Nose Gear Indicator .... Check
[ ]  Gear Position .... Check with an Observer
[ ]  Gear Recycle .... (If Appropriate)
IF GEAR STILL FAILS TO EXTEND
[ ]  Gear Switch .... DOWN
[ ]  Gear Motor Circuit Breaker .... Pull (Right Console)
[ ]  Emergency Hand Crank .... Counterclockwise Until Gear Down Indication **
[ ]  Nose Gear Indicator .... Check
[ ]  Gear Horn .... Check (< 11” MP)
[ ]  Emergency Hand Crank .... Stow
NOTE: Allow circuit breaker to cool 3 minutes before resetting
NOTE: If complete electrical failure has occurred, turn handcrank counterclockwise AS FAR AS POSSIBLE (( 50 Turns)

For All Landings With a Gear Malfunction  [EMERGENCY]
All landings with a gear malfunction
[ ]  Reduce Fuel Load to a Minimum .... REDUCE
[ ]  Divert to a Field With Adequate Crash Response .... DIVERT
[ ]  Heater .... OFF
[ ]  Seat Belts and Harnesses .... Tighten
[ ]  Cabin Door .... Unlatch Prior to Touchdown
[ ]  Emergency Exit Windows .... Jettison As Appropriate
[ ]  Abandon Aircraft Immediately Once Stopped .... ABANDON

Gear-Up Landing  [EMERGENCY]
Gear-up landing
[ ]  Flaps .... 28° (Full DOWN)
[ ]  Final Approach Speed .... 90 KIAS
WHEN LANDING IS ASSURED
[ ]  Mixtures .... IDLE CUT-OFF
[ ]  Propellers .... FEATHER **
[ ]  Ignition Switches .... OFF
[ ]  Battery & Alternators .... OFF
[ ]  Fuel Selectors .... OFF

Landing With Only One Main Gear Extended  [EMERGENCY]
Landing with only one main gear extended
[ ]  Land With Crosswind on the Side of the Extended Gear .... LAND
[ ]  Flaps .... 28° (Full DOWN)
[ ]  Final Approach Speed .... 90 KIAS
AT TOUCHDOWN OR WHEN LANDING IS ASSURED
[ ]  Mixtures .... IDLE CUT-OFF
[ ]  Propellers .... FEATHER **
[ ]  Ignition Switches .... OFF
[ ]  Battery & Alternators .... OFF
[ ]  Fuel Selectors .... OFF
[ ]  Hold Nose Off as Long as Possible .... HOLD
[ ]  Brakes .... DO NOT Apply
NOTE: If time permits, rotate propellers to horizontal with starter

For All Landings With a Gear Malfunction  [EMERGENCY]
All landings with a gear malfunction
[ ]  Reduce Fuel Load to a Minimum .... REDUCE
[ ]  Divert to a Field With Adequate Crash Response .... DIVERT
[ ]  Heater .... OFF
[ ]  Seat Belts and Harnesses .... Tighten
[ ]  Cabin Door .... Unlatch Prior to Touchdown
[ ]  Emergency Exit Windows .... Jettison As Appropriate
[ ]  Abandon Aircraft Immediately Once Stopped .... ABANDON

Landing With the Nose Gear Up or Unsafe  [EMERGENCY]
Landing with the nose gear up or unsafe
[ ]  Flaps .... Minimum Required
[ ]  Final Approach Speed .... 90 KIAS
AT TOUCHDOWN OR WHEN LANDING IS ASSURED
[ ]  Mixtures .... IDLE CUT-OFF
[ ]  Propellers .... FEATHER **
[ ]  Ignition Switches .... OFF
[ ]  Battery & Alternators .... OFF
[ ]  Fuel Selectors .... OFF
[ ]  Lower Nosewheel Gently as Aircraft Slows .... LOWER

Landing With One Main Gear Up or Unsafe  [EMERGENCY]
Landing with one main gear up or unsafe
[ ]  Flaps .... 28° (Full Down)
[ ]  Final Approach Speed .... 90 KIAS
[ ]  Touchdown on the Side of the Runway of Extended Gear .... TOUCHDOWN
AT TOUCHDOWN OR WHEN LANDING IS ASSURED
[ ]  Mixtures .... IDLE CUT-OFF
[ ]  Propellers .... FEATHER **
[ ]  Ignition Switches .... OFF
[ ]  Battery & Alternators .... OFF
[ ]  Fuel Selectors .... OFF
NOTE: If time permits, rotate propellers to horizontal with starter

Tire Blow Out on Takeoff  [EMERGENCY]
Tire blow out on takeoff
[ ]  Do Not Retract Gear [MEMORY] .... DO NOT RETRACT

Landing With a Flat Main Tire  [EMERGENCY]
Landing with a flat main tire
[ ]  Use Crossfeed to Reduce Weight on Side of Flat Tire .... CROSSFEED
[ ]  If Practical, Land with any Crosswind From the Opposite Side of the Flat Tire .... LAND
[ ]  Flaps .... 28° (Full DOWN)
[ ]  Align With the Side of the Runway of the Good Tire .... ALIGN
[ ]  Touchdown .... Slightly Wing-Low on Side of the Good Tire
[ ]  Lower Nosewheel Immediately for Directional Control .... LOWER
[ ]  Braking .... On Good Wheel Only

Landing With a Flat Nose Tire  [EMERGENCY]
Landing with a flat nose tire
[ ]  Flaps .... Full DOWN
[ ]  Touchdown on the Center of the Runway .... TOUCHDOWN
[ ]  Control Wheel .... Full Aft to Minimize Weight on the Nose Wheel
[ ]  Braking .... Minimum Required

Spin  [EMERGENCY]
Spin
[ ]  Throttles [MEMORY] .... IDLE
[ ]  Ailerons [MEMORY] .... Neutral
[ ]  Rudder [MEMORY] .... Full Opposite the Direction of the Spin
[ ]  Control Wheel [MEMORY] .... Briskly Forward
[ ]  Rudder [MEMORY] .... Neutral Once Rotation Stops
[ ]  Recover Smoothly From Ensuing Dive [MEMORY] .... RECOVER

Emergency Descent  [EMERGENCY]
Emergency descent
[ ]  Throttles .... IDLE
[ ]  Propellers .... Full HIGH RPM (Forward)
[ ]  Mixtures .... Full RICH
[ ]  Gear .... DOWN (<143 KIAS)
[ ]  Flaps .... UP
[ ]  Max Airspeed .... 225 KIAS (143 for Training)

Propeller Overspeed  [EMERGENCY]
Propeller overspeed
[ ]  Airspeed .... Reduce (Increase Pitch)
[ ]  Throttle .... Reduce
[ ]  Propeller .... Retard to Detent
IF CONTROL IS NOT REGAINED BY CYCLING PROPELLER SEVERAL TIMES AND SAFE LANDING IS ASSURED WITH ONE ENGINE INOPERATIVE
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Propeller .... FEATHER
[ ]  Complete SECURING SHUTDOWN ENGINE [E - 4] .... COMPLETE
IF THE PROPELLER FAILS TO FEATHER
[ ]  Engine .... RESTART [E - 5]
[ ]  Throttle / Propeller .... Adjust for Minimum RPM
[ ]  Airspeed .... 100-110 KIAS

Cabin Door Open Inflight  [EMERGENCY]
Cabin door open in flight
[ ]  Land and Close Door Once Aircraft has Come to a Stop .... LAND
IF LANDING IS IMPRACTICAL
[ ]  Gear .... DOWN (< 143 KIAS)
[ ]  Flaps .... 28° (< 143 KIAS)
[ ]  Airspeed .... 95 KIAS
[ ]  Storm Window .... OPEN
[ ]  Push Door Open Against Slipstream Then Slam it Closed .... PUSH/SLAM

Pitot-Static System Failure  [EMERGENCY]
Pitot-static system failure
[ ]  Pitot Heat .... ON
[ ]  Alternate Static Source .... ON (Rotate Aft)
[ ]  Consult POH for Airspeed & Altitude Corrections .... CONSULT

Asymmetric Flaps  [EMERGENCY]
Asymmetric flaps
[ ]  Flaps .... Retract
[ ]  Make a No-Flap Landing .... LAND
IF ROLLING TENDENCY IS NOT REDUCED
[ ]  Flaps .... Adjust to Minimize Rolling Tendency
[ ]  Use Ailerons and Differential Power as Required .... USE

Fuel Tank Siphoning  [EMERGENCY]
Fuel tank siphoning
[ ]  Power .... Reduce
[ ]  Airspeed .... 120 KIAS
[ ]  Land as Soon as Practicable (Flaps 10° Max) .... LAND

After Emergency Landing  [EMERGENCY]
After emergency landing
[ ]  Battery .... Confirm OFF
[ ]  Abandon Aircraft Until All Danger of Fire is Passed .... ABANDON
WHEN IT IS SAFE TO RETURN TO THE AIRCRAFT
[ ]  ELT .... ON (ELT is located on right rear bulkhead behind the panel at the rear of the baggage area)
IF RADIO IS STILL OPERATIVE
[ ]  Make Periodic Mayday Call and Monitor 121.5 for Instructions .... MAYDAY

Radio Failure  [EMERGENCY]
Radio failure
[ ]  Audio Controls .... Check
[ ]  Circuit Breakers .... Check
[ ]  Attempt Contact on Another Frequency .... ATTEMPT
[ ]  Speaker .... ON
[ ]  Attempt Contact Using Hand Held Microphone .... ATTEMPT
IF RADIO CONTACT CANNOT BE ESTABLISHED AND IS REQUIRED (CLASS B, C, AND D AIRSPACE)
[ ]  Transponder .... 7600
[ ]  Continue Transmissions (Only Receiver May Be Inop) .... CONTINUE
[ ]  Monitor Navaids For Voice Transmissions .... MONITOR
NOTE: Allow circuit breaker to cool 3 minutes before resetting
ATC LIGHT SIGNALS
[ ]  Steady Green — On the Ground: Cleared for takeoff; In Flight: Cleared to land .... STEADY GREEN
[ ]  Flashing Green — On the Ground: Cleared for taxi; In Flight: Return for landing (to be followed by steady green) .... FLASHING GREEN
[ ]  Steady Red — On the Ground: STOP; In Flight: Give way to other aircraft and continue circling .... STEADY RED
[ ]  Flashing Red — On the Ground: Taxi clear of the runway in use; In Flight: Airport unsafe, do not land .... FLASHING RED
[ ]  Flashing White — On the Ground: Return to starting point on airport; In Flight: Not applicable .... FLASHING WHITE
[ ]  Alternating Red and Green — On the Ground: Exercise extreme caution; In Flight: Exercise extreme caution .... ALTERNATING
NOTE: Acknowledge all light signals by flashing landing light or rocking aircraft’s wings.

NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
Source: Beechcraft/BE-55 _ BE-58 Baron/Baron_eps_cklist.txt
Rights: licensed
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Verify against the aircraft's own approved documentation before use.
