Beechcraft BE-95 Travel Air — Beech95-checklist_selkirk_college
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Hot or Flooded Start" item count differs between passes (16 vs 15); verify nothing was dropped.
content_gap: Section "Pre-Takeoff" item count differs between passes (28 vs 27); verify nothing was dropped.

Pre Start
[ ]  Hobbs .... Checked
[ ]  Dispatch log .... Completed
[ ]  Logs and documents .... On board & valid
[ ]  Passenger briefing .... Completed
[ ]  Seats and belts .... Locked and secure *
[ ]  Controls .... Free and correct
[ ]  Parking brake .... Set
[ ]  Circuit breakers .... All in
[ ]  Electrics .... Off
[ ]  Alternators .... Off
[ ]  Avionics emergency .... Off
[ ]  Avionics master .... Off
[ ]  Gear selector .... Down
[ ]  Battery .... On, Gear locked
[ ]  Fuel Quantities .... Checked
[ ]  Fuel selectors .... On Aux.
[ ]  Flaps .... Up
[ ]  Cowl flaps .... Open
[ ]  Beacon .... On

Cold Engine Start
[ ]  Mixtures .... Full rich
[ ]  Propellers .... Full fine
[ ]  Throttles .... Set
[ ]  Boost pumps .... Checked & primed
[ ]  Left engine (start) .... Started
[ ]  Oil Pressure .... Normal
[ ]  Left Suction .... Normal
[ ]  Left Alternator .... On
[ ]  Right engine (start) .... Started
[ ]  Oil pressure .... Normal
[ ]  Right Suction .... Normal
[ ]  Right alternator .... On, Load split
[ ]  Engine gauges .... Normal

Hot or Flooded Start
[ ]  Mixtures .... Full rich
[ ]  Propellers .... Full fine
[ ]  Throttles .... Full forward
[ ]  Boost Pumps .... Checked & primed
[ ]  Mixtures .... Idle cut off
[ ]  Throttles .... Set
[ ]  Left engine (start) .... Started
[ ]  Oil pressure .... Normal
[ ]  Left Suction .... Normal
[ ]  Left Alternator .... On
[ ]  Right engine (start) .... Started
[ ]  Oil Pressure .... Normal
[ ]  Right Suction .... Normal
[ ]  Right alternator .... On, Load split
[ ]  Engine gauges .... Normal


Post Start
[ ]  Avionics master .... On
[ ]  PN-101 .... On and slave set
[ ]  Electrics .... On (as req=d)
[ ]  ELT .... Checked
[ ]  Instrument panel .... Panel checked
[ ]  Radios .... Radios checked
[ ]  Left fuel selector .... On crossfeed

Taxi
[ ]  Brakes .... Checked *
[ ]  Fuel crossfeed .... Checked
[ ]  Instruments .... Checked

Runup
[ ]  Parking brake .... Set
[ ]  Fuel selectors .... Quantity checked, on mains
[ ]  Mixtures .... Full rich
[ ]  Propellers .... Full fine
[ ]  Engine gauges .... Normal
[ ]  Throttles .... 2200
[ ]  Engine gauges .... Normal
[ ]  Suction .... Normal
[ ]  Propellers .... Exercised
[ ]  Throttles .... 2000
[ ]  Magnetos .... Checked
[ ]  Mixtures .... Checked
[ ]  Alternators .... Checked
[ ]  Alternate airs .... Checked
[ ]  Throttles .... 1500
[ ]  Feather .... Checked
[ ]  Throttles .... Idle checked, 1300 Set

Pre-Takeoff
[ ]  Seats & belts .... Locked & secure *
[ ]  Controls .... Free
[ ]  Trims .... Three set
[ ]  Fuel selectors .... Quantity checked, on Mains
[ ]  Alternate airs .... Off
[ ]  Flaps .... Set for takeoff
[ ]  Cowl flaps .... Open
[ ]  Circuit breakers .... All in
[ ]  Alternate static .... Checked and off
[ ]  Magnetos .... Both on both
[ ]  Alternators .... On
[ ]  Mixtures .... Full rich
[ ]  Propellers .... Full fine
[ ]  Altimeters .... _____ set
[ ]  Clock .... ______checked
[ ]  Heading indicators .... Checked & set
[ ]  Rear windows .... Closed & locked
[ ]  IFR clearance .... Clearance reviewed
[ ]  Crew briefing .... Briefing completed
[ ]  Cabin door & window .... Closed & locked *
[ ]  Boost pumps .... On
[ ]  Landing light .... On (if req=d)
[ ]  Pulse light .... On
[ ]  Pitot heat .... On (if req=d)
[ ]  Transponder .... On Alt ______
[ ]  Takeoff time .... Noted
[ ]  Heading indicator .... Checked on runway


Post Takeoff
[ ]  Gear .... Up
[ ]  Flaps .... Up
[ ]  Power .... Set
[ ]  Fuel selectors .... Quantity checked, on Aux
[ ]  Boost pumps .... Off
[ ]  Cowl flaps .... Set
[ ]  Landing light .... Off

Pre-Landing
[ ]  Seats & belts .... Locked & secure
[ ]  Parking brake .... Off
[ ]  Mixtures .... Full rich
[ ]  Propellers .... 2500
[ ]  Magnetos .... Both on both
[ ]  Electrics .... On (as req=d)
[ ]  Boost pumps .... On
[ ]  Fuel selectors .... Quantity checked, on mains
[ ]  Landing light .... On (if req=d)
[ ]  Gear .... Down & locked

Post Landing
[ ]  Flaps .... Up
[ ]  Cowl flaps .... Open
[ ]  Boost pumps .... Off
[ ]  Minimum electrics .... Set
[ ]  Transponder .... Standby

Shut Down
[ ]  Parking brake .... Set
[ ]  Throttles .... 1100
[ ]  ELT .... Checked
[ ]  Electrics .... Off
[ ]  Avionics master .... Off
[ ]  Battery .... Off
[ ]  Alternators .... Off
[ ]  Throttles .... Idle
[ ]  Live/dead mag .... Checked
[ ]  Mixtures .... Idle cut off
[ ]  Magnetos .... off

Rejected Takeoff Before Lift-off  [EMERGENCY]
[ ]  Throttles [MEMORY] .... closed
[ ]  Braking [MEMORY] .... maximum
[ ]  Stop [MEMORY] .... on remaining runway
IF THERE IS INSUFFICIENT RUNWAY TO STOP:
[ ]  Switches (master and alternators) [MEMORY] .... off
[ ]  Fuel Selectors [MEMORY] .... off

Rejected Takeoff - Airborne  [EMERGENCY]
[ ]  Throttles [MEMORY] .... as required, then off
[ ]  Braking [MEMORY] .... maximum
[ ]  Stop [MEMORY] .... on remaining runway
IF THERE IS INSUFFICIENT RUNWAY TO LAND AND STOP:
[ ]  Switches (master and alternators) [MEMORY] .... off
[ ]  Fuel Selectors [MEMORY] .... off

Engine Failure - Continuing Takeoff  [EMERGENCY]
[ ]  Control [MEMORY] .... Yaw and roll.
[ ]  Attitude [MEMORY] .... to control airspeed
[ ]  Power [MEMORY] .... full
[ ]  Drag [MEMORY] .... retract flaps and gear
[ ]  Identify [MEMORY] .... retard throttle on suspected engine
[ ]  Feather [MEMORY] .... propeller on failed engine
[ ]  Mixture [MEMORY] .... ico on failed engine
[ ]  Climb [MEMORY] .... at best S/E climb speed
[ ]  Trim [MEMORY] .... rudder, elevator, ailerons
GO TO: Complete Failed Engine Shutdown Checklist

Engine Failure ..Cruise  [EMERGENCY]
[ ]  Control [MEMORY] .... Adverse yaw and roll
[ ]  Attitude [MEMORY] .... altitude... (airspeed above Vyse)
[ ]  Power [MEMORY] .... to climb power
[ ]  Drag [MEMORY] .... confirm flaps and gear retracted
[ ]  Identify [MEMORY] .... retard throttle on suspected engine
[ ]  Check for Fire [MEMORY] .... if no fire
[ ]  Cause [MEMORY] .... check fuel pressure
[ ]  Boost pumps .... on
[ ]  Check fuel quantity
[ ]  Switch fuel tank .... as req=d
[ ]  Alternate air .... both on
[ ]  Magnetos .... on
[ ]  Test [MEMORY] .... advance throttle on affected engine.
IF ENGINE DOES NOT RE-START --- 9 TO 10
[ ]  Feather [MEMORY] .... prop control to feather detent
[ ]  Mixture [MEMORY] .... Idle cut-off
GO TO: Complete Failed Engine Shutdown Checklist

Failed Engine Shutdown Checklist  [EMERGENCY]
[ ]  Throttle .... closed on failed engine
[ ]  Prop control .... feather detent
[ ]  Mixture control .... idle cut-off
[ ]  Drag .... confirm flaps and gear as req=d
[ ]  Cowl flap .... closed
[ ]  Boost pump .... off
[ ]  Magnetos .... off (one at a time)
[ ]  Alternator .... off
[ ]  Fuel selector .... off
[ ]  Reduce electrical load
[ ]  Monitor condition of remaining engine
[ ]  Declare an emergency
[ ]  Land at nearest suitable aerodrome

Precautionary Engine Shutdown  [ABNORMAL]
[ ]  Throttle .... closed on failed engine
[ ]  Prop control .... feather detent
[ ]  Mixture control .... idle cut-off
[ ]  Drag .... confirm flaps and gear as req=d
[ ]  Cowl flap .... closed
[ ]  Boost pump .... off
[ ]  Magnetos .... off (one at a time)
[ ]  Alternator .... off
[ ]  Fuel selector .... off
[ ]  Reduce electrical load
[ ]  Monitor condition of remaining engine
[ ]  Declare an emergency
[ ]  Land at the nearest suitable aerodrome

Engine Restart In Flight  [ABNORMAL]
[ ]  Fuel Selector .... on main or aux.
[ ]  Magnetos .... on
[ ]  Boost pump .... on
[ ]  Mixture control .... idle cut-off
[ ]  Throttle .... open 2 inch
[ ]  Propeller control .... move into governing range
[ ]  Once engine is wind-milling, advance mixture to the full rich position.
[ ]  Warm up engine .... at 2000 RPM and 15" MAP
[ ]  Alternator .... on
[ ]  All cockpit switches and controls .... normal.

Engine Fire on Start-up  [EMERGENCY]
[ ]  Mixture [MEMORY] .... idle cut-off
[ ]  Throttle [MEMORY] .... full open
[ ]  Cranking [MEMORY] .... continue
IF FIRE CONTINUES LONGER THAN A FEW SECONDS
[ ]  Fuel selectors [MEMORY] .... both off
[ ]  Mixture controls [MEMORY] .... both idle cut-off
[ ]  Switches [MEMORY] .... off
[ ]  Evacuate the aircraft [MEMORY]
NOTE: Extinguish the fire with ground equipment if practical.

Engine Fire in Flight  [EMERGENCY]
[ ]  Fuel selector [MEMORY] .... off
[ ]  Mixture [MEMORY] .... idle cut-off
[ ]  Propeller [MEMORY] .... feather
[ ]  Boost pump .... off
[ ]  Magneto switch .... off
[ ]  Alternator .... off
NOTE: If fire continues, consider increasing airspeed in an attempt to extinguish it.
[ ]  Declare an emergency and indicate intentions.
[ ]  Expedite your approach to the nearest suitable landing area.

Cabin Fire  [EMERGENCY]
[ ]  Vents [MEMORY] .... close
[ ]  Extinguisher [MEMORY] .... activate if necessary.
NOTE: (Get assistance from passengers if needed).
[ ]  Ventilate [MEMORY] .... the cabin
[ ]  Land .... as soon as practicable.
[ ]  Inspect for damage.

Landing Gear Manual Extension  [ABNORMAL]
[ ]  Reduce speed .... to 120 KIAS or less
[ ]  Landing gear motor circuit breaker .... pulled
[ ]  Landing gear selector .... down
[ ]  Engage the hand- crank and turn counter-clockwise as far as possible (approx. 50 turns).
[ ]  Check mechanical indicator to ascertain that the gear is down.
[ ]  If electrical system is operative, check gear position light and warning horn.
[ ]  Disengage hand-crank.
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