Beechcraft Beech 18 — david_a_seest_Beech_18_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Pre-Start Checklist
[ ]  1.  Cabin Door .... CLOSED
[ ]  2.  Controls .... FREE
[ ]  3.  Landing Gear SW. .... DOWN
[ ]  4.  Parking Brake .... ON
[ ]  5.  Bat. & Gen. SWS. .... ON
[ ]  6.  Gear Safe Light .... CHECK
[ ]  7.  Fuel Quantity .... CHECK
[ ]  8.  Fuel Selectors .... MAIN
[ ]  9.  Crossfeed .... OFF
[ ]  10.  Anti-Ice Fluid .... CHECKED
[ ]  11.  Trim .... SET > T/O
[ ]  12.  Flap Switch .... NEUTRAL
[ ]  13.  Throttles .... 1/8 OPEN
[ ]  14.  Mixtures .... RICH
[ ]  15.  Props. .... HIGH
[ ]  16.  Manifold Heat .... COLD
[ ]  17.  Oil Shutters .... HOT
[ ]  18.  Oil Shutoff Valves .... OPEN
[ ]  19.  Circuit Breakers .... CHECKED
[ ]  20.  Electrical Switchs .... OFF
[ ]  21.  Alt. Static Source .... NORMAL
[ ]  22.  Oil By-Pass Valves .... AS REQUIRED
[ ]  23.  Warning Lights .... CHECKED

Start Checklist
[ ]  1.  Fuel Boost Pumps .... ON
[ ]  2.  Magnetos .... OFF
[ ]  3.  Engine Sel. SW. .... RT or LT
[ ]  4.  Starter (2 Revs) .... ENGAGE
[ ]  5.  Magnetos. .... ON
[ ]  6.  Ignition Boost SW. .... ON
[ ]  7.  Primer .... AS REQUIRED
NOTE: (SAME PROC. FOR OTHER ENGINE)
[ ]  8.  Fuel Boost Pumps .... OFF
[ ]  9.  Warm Up Engines .... 1000-1200 RPM

After-Starting Engines
[ ]  1.  Oil Pressure .... UP
[ ]  2.  Fuel Boost Pumps .... OFF
[ ]  3.  Lights .... AS REQUIRED
[ ]  4.  Radios .... ON
[ ]  5.  Tailwheel .... UNLOCKED
[ ]  6.  Parking Brake .... UNLOCKED

Run-Up
[ ]  1.  Temps. & Press. .... GREEN ARC
[ ]  2.  Props (1500 rpm) .... EXERCISE
[ ]  3.  Manifold Heat .... CHECK
[ ]  4.  Vacuum .... CHECK
[ ]  5.  Volt/Ammeters .... CHECK
[ ]  6.  Mags. (1800 rpm) .... CHECK

Before Take-Off
[ ]  1.  Controls .... FREE
[ ]  2.  Mixture .... RICH
[ ]  3.  Props. .... HIGH RPM
[ ]  4.  Friction Locks .... SET
[ ]  5.  Oil Shutters .... AS REQUIRED
[ ]  6.  Manifold Heat .... COLD
[ ]  7.  Flaps .... UP
[ ]  8.  Fuel Selector .... MAIN TANKS
[ ]  9.  Oil By-Pass .... CLOSED
[ ]  10.  Trim .... SET
[ ]  11.  D.G.’s .... SET
[ ]  12.  Instruments .... CHECK
[ ]  13.  Navs. .... CHECK / SET

Take-Off
[ ]  1.  Time .... RECORD
[ ]  2.  Fuel Boost Pumps .... ON
[ ]  3.  Landing Lights .... ON
[ ]  4.  Inverter .... ON
[ ]  5.  Transponder .... ALT
[ ]  6.  Tail Wheel .... LOCKED
[ ]  7.  D.G.’s .... R.W. HEADING
[ ]  8.  Pitot Heat .... AS REQUIRED
[ ]  9.  Throttles .... 36.5” & 2300 RPM
[ ]  10.  Oil Pressure .... GREEN ARC
[ ]  11.  Oil Temperature .... GREEN ARC

Climb
[ ]  1.  Gear .... UP
[ ]  2.  Flaps .... UP
[ ]  3.  Manifold Pressure .... 32”
[ ]  4.  Prop. RPM .... 2150 RPM
[ ]  5.  Fuel Boost Pumps .... OFF – PX CK
[ ]  6.  Landing Lights .... OFF
[ ]  7.  Airspeed .... 120/140 MPH
[ ]  8.  Flight Plan .... OPEN

Cruise
[ ]  1.  Manifold Pressure .... 28”
[ ]  2.  Prop. RPM .... 2000 RPM
[ ]  3.  Mixture .... Lean
[ ]  4.  Oil Shutters .... 150 F.
[ ]  5.  Manifold Heat .... AS REQUIRED
[ ]  6.  Fuel Quantity .... Manage

Approach / Descent Checklist
[ ]  1.  Customs Code .... OBTAIN
[ ]  2.  Fuel Selectors .... MAIN TANKS
[ ]  3.  Mixtures .... ENRICHEN
[ ]  4.  Manifold Pressure .... 26”
[ ]  5.  Manifold Heat .... AS REQUIRED
[ ]  6.  Altimeters .... SET
[ ]  7.  Navs .... SET
[ ]  8.  Flight Plan .... CLOSED

Before Landing Checklist
[ ]  1.  Fuel Boost Pumps .... ON
[ ]  2.  Landing Lights .... ON
[ ]  3.  Props. .... 2150 RPM
[ ]  4.  Landing Gear .... DOWN/GREEN
[ ]  5.  Manifold Heat .... OFF
[ ]  6.  Heater .... CYCLE
[ ]  7.  Brakes .... CHECK
[ ]  8.  Flaps .... AS NEEDED

After Landing Checklist
[ ]  1.  Fuel Boost Pumps .... OFF
[ ]  2.  Landing Lights .... OFF
[ ]  3.  Inverter .... OFF
[ ]  4.  Transponder .... STBY
[ ]  5.  Props. .... HIGH RPM
[ ]  6.  Oil Shutters .... 150 F.
[ ]  7.  Flaps .... UP
[ ]  8.  Pitot Heat .... OFF
[ ]  9.  Taxi Lights .... AS REQUIRED
[ ]  10.  Time .... RECORD

Shutdown Checklist
[ ]  1.  Parking Brake .... SET
[ ]  2.  Radios .... OFF
[ ]  3.  Mixtures .... IDLE CUT-OFF
[ ]  4.  Magnetoes .... OFF
[ ]  5.  Battery/Gen SW’s .... OFF
[ ]  6.  Tailwheel .... LOCK
[ ]  7.  Controls .... LOCK
[ ]  8.  Tiedowns .... (3 POINTS)
[ ]  9.  Chocks .... ALL WHEELS

Airspeeds – Miles-Per-Hour
NOTE: Vne 257  Vyse 122    Vmc 86
NOTE: Vno 205  Vyxe 110    Vle 160
NOTE: Vy 135   Vlo 160     Vx 119
NOTE: Va 153   Vfe 120     Vso 75
NOTE: Vs 80    Max T\O Wt:  10,100
NOTE:     Max Lnd Wt:    9,800
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