Bell 206 _ 206B _ 206L Skywagon _ Super Skywagon — aid_smith_bell_206_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "After Landing / Shutdown" item count differs between passes (11 vs 10); verify nothing was dropped.
content_gap: Section "Other Emergencies" item count differs between passes (21 vs 20); verify nothing was dropped.

Initial
[ ]  Batt .... On
[ ]  Fuel .... Check
[ ]  Fuel Boost .... Out
[ ]  CBs
[ ]  Anti-Col .... On
[ ]  Batt .... Off

Exterior
[ ]  Surfaces .... Condition
[ ]  Batt .... Connected
[ ]  Levels .... Correct
[ ]  Hatches .... Secure
[ ]  Drains .... Clear
[ ]  Tx Temp Plate .... Colour Check
[ ]  Filters .... Check
[ ]  Filler Caps .... Secure
[ ]  G'box Mounts .... Check
[ ]  TR Drive .... Free splines
[ ]  Blades .... Free & positioned

Interior
[ ]  General .... Condition
[ ]  Fire Extinguisher .... Check
[ ]  Headsets .... Sufficient
[ ]  Lifejackets .... Sufficient
[ ]  Pax Brief Cards .... Sufficient
[ ]  Co-pilot Controls .... Removed?
[ ]  Co-pilot Harness .... Secure?
[ ]  Cabin Loading .... Correct
[ ]  Doors .... Secure

Pre-Start
[ ]  Harness .... Secure
[ ]  Pedals .... Adjusted
[ ]  Controls .... Full & Free
[ ]  Throttle .... Full & Free, Closed
[ ]  Avionics .... Off
[ ]  Electrics .... Off, except Anti-Col
[ ]  Batt .... Off (Extnl Start)
[ ]  Wander Light .... Off
[ ]  Heater .... Off
[ ]  Firewall Shutoff .... Open
[ ]  Rotor Brake .... Off
[ ]  CBs .... In except gyros
[ ]  Warnings .... Test
[ ]  TOT Light .... Test (if fitted)
[ ]  Fuel Boost Pumps .... Check & On
[ ]  OAT .... Note
[ ]  Instruments .... Check
[ ]  Fuel Valve .... On & Guarded
[ ]  Hyd Switch .... On
[ ]  Ant-Ice .... Off
[ ]  Landing Light .... Off
[ ]  Throttle .... Closed
[ ]  Collective .... Down

Engine Start
[ ]  Rotors .... Clear & Untied
[ ]  Starter .... Engage & Hold
[ ]  Oil Pressure .... Rising
[ ]  TOT .... <150 ºC
[ ]  By 25 % N1 .... Rotor Turning
[ ]  58 % N1 .... Release Starter
[ ]  Throttle .... Assist through yellow
[ ]  Ts & Ps .... Check
[ ]  60-62% N1 .... Idle for 1 min
[ ]  Ext Pwr .... Out/Batt On
[ ]  Throttle .... Open to 70 % N1
[ ]  Gen .... On, Check Load
[ ]  Caution CB .... In
[ ]  Avionics & Electrics .... On
[ ]  Hyd Switch .... Off, Check Runaway

Engine Run-Up
[ ]  Hyd System .... Check
[ ]  Anti-Ice .... Check
[ ]  Throttle .... Idle, N1 61-63% in 3 Secs
[ ]  Throttle .... Fully Open

Pre Take-Off
[ ]  CBs .... In
[ ]  Fuel .... Check
[ ]  Ts & Ps .... Check
[ ]  Instruments .... Set & Aligned
[ ]  Warning Lights .... Out
[ ]  Lights .... A/R
[ ]  Radios .... A/R
[ ]  Flotation Gear .... A/R
[ ]  Doors & Harnesses .... Secure
[ ]  Frictions .... Adjust
[ ]  Throttle .... Fully Open

After Take-Off
[ ]  Hover Power .... Check Perf
[ ]  Ts & Ps .... Check
[ ]  NR .... 100%

En-Route / Cruise
[ ]  Fuel .... Sufficient
[ ]  Warning Lights .... Clear
[ ]  Ts & Ps .... Check
[ ]  DG .... Aligned
[ ]  Altimeter .... Setting
[ ]  Anti-Ice .... A/R, check OAT

After Landing / Shutdown
[ ]  Collective .... Down
[ ]  Throttle .... Idle for 2 mins
[ ]  Frictions .... On
[ ]  Avionics & Electrics .... Off
[ ]  Anti-Ice & Heater .... Off
[ ]  Throttle (2 mins) .... Close, hold
[ ]  Boost Pumps .... Off
[ ]  30-38% .... Rotor Brake
[ ]  Batt .... Off
[ ]  Rotor .... Tie Down
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Warning Lights  [ABNORMAL]
BATT HOT (TEMP > 140 ºF)
[ ]  Batt .... Off
[ ]  Land .... ASAP
ENGINE OUT (AUDIO, N1<55%)
[ ]  Autorotation .... Establish
[ ]  Investigate Failure .... If Time
[ ]  Passengers .... Warn
[ ]  EOL .... Complete
ROTOR LOW ROM (AUDIO)
[ ]  Pitch .... Reduce
[ ]  Throttle .... Check Open
TRANS TEMP (TEMP > RED LINE)
[ ]  Ts & Ps .... Check
[ ]  Power .... Reduce
[ ]  Land .... ASAP
TRANS TEMP (PX BELOW MINIMUM)
[ ]  Pressure Gauge .... Check
[ ]  Land .... ASAP
GEN FAIL
[ ]  Gen Switch .... Reset & On
[ ]  Loadshed .... A/R < 6000 ft
[ ]  Land .... ASA Practical
FUEL FILTER (CLOGGED)
[ ]  Land .... ASA Practical
[ ]  Filter .... Clean
CHIP - ENG, TRANS OR T/R
[ ]  Land .... ASAP
BATT TEMP (TEMP > 130ºF)
[ ]  Batt .... Off until Light Out
FUEL PUMP (ONE OR BOTH INOPERATIVE)
[ ]  CBs .... Check
SINGLE FAIL:
[ ]  Altitude .... Below 6000 ft
[ ]  Land .... ASA Practical
DOUBLE FAIL:
[ ]  Land .... ASAP

Other Emergencies  [EMERGENCY]
ENGINE FIRE ON GROUND
[ ]  Throttle .... Close to Shutoff
[ ]  Starter .... Motor
[ ]  Fuel Valve .... Off
[ ]  Ignition CB .... Out
ENGINE FIRE IN FLIGHT
[ ]  Throttle .... Close to Shutoff
[ ]  Autorotation .... Establish
[ ]  Passengers .... Warn
[ ]  Fuel Valve .... Off
[ ]  Boost Pumps .... Off
[ ]  R/T .... Transmit Mayday
[ ]  EOL .... Complete
HYDRAULIC SYSTEM FAILURE
[ ]  Airspeed .... 61 - 69 kts
[ ]  Hydraulic CB .... Out
NOT RESTORED:
[ ]  Hydraulic CB .... In
[ ]  Hyd Switch .... Off
[ ]  Land .... ASA Practical
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