Bell 206 _ 206B _ 206L Skywagon _ Super Skywagon — Eric_Triantafilo_Cessna_206_Super_Skywagon_Checklists
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "ENGINE FAILURE" item count differs between passes (16 vs 15); verify nothing was dropped.

BEFORE START
[ ]  EXTERIOR CHECK .... COMPLETE
[ ]  SEATS & SEAT BELTS .... ADJUST & LOCK
[ ]  DOOR .... LOCKED
[ ]  COWL FLAPS .... OPEN
[ ]  CIRCUIT BREAKERS .... CHECK
[ ]  MASTER .... ON
[ ]  FUEL SELECTOR .... FULLEST TANK
[ ]  RADIO SWITCHES .... OFF

START
[ ]  MIXTURE .... FULL RICH
[ ]  PROPELLER .... HIGH RPM
[ ]  THROTTLE .... FULL
[ ]  AUX FUEL PUMP .... LO & PRIME WITH HI
[ ]  THROTTLE .... ½ INCH OPEN
[ ]  STARTER .... ENGAGE
[ ]  THROTTLE .... 1000 RPM
[ ]  OIL PRESSURE .... CHECK
[ ]  AUX FUEL PUMP .... OFF
[ ]  LIGHTS .... AS REQUIERED
[ ]  TIME .... CHECK

BEFORE TAKE OFF
[ ]  INDUCTION AIR .... CLOSED
[ ]  COWL FLAPS .... OPEN
[ ]  FLIGHT CONTROLS .... CHECK
[ ]  ELEV & RUDDER TRIMS .... SET
[ ]  FLAPS .... CHECK & SET
[ ]  FLT INSTR. & RADIOS .... SET
[ ]  ENGINE INSTR. .... CHECK GREEN
[ ]  THROTTLE .... 1700 RPM
[ ]  MIXTURE .... CHECK
[ ]  MAGNETOS .... CHK (50 RPM MAX DIF.)
[ ]  PROPELLER .... CYCLE TO CHECK
[ ]  AMMETER .... CHECK
[ ]  SUCTION .... CHECK
[ ]  DOORS & WINDOW .... CLOSED & LOCKED
[ ]  LAND. & STROBE LTS .... ON
[ ]  TIME .... CHECK

AFTER LANDING
[ ]  COWL FLAPS .... OPEN
[ ]  FLAPS .... UP
[ ]  LANDING LIGHTS .... OFF
[ ]  TRANSPONDER .... STAND BY

SHUT OFF
[ ]  LIGHTS & RADIOS .... OFF
[ ]  MIXTURE .... IDLE CUT-OFF
[ ]  MAGNETOS .... OFF
[ ]  MASTER SWITCH .... OFF
[ ]  TIME .... CHECK

GENERAL SPECS
NOTE: Vx    78 MPH
NOTE: V l/d 80 MPH
NOTE: Vy    100 MPH
NOTE: Va    138 MPH
NOTE: V l/d 80 MPH
NOTE: Ground Run 380 mts.
NOTE: T.O. Dist over 50´    680 mts.
NOTE: Ground Roll      300 mts.
NOTE: L. Dist over 50´ 540 mts.
NOTE: Fuel Capacity_____________80 US GALLONS

TAKE OFF
[ ]  THROTTLE .... FULL (2700 RPM)
[ ]  ACCELERATE TO 70MPH .... ROTATE
[ ]  CLIMB SPEED .... 100 MPH

CLIMB
[ ]  FLAPS .... UP
[ ]  AIRSPEED .... 110 TO 120 MPH
[ ]  POWER .... 24,5´ X  2500 RPM
[ ]  MIXTURE .... LEAN
[ ]  COWL FLAPS .... AS REQUIRED
[ ]  LANDING LIGHTS .... OFF

CRUISE
[ ]  CRUISE POWER .... SET
[ ]  COWL FLAPS .... AS REQUIRED
[ ]  MIXTURE .... LEAN

DESCENT
[ ]  MIXTURE .... RICH
[ ]  POWER .... AS DESIRED
[ ]  COWL FLAPS .... CLOSED

BEFORE LANDING
[ ]  FUEL SELECTOR .... FULLEST TANK
[ ]  COWL FLAPS .... CLOSED
[ ]  AIRSPEED .... 90-100 MPH (FLAPS UP)
[ ]  LANDING LIGHTS .... ON
[ ]  FLAPS .... SET (BELOW 110MPH)
[ ]  MIXTURE .... RICH
[ ]  PROPELLER .... HIGH RPM
[ ]  AIRSPEED .... 80-90 MPH (FLAPS DOWN)

ENGINE FAILURE  [EMERGENCY]
[ ]  AIRSPEED .... 80 MPH
[ ]  MIXTURE .... RICH
[ ]  INDUCTION AIR .... OPEN
[ ]  PROPELLER .... HIGH RPM
[ ]  FUEL SELECTOR .... OPPOSITE TANK
[ ]  FUEL PUMP .... HI
[ ]  MAGNETOS .... BOTH
[ ]  ELECTRICAL LOAD .... REDUCE
[ ]  RESTART .... ATTEMP
NOTE: - IF RESTART IS NOT POSSIBLE, FIND A SUITABLE
NOTE: FIELD TO LAND ON AND PROCEED AS FOLLOWS -
[ ]  PASSENGERS .... BRIEF
[ ]  FLAPS .... 40º
[ ]  APPROACH SPEED .... 70 MPH
[ ]  LAND ON MAIN WHEELS FIRST, LOWER THE NOSE
[ ]  AND APPLY BRAKES HEAVILY.

MAX PERFORMANCE TAKE OFF
[ ]  FLAPS .... 20º
[ ]  BRAKES .... APPLY
[ ]  THROTTLE .... FULL (2700 RPM)
[ ]  BRAKES .... RELEASE
[ ]  ELEVATOR .... SLIGHTLY NOSE UP ATT.
[ ]  MAINTAIN Vx (78 MPH) UNTIL OBST. ARE CLEARED
[ ]  ACCELERATE TO 100 MPH THEN RETRACT FLAPS
[ ]  COWL FLAPS .... OPEN
CAUTION: DO NOT REDUCE POWER BEFORE FLAPS RETRACTION
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