Bellanca 7GCAA Citabria — laura_laster_7GCAA_chk_citabria
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Preflight
CABIN
[ ]  Magneto Switches .... off
[ ]  Master and Electrical Switches .... off
[ ]  Radio Switches .... off
[ ]  Flight Controls .... unlock and check
[ ]  Fuel Quantity Gauge .... check
RIGHT WING
[ ]  Fuel Sump .... drain
[ ]  Aileron .... check
[ ]  Navigation Lights .... check
[ ]  Pitot and Static Tube .... check
[ ]  Tiedown .... remove
[ ]  Fuel Quantity .... check quantity
[ ]  Fuel Caps .... secure
[ ]  Tire .... check
[ ]  Brakes .... check
NOSE
[ ]  Oil Quantity .... at least 6 quarts
[ ]  Engine Compartment .... check
[ ]  Windshield and Windows .... clean
[ ]  Propeller and Spinner .... check for nicks, security
[ ]  Fuel Sump .... drain
[ ]  Cowling .... secure
LEFT WING
[ ]  Fuel Sump .... drain
[ ]  Brakes .... check
[ ]  Tire .... check
[ ]  Fuel Quantity .... check quantity
[ ]  Fuel Caps .... secure
[ ]  Fuel Vent .... clear
[ ]  Tiedown .... remove
[ ]  Navigation Lights .... check
[ ]  Aileron .... check
EMPENNAGE
[ ]  Fuel Sump .... drain
[ ]  Antennas .... secure
[ ]  Control Surfaces, Hinges, and Attachments .... check
[ ]  Control Cables .... check
[ ]  Rudder Lock .... remove
[ ]  Tailwheel Assembly .... check
[ ]  Tire .... check
ENTIRE AIRCRAFT
[ ]  Inspection Covers .... secure
[ ]  Fabric Integrity .... check

Before Starting
[ ]  Passenger Briefing .... complete
[ ]  Seat Belts .... on
[ ]  Brakes .... set
NOTE: hold the brakes with your feet. Do not set the parking brake.
[ ]  Fuel .... on
[ ]  Mixture .... rich
[ ]  Prime as required
[ ]  Primer .... locked
[ ]  Radio and Electrical Switches .... off
[ ]  Master Switch .... on
[ ]  Beacon .... on
[ ]  Control Stick .... full aft
[ ]  Propeller Area .... clear
[ ]  Left Magneto Switch .... on
[ ]  Throttle .... open ¼ to ½ inch
[ ]  Starter .... engage
[ ]  Power .... 800 – 1000
[ ]  Right Magneto Switch .... on
[ ]  Oil Pressure .... check
[ ]  Mixture .... lean for taxi
[ ]  Altimeter .... set
[ ]  Brakes .... test
[ ]  Radio on, call for taxi

Before Takeoff
[ ]  Brakes .... set
[ ]  Mixture .... rich
[ ]  Control Stick .... full aft
[ ]  Power .... 2000 rpm
[ ]  Magnetos .... check
NOTE: Max drop 175 rpm, max difference 50 rpm
[ ]  Carb Heat .... check
[ ]  Engine Instruments .... check
[ ]  Power .... Reduce 800 – 1000
[ ]  Controls .... free and correct
[ ]  Trim .... set for takeoff
[ ]  Door and Windows .... latch
[ ]  Takeoff Performance .... review
[ ]  Engine Failure Brief .... complete
[ ]  Transponder .... on altitude
[ ]  Radio call for takeoff
[ ]  Landing Light .... on

Cruise
[ ]  Power .... 2400 rpm
[ ]  Trim .... set
[ ]  Mixture .... set
[ ]  Landing Light .... off

Before Landing
[ ]  Seat Belts .... secure
[ ]  Landing Light .... on
[ ]  Carb Heat .... check
[ ]  Mixture .... set
[ ]  Fuel .... on

After Landing
[ ]  Landing Light .... off
[ ]  Transponder .... off
[ ]  Mixture .... lean for taxi

Shutdown
[ ]  Radios and Electrical Switches (except beacon) .... off
[ ]  Mixture .... idle cutoff
[ ]  Magneto Switches .... off
[ ]  Beacon .... off
[ ]  Master Switch .... off
[ ]  Aircraft and Controls .... secure

Engine Fire During Start  [EMERGENCY]
[ ]  Starter .... crank engine
[ ]  Mixture .... idle cutoff
[ ]  Throttle .... open
[ ]  Fuel Selector .... off
[ ]  Abandon if fire continues

Engine Power Loss During Takeoff  [EMERGENCY]
[ ]  If sufficient runway remains for a normal landing, land straight ahead.
[ ]  If insufficient runway remains, maintain safe airspeed and make only shallow turns to avoid obstructions.
NOTE: If sufficient altitude has been gained to attempt a restart:
[ ]  Airspeed .... 80 mph
[ ]  Fuel Selector .... check on
[ ]  Mixture .... check rich
[ ]  Throttle .... full
[ ]  Carburetor Heat .... on
[ ]  Primer .... locked
[ ]  If power is not regained, proceed with Power Off Landing.

Engine Power Loss In Flight  [EMERGENCY]
[ ]  Fuel Selector .... check on
[ ]  Mixture .... rich
[ ]  Carburetor Heat .... on
[ ]  Engine Gauges .... check for indication
[ ]  Primer .... check locked
[ ]  Throttle .... full
NOTE: When power is restored:
[ ]  Carburetor Heat .... off
[ ]  If power is not restored, prepare for Power Off Landing.

Power Off Landing  [EMERGENCY]
[ ]  Locate suitable field.
[ ]  Establish spiral pattern 1000 ft. above field at downwind position for normal landing approach. When field can easily be reached, slow to 80 mph for shortest landing.
NOTE: When committed to landing:
[ ]  Ignition .... off
[ ]  Master Switch .... off
[ ]  Fuel Selector .... off
[ ]  Mixture .... idle cutoff
[ ]  Seat belt and harness .... tight

Fire In Flight  [EMERGENCY]
[ ]  Source of Fire .... check
ELECTRICAL FIRE (SMOKE IN CABIN):
[ ]  Master Switch .... off
[ ]  Cabin Heat .... off
[ ]  Land as soon as practicable.
ENGINE FIRE:
[ ]  Fuel Selector .... off
[ ]  Throttle .... closed
[ ]  Mixture .... idle cutoff
[ ]  Heater .... off
[ ]  Magnetos .... off
[ ]  Primer .... locked
[ ]  Proceed with Power Off Landing procedure.

Loss of Oil Pressure  [EMERGENCY]
[ ]  Land as soon as possible and investigate cause. Prepare for Power Off Landing.

High Oil Pressure  [EMERGENCY]
[ ]  Land at nearest airport and investigate the problem. Prepare for Power Off Landing.

Alternator Failure  [EMERGENCY]
[ ]  Verify failure.
[ ]  Reduce electrical load as much as possible.
[ ]  Alternator Circuit Fuses .... check
[ ]  Master Switch .... off (for 1 second) then on
NOTE: If no output:
[ ]  Master Switch .... off
[ ]  Reduce electrical load and land as soon as possible.

Spin Recovery  [EMERGENCY]
[ ]  Throttle .... idle
[ ]  Ailerons .... neutral
[ ]  Rudder .... full opposite direction of rotation
[ ]  Control Stick .... forward
[ ]  Smoothly regain level flight attitude.

Engine Roughness  [EMERGENCY]
[ ]  Carburetor Heat .... on
NOTE: If roughness continues after one minute:
[ ]  Carburetor Heat .... off
[ ]  Mixture .... adjust for max. smoothness
[ ]  Fuel Selector .... check on
[ ]  Engine Gauges .... check
[ ]  Magneto Switches .... “L” then “R” then both
NOTE: if operation is satisfactory on either one, continue on that magneto at reduced power and full “rich” mixture to first airport.
[ ]  Prepare for Power Off Landing.

Carburetor Icing  [EMERGENCY]
[ ]  Carburetor Heat .... on
[ ]  Mixture .... adjust for max. smoothness
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