Cessna 150 Commuter — aviatickyklub.cz_cessna_c150_engl_checklists
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

BEFORE STARTING ENGINE
[ ]  Exterior Preflight .... COMPLETE.
[ ]  Tach/Hobbs Meter .... RECORD
[ ]  Seats, Belts, Harnesses .... ADJUST & LOCKED.
[ ]  Fuel Shutoff Valve .... ON.
[ ]  Radios & Electrical Equipment .... OFF.
[ ]  Brakes .... TEST & SET.

STARTING ENGINE
[ ]  Mixture .... RICH.
[ ]  Carburetor Heat .... COLD.
[ ]  Master Switch .... ON.
[ ]  Prime .... AS REQUIRED.
[ ]  Throttle .... OPEN ¼ INCH.
[ ]  Propeller Area .... CLEAR.
[ ]  Ignition Switch .... START. (release when engine starts)
[ ]  Oil Pressure .... CHECK.

BEFORE TAKEOFF
[ ]  Cabin Doors .... LATCHED.
[ ]  Flight Controls .... FREE & CORRECT.
[ ]  Elevator Trim .... TAKEOFF POSITION.
[ ]  Fuel Shutoff Valve .... ON.
[ ]  Brakes .... SET.
[ ]  Throttle .... 1700 RPM.
[ ]  Magnetos .... CHECK.
[ ]  Carburetor Heat .... CHECK FOR RPM DROP.
[ ]  Engine Instruments and Ammeter .... CHECK.
[ ]  Suction Gauge .... CHECK.
[ ]  Flight Instruments and Radio .... SET.
[ ]  Throttle Friction Lock .... ADJUST.
[ ]  Wing Flaps .... AS REQUIRED.

TAKEOFF — Normal Takeoff
NORMAL TAKEOFF
[ ]  Wing Flaps .... UP (0).
[ ]  Carburetor Heat .... COLD.
[ ]  Throttle .... FULL OPEN.
[ ]  Elevator Control .... LIFT NOSE WHEEL.
[ ]  Climb Speed .... 70-80 MPH.

TAKEOFF — Maximum Performance Takeoff
MAXIMUM PERFORMANCE TAKEOFF
[ ]  Wing Flaps .... UP (0).
[ ]  Carburetor Heat .... COLD.
[ ]  Brakes .... HOLD.
[ ]  Throttle .... FULL OPEN.
[ ]  Brakes .... RELEASE.
[ ]  Elevator Control .... SLIGHTLY TAIL LOW.
[ ]  Climb Speed .... 70 MPH (with obstacles ahead).

ENROUTE CLIMB
[ ]  Airspeed .... 75 – 85 MPH.
[ ]  Throttle .... FULL OPEN.
[ ]  Mixture .... RICH. (Unless engine is rough).

CRUISE
[ ]  Power .... 2000 to 2750. (No more than 75%).
[ ]  Elevator Trim .... ADJUST.
[ ]  Mixture .... LEAN.

BEFORE LANDING
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON (apply before closing throttle).
[ ]  Airspeed .... 70-80 MPH (flaps up).
[ ]  Wing Flaps .... AS DESIRED (below 100 MPH)
[ ]  Airspeed .... 60-70 MPH (flaps down).

BALKED LANDING  [ABNORMAL]
[ ]  Throttle .... FULL OPEN.
[ ]  Carburetor Heat .... COLD.
[ ]  Wing Flaps .... RETRACT TO 20.
[ ]  Airspeed .... 65 MPH
[ ]  Wing Flaps .... RETRACT (slowly).

NORMAL LANDING
[ ]  Touchdown .... MAIN WHEELS FIRST.
[ ]  Landing Roll .... LOWER NOSE WHEEL GENTLY.
[ ]  Braking .... MINIMUM REQUIRED.

AFTER LANDING
[ ]  Wing Flaps .... UP.
[ ]  Carburetor Heat .... COLD.
[ ]  Unnecessary Equipment .... OFF.

SECURING AIRCRAFT
[ ]  Parking Brake .... SET
[ ]  Radios, Electrical Equipment .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF.
[ ]  Control Lock .... INSTALL.
[ ]  Tach/Hobbs Meter .... RECORD.

C150G/C150L Airspeeds (MCAS)
[ ]  Vr .... 55
[ ]  Vx .... 70
[ ]  Vy .... 78
[ ]  Va .... 109
[ ]  Vs1 .... 55
[ ]  Vso .... 48
[ ]  Vfe .... 100
[ ]  Vno .... 120
[ ]  Vne .... 162
[ ]  Glide .... 70
[ ]  XW demo .... 15
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