Cessna 150 Commuter — c150_abbreviated_millstone_valley_flight_school
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BEFORE STARTING ENGINE
[ ]  Exterior Preflight .... COMPLETE
[ ]  Tach/Hobbs Meter .... RECORD
[ ]  Seats, Belts, Harnesses .... ADJUST & LOCKED
[ ]  Fuel Shutoff Valve .... ON
[ ]  Radios & Electrical Equipment .... OFF
[ ]  Brakes .... TEST & SET

STARTING ENGINE
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... COLD
[ ]  Master Switch .... ON
[ ]  Prime .... AS REQUIRED
[ ]  Throttle .... OPEN 1/4 INCH
[ ]  Propeller Area .... CLEAR
[ ]  Ignition Switch .... START
Release when engine starts.
[ ]  Oil Pressure .... CHECK

BEFORE TAKEOFF
[ ]  Cabin Doors .... LATCHED
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Elevator Trim .... TAKEOFF POSITION
[ ]  Fuel Shutoff Valve .... ON
[ ]  Brakes .... SET
[ ]  Throttle .... 1700 RPM
[ ]  Magnetos .... CHECK
[ ]  Carburetor Heat .... CHECK FOR RPM DROP
[ ]  Engine Instruments and Ammeter .... CHECK
[ ]  Suction Gauge .... CHECK
[ ]  Flight Instruments and Radio .... SET
[ ]  Throttle Friction Lock .... ADJUST
[ ]  Wing Flaps .... AS REQUIRED

TAKEOFF
NORMAL TAKEOFF
[ ]  Wing Flaps .... UP (0)
[ ]  Carburetor Heat .... COLD
[ ]  Throttle .... FULL OPEN
[ ]  Elevator Control .... LIFT NOSE WHEEL
[ ]  Climb Speed .... 70-80 MPH
MAXIMUM PERFORMANCE TAKEOFF
[ ]  Wing Flaps .... UP (0)
[ ]  Carburetor Heat .... COLD
[ ]  Brakes .... HOLD
[ ]  Throttle .... FULL OPEN
[ ]  Brakes .... RELEASE
[ ]  Elevator Control .... SLIGHTLY TAIL LOW
[ ]  Climb Speed .... 70 MPH (with obstacles ahead)

ENROUTE CLIMB
[ ]  Airspeed .... 75 - 85 MPH
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... RICH
Unless engine is rough.

CRUISE
[ ]  Power .... 2000 to 2750
No more than 75%.
[ ]  Elevator Trim .... ADJUST
[ ]  Mixture .... LEAN

BEFORE LANDING
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON
Apply before closing throttle.
[ ]  Airspeed .... 70-80 MPH (flaps up)
[ ]  Wing Flaps .... AS DESIRED
[ ]  Airspeed .... 60-70 MPH (flaps down)

BALKED LANDING
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... COLD
[ ]  Wing Flaps .... RETRACT TO 20
[ ]  Airspeed .... 65 MPH
[ ]  Wing Flaps .... RETRACT
Slowly.

NORMAL LANDING
[ ]  Touchdown .... MAIN WHEELS FIRST
[ ]  Landing Roll .... LOWER NOSE WHEEL GENTLY
[ ]  Braking .... MINIMUM REQUIRED

AFTER LANDING
[ ]  Wing Flaps .... UP
[ ]  Carburetor Heat .... COLD
[ ]  Unnecessary Equipment .... OFF

SECURING AIRCRAFT
[ ]  Parking Brake .... SET
[ ]  Radios, Electrical Equipment .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
[ ]  Tach/Hobbs Meter .... RECORD

C150G/C150L Airspeeds (MCAS)
[ ]  Vr .... 55
[ ]  Vx .... 70
[ ]  Vy .... 78
[ ]  Va .... 109
[ ]  Vs1 .... 55
[ ]  Vso .... 48
[ ]  Vfe .... 100
[ ]  Vno .... 120
[ ]  Vne .... 162
[ ]  Glide .... 70
[ ]  XW demo .... 15
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