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Airspeed Limitations
AIRSPEED LIMITATIONS
[ ]  VNE — Never Exceed Speed. Do not exceed this speed in any operation .... 141 KT / 162 MPH
[ ]  VNO — Maximum structural cruising speed. Do not exceed this speed except in smooth air and then only with caution .... 107 KT / 123 MPH
[ ]  VA — Maneuvering speed, 1,600 Pounds .... 97 KT / 111 MPH
[ ]  VA — Maneuvering speed, 1,450 Pounds .... 93 KT / 107 MPH
[ ]  VA — Maneuvering speed, 1,300 Pounds .... 88 KT / 101 MPH
[ ]  VFE — Maximum flap extended speed .... 85 KT / 97 MPH
[ ]  Maximum window open speed .... 141 KT / 162 MPH
[ ]  VS — Stall speed .... 47 KT / 54 MPH
[ ]  VS1 — Stall speed (10° Flaps) .... 45 KT / 52 MPH
[ ]  VS0 — Stall speed in landing configuration .... 42 KT / 49 MPH
[ ]  Demonstrated crosswind capability .... 13 KT / 15 MPH

Optimum/Recommended Speeds
OPTIMUM/RECOMMENDED SPEEDS
[ ]  VX — Best angle of climb .... 56 KT / 64 MPH
[ ]  VY — Best rate of climb .... 68 KT / 78 MPH
[ ]  VR — Normal rotation speed .... 50 KT / 58 MPH
[ ]  Normal climb speed .... 65–75 KT / 75–85 MPH
[ ]  Normal landing (no flaps) .... 60–70 KT / 70–80 MPH
[ ]  Normal landing (full flaps) .... 50–60 KT / 57–69 MPH
[ ]  Powered landing (no flaps) .... 65 KT / 75 MPH
[ ]  Powered landing (full flaps) .... 55 KT / 63 MPH
[ ]  Maximum performance approach .... 52 KT / 60 MPH
[ ]  Optimum glide speed .... 60 KT / 69 MPH

Maneuvering Limits
MANEUVERING LIMITS
[ ]  Chandelles maximum airspeed .... 95 KT / 109 MPH
[ ]  Lazy Eights maximum airspeed .... 95 KT / 109 MPH
[ ]  Steep Turns maximum airspeed .... 95 KT / 109 MPH
[ ]  Spins .... Use slow deceleration
[ ]  Stalls (except whip stalls) .... Use slow deceleration

Stall Speed Table (Max Gross/CG Forward)
STALL SPEED TABLE (MAX GROSS/CG FORWARD)
[ ]  0° Angle of Bank, 0° Flaps .... 47 KIAS / 54 MPH
[ ]  30° Angle of Bank, 0° Flaps .... 51 KIAS / 59 MPH
[ ]  45° Angle of Bank, 0° Flaps .... 56 KIAS / 64 MPH
[ ]  60° Angle of Bank, 0° Flaps .... 66 KIAS / 76 MPH
[ ]  0° Angle of Bank, 40° Flaps .... 42 KIAS / 48 MPH
[ ]  30° Angle of Bank, 40° Flaps .... 45 KIAS / 52 MPH
[ ]  45° Angle of Bank, 40° Flaps .... 50 KIAS / 58 MPH
[ ]  60° Angle of Bank, 40° Flaps .... 59 KIAS / 68 MPH

Engine Failure During Takeoff Run  [EMERGENCY]
[ ]  Throttle .... Idle
[ ]  Brakes .... Apply
[ ]  Flaps .... Retract
[ ]  Mixture .... Idle Cutoff
[ ]  Ignition Switch .... Off
[ ]  Master Switch .... Off

Engine Failure Immediately After Takeoff  [EMERGENCY]
1. IF ENOUGH RUNWAY REMAINING TO LAND
[ ]  Throttle .... Idle
[ ]  Land .... Straight ahead
[ ]  Brakes .... Apply
[ ]  Flaps .... Up
[ ]  Mixture .... Idle cutoff
[ ]  Ignition Switch .... Off
[ ]  Master Switch .... Off
2. NOT ENOUGH RUNWAY TO LAND
[ ]  Airspeed .... 60 KIAS (69 MPH)
[ ]  Fly runway heading to emergency landing site .... Fly
[ ]  Mixture .... Idle cutoff
[ ]  Fuel shutoff .... Off
[ ]  Ignition switch .... Off
[ ]  Flaps .... As required
[ ]  Master switch .... Off
[ ]  Doors .... Ajar

Engine Failure In Flight  [EMERGENCY]
[ ]  1. Gain all the altitude you can — pull back (gently) to use the aircraft’s momentum until airspeed falls to optimum glide speed .... Pull back
[ ]  3. Airspeed .... Optimum glide speed 60 KIAS (69 MPH)
[ ]  Trim .... For optimum glide speed
[ ]  4. Find a suitable place to land and fly to it .... Fly
NOTE: If altitude and distance permit, set up a normal landing pattern. If not possible, take what you can get. Make sure the approach results in a landing parallel to any furrows in the selected field.
5. IF TIME PERMITS, TRY TO CORRECT THE PROBLEM
[ ]  Fuel shut-off .... On
[ ]  Mixture .... Rich (in)
[ ]  Throttle .... 1/4 Inch
[ ]  Carburetor Heat .... On (out)
[ ]  Primer .... In and Locked
[ ]  Master Switch .... On (Both sides)
[ ]  Ignition switch .... Both magnetos
[ ]  Start .... If propeller is stopped
6. IF STILL HAVE TIME COMMUNICATE
[ ]  Transponder .... 7700
[ ]  Comm Radio .... 121.5

Emergency Landing Without Engine Power  [EMERGENCY]
[ ]  1. Fly the airplane — Airspeed .... 65 KIAS / 75 MPH (flaps up); 55 KIAS / 64 MPH (flaps down)
7. PREPARE AIRCRAFT FOR LANDING
[ ]  Mixture .... Idle cutoff
[ ]  Fuel Shutoff .... Off
[ ]  Ignition Switch .... Off
[ ]  Flaps .... As required (40° recommended)
[ ]  Master Switch .... Off
[ ]  Doors .... Unlatch prior to touchdown
8. LANDING
[ ]  Touchdown .... Slightly tail low
[ ]  Brakes .... Apply heavily

Precautionary Landing With Engine Power  [EMERGENCY]
[ ]  1. Fly the airplane — Airspeed .... 60 KIAS (69 MPH)
[ ]  Flaps .... 20°
[ ]  Selected Field .... Inspect
NOTE: Fly over field noting terrain and obstructions then retract flaps upon reaching a safe altitude and airspeed.
9. PREPARE AIRPLANE FOR LANDING
[ ]  Radios and Electrical .... Off
[ ]  Flaps .... 40° (On final approach)
[ ]  Airspeed .... 55 KIAS (64 MPH) on final
[ ]  Master Switch .... Off
[ ]  Doors .... Unlatch prior to touchdown
10. LANDING
[ ]  Touchdown .... Tail slightly low
[ ]  Ignition Switch .... Off
[ ]  Brakes .... Apply heavily

Ditching  [EMERGENCY]
1. PREPARE FOR DITCHING
[ ]  Radio .... Transmit MAYDAY on 121.5
NOTE: Give location, situation and intentions. If already communicating with ATC, report situation to controller rather than using 121.5.
[ ]  Transponder .... 7700
[ ]  Heavy Baggage .... Secure or jettison
11. FLY THE AIRPLANE
[ ]  Approach with high wind / heavy seas .... Into the wind
[ ]  Approach with light winds / heavy swells .... Parallel to the swells
[ ]  Flaps .... 40°
[ ]  Power .... 300 ft./min. descent, 55 KIAS (64 MPH)
[ ]  Cabin Doors .... Unlatch prior to touchdown
12. LANDING
[ ]  Touchdown .... Level attitude at 300 ft./min. descent
[ ]  Face .... Cushion with folded coat
[ ]  Evacuate .... Through doors
NOTE: If necessary, open windows to allow cabin to flood to equalize pressure so doors can be opened.
[ ]  Life Vests and Raft .... Inflate

Engine Fire During Start Up  [EMERGENCY]
[ ]  Cranking .... Continue
NOTE: Getting the engine to start will suck flames and accumulated fuel into the engine.
IF ENGINE STARTS
[ ]  Power .... 1,700 RPM for a few minutes
[ ]  Engine .... Shutdown and inspect for damage
IF ENGINE FAILS TO START
[ ]  Continue cranking .... For 2 to 3 minutes
[ ]  Obtain fire extinguisher .... Obtain
[ ]  Master Switch .... Off
[ ]  Ignition Switch .... Off
[ ]  Fuel Shutoff .... Off
[ ]  Extinguish fire .... With extinguisher, seat cushion, blanket, etc. or dirt
[ ]  Try to remove air filter if it is on fire .... Remove
[ ]  Inspect for damage and have repairs made before attempting another flight .... Inspect

Engine Fire In Flight  [EMERGENCY]
[ ]  Mixture .... Idle cutoff
[ ]  Fuel Shutoff .... Off
[ ]  Master Switch .... Off
[ ]  Cabin Heat and Air .... Off (except overhead vents)
[ ]  Airspeed .... 85 KIAS (98 MPH)
NOTE: If that does not extinguish the fire increase airspeed to that which produces an incombustible mixture. Be aware of critical speeds; VNO (107 KIAS/123 MPH) and VNE (141 KIAS/162 MPH).
[ ]  Landing .... Forced Landing Without Power

Electrical Fire In Flight  [EMERGENCY]
1. EXTINGUISH FIRE
[ ]  Master Switch .... Off
[ ]  All other Switches .... Off
[ ]  Ignition .... On
[ ]  Vents, Cabin Heat/Air .... Closed
[ ]  Fire Extinguisher .... Activate
13. IF FIRE APPEARS TO BE OUT AND ELECTRICAL EQUIPMENT IS NEEDED
[ ]  Master Switch .... On
[ ]  Circuit Breakers .... Check for faulty circuit — do not reset
[ ]  Radio/Electrical .... On one at a time, with delay between until short circuit is localized
[ ]  Vents, Cabin Heat/Air .... Open once it is ascertained that the fire is completely extinguished

Cabin Fire  [EMERGENCY]
[ ]  Master Switch .... Off
[ ]  Vents, Cabin Heat/Air .... Closed
[ ]  Fire Extinguisher .... Activate
NOTE: After using fire extinguisher within a closed cabin ventilate the cabin.
[ ]  Landing .... As soon as possible

Wing Fire  [EMERGENCY]
[ ]  Navigation lights .... Off
[ ]  Strobe Lights .... Off
[ ]  Pitot Heat .... Off
[ ]  Attitude .... Perform side-slip to keep the flames away from the fuel tank and cabin
[ ]  Land .... ASAP. Do not use flaps

Pre-Flight Inspection Checklist
1. WING TOPS/FUEL TANKS
[ ]  Fuel Level .... Both Wings — Visual check
NOTE: If needed get gas (AVGAS 100) before proceeding with other fuel tank related items.
[ ]  Filler caps .... Both Wings — Secure
NOTE: Make sure vent on right wing cap is not blocked.
[ ]  Wing Tops .... Inspect for loose screws, rivets and damage
14. COCKPIT
[ ]  Control wheel lock .... Remove
[ ]  Ignition switch .... Off
[ ]  Master switch .... On (both sides)
[ ]  Fuel gauges .... Check quantity
[ ]  Flaps .... 10°
[ ]  Pitot Heat .... On — observe Ammeter drop — then off
[ ]  Strobe/Beacon .... On — visually check — off
[ ]  Master Switch .... Off
[ ]  Fuel shut-off valve .... On
PAPERWORK
[ ]  Airworthiness certificate
[ ]  Registration
[ ]  Radio station license
[ ]  Operating limitations (POH)
[ ]  Weight/loading data
15. COCKPIT — NIGHT FLIGHTS
[ ]  Nav Lights & Strobes .... On
NOTE: Walk around plane and visually check to see that all are operating.
[ ]  Landing Light .... On
NOTE: Visually check from outside if not dark enough to see that it’s on from inside the cockpit.
[ ]  Instrument Lights .... On
[ ]  Fuses .... 3 Spares of each type required
16. FUSELAGE — LEFT SIDE
[ ]  Radio antennas .... Check security
[ ]  Miscellaneous .... Check for loose screws/rivets, etc.
17. EMPENNAGE
[ ]  Rudder gust lock .... Remove
[ ]  Tail tie-down .... Disconnect
[ ]  Control surfaces .... Check freedom of movement, actuators, security, loose rivets, damage
18. FUSELAGE RIGHT SIDE
[ ]  Miscellaneous .... Check for loose screws/rivets, etc.
[ ]  Fuel strainer drain (belly) .... Check sample for water/dirt (some models)
19. RIGHT WING
[ ]  Flaps .... Check actuator and rollers
[ ]  Aileron .... Check freedom, hinge pins and counterweights
[ ]  Wing tip .... Check for cracks
[ ]  Check navigation light
[ ]  Leading edge .... Check for dents, cracks, etc.
[ ]  Wing tie-down .... Disconnect
[ ]  Main wheel tire .... Check for proper inflation/wear
[ ]  Check cotter pin in wheel nut
[ ]  Main wheel brake .... Check for fluid leaks
[ ]  Check brake pads
[ ]  Fuel drain .... Check sample for water/dirt and fuel type (100LL — Blue)
20. NOSE
[ ]  Engine Oil .... Check level
NOTE: Minimum 4 qts.; 5 qts. for short flights; 6 qts. extended flights
[ ]  Fuel bowl drain .... Check sample for water/dirt and fuel type (100LL — Blue)
[ ]  Prop/Spinner .... Check for nicks and security
[ ]  Air filter .... Check for restrictions & excessive dirt
[ ]  Landing Light .... Check condition and cleanliness
[ ]  Cowling .... Look for birds or nests inside
[ ]  Nose wheel .... Check for proper inflation/wear; Check for cotter pins in wheel nuts; Check for leaking fluids
[ ]  Nose tie-down .... Disconnect
[ ]  Static source opening .... Check not blocked
21. LEFT WING
[ ]  Wing tie-down .... Disconnect
[ ]  Leading edge .... Check for dents, cracks, etc.
[ ]  Pitot tube .... Remove cover, check for blockage
[ ]  Stall warning opening .... Check for blockage
[ ]  Fuel Tank Vent .... Check for blockage
[ ]  Wing tip .... Check for cracks
[ ]  Check navigation light
[ ]  Aileron .... Check freedom, hinge pins and counterweights
[ ]  Flaps .... Check actuator and rollers
[ ]  Fuel drain .... Check sample for water/dirt and fuel type (100LL — Blue)
[ ]  Main wheel tire .... Check for proper inflation/wear
[ ]  Check cotter pin in wheel nut
[ ]  Main wheel brake .... Check for fluid leaks
[ ]  Check brake pads

Normal Engine Starting Checklist
1. BEFORE STARTING
[ ]  Preflight Inspection .... Completed
[ ]  Seat position .... Adjust & ensure locked
[ ]  Seat belts/harness .... Adjust and lock
NOTE: Brief passengers on use of belts/harnesses and requirements for wearing them.
[ ]  Fuel shut-off .... On
[ ]  Radios/electrical .... Off
[ ]  Brakes .... Test and set
[ ]  Circuit Breakers .... Check all in
22. STARTING ENGINE
[ ]  Mixture .... Rich (in)
[ ]  Carburetor heat .... Cold (in)
[ ]  Primer .... Prime if required
NOTE: Make sure locked in.
[ ]  Throttle .... 1/4 Inch
[ ]  Key .... In ignition
[ ]  Master Switch .... On (both sides)
[ ]  Propeller Area .... Call “Clear” & check prop area and behind plane
[ ]  Ignition .... Start — release on start
[ ]  Throttle .... 1,000 RPM
[ ]  Oil Pressure .... Check in green
23. BEFORE TAXIING
[ ]  Radios .... On and set to appropriate frequency. Call for radio check
[ ]  Transponder .... Standby
[ ]  Beacon/Strobe .... On
[ ]  Nav. Lights/Strobes .... On if required
[ ]  Flaps .... Full up (normal takeoff)
24. TAXIING
[ ]  Clearance .... Check for things in way of wings
[ ]  Check for people ahead of and behind plane
[ ]  Flight Controls .... Set for existing wind conditions
[ ]  Brakes .... Come to full stop immediately after starting taxi roll
25. IFR INSTRUMENT CHECKS
[ ]  Turn Coordinator .... Should indicate turn in proper direction while taxiing
[ ]  Attitude Indicator .... Very little change due to turns; slight pitch indications due to acceleration or deceleration
[ ]  Heading Indicator .... Should track headings
[ ]  Altimeter .... When set to current altimeter setting should indicate within 75 ft. of airport elevation
[ ]  VSI .... Should indicate zero. If not, note indication and use for level indication in flight
[ ]  VORs .... Check at local ground check point or against each other based on some receivable signal

Cold Weather Starting Without Pre-Heat
1. BEFORE STARTING
[ ]  Preflight Inspection .... Completed
[ ]  Seat position .... Adjust & ensure locked
[ ]  Seat belts/harness .... Adjust and lock
NOTE: Brief passengers on use of belts/harnesses and requirements for wearing them.
[ ]  Fuel shut-off .... On
[ ]  Radios/electrical .... Off
[ ]  Brakes .... Test and set
[ ]  Circuit Breakers .... Check all in
26. STARTING ENGINE
[ ]  Ignition .... Off (take key out and hang it up)
[ ]  Master Switch .... Off (both sides)
[ ]  Prime .... With ignition switch off and throttle closed, prime four to ten strokes as propeller is turned by hand
NOTE: Use heavy primer strokes for best atomization of fuel. If doing this by yourself, tie the plane down securely and set parking brake. Treat propeller as if the ignition is on and engine could start. Leave primer charged and ready for a stroke.
[ ]  Propeller Area .... Clear
[ ]  Master Switch .... On
[ ]  Mixture .... Full Rich
[ ]  Throttle .... Open 1/4 inch
[ ]  Ignition Switch .... Start
[ ]  Throttle .... Pump to full open twice then return to 1/4 inch open position
[ ]  Primer .... Continue to prime until engine is running smoothly. Alternately pump throttle rapidly over first 1/4 of travel
[ ]  Oil Pressure .... In the green
NOTE: This might take a little time since the engine is cold. If pressure doesn’t come up in about 30 seconds, shut the engine down.
[ ]  Carburetor Heat .... Full on after engine started. Leave on until running smoothly
[ ]  Primer .... In and locked
CAUTION: If engine does not start during the first few attempts, or if engine firing diminishes in strength, it is probable that the spark plugs have frosted over. Pre-heat must be used before another start is attempted.
CAUTION: Pumping the throttle may cause raw fuel to accumulate in the intake air duct, creating a fire hazard in the event of a back-fire. If this occurs, maintain a cranking action to suck flames into the engine. An outside attendant with a fire extinguisher is advised for cold starts without pre-heat.
GO TO: Perform steps 3 through 5 on normal start checklist

Cold Weather Starting With Pre-Heat
1. BEFORE STARTING
[ ]  Preflight Inspection .... Completed
[ ]  Seat position .... Adjust & ensure locked
[ ]  Seat belts/harness .... Adjust and lock
NOTE: Brief passengers on use of belts/harnesses and requirements for wearing them.
[ ]  Fuel shut-off .... On
[ ]  Radios/electrical .... Off
[ ]  Brakes .... Test and set
[ ]  Circuit Breakers .... Check all in
28. STARTING ENGINE
[ ]  Ignition .... Off (take key out and hang it up)
[ ]  Master Switch .... Off (both sides)
[ ]  Prime .... With ignition switch off and throttle closed, prime four to ten strokes as propeller is turned by hand
NOTE: Use heavy primer strokes for best atomization of fuel.
[ ]  Primer .... In and locked
[ ]  Propeller Area .... Clear
[ ]  Master Switch .... On
[ ]  Mixture .... Full Rich
[ ]  Throttle .... Open 1/4 inch
[ ]  Ignition Switch .... Start — to Both when engine starts
[ ]  Oil Pressure .... In the green
NOTE: This might take a little time since the engine is cold. If pressure doesn’t come up in about 30 seconds, shut the engine down.
GO TO: Perform steps 3 through 5 on normal start checklist

Before Takeoff Checklist
1. FINAL COCKPIT CHECK
[ ]  Cabin doors .... Closed and latched
[ ]  Windows .... Closed
[ ]  Flight Controls .... Free and correct
[ ]  Elevator trim .... Takeoff position
[ ]  Flight Instruments .... Check and set
NOTE: Set attitude indicator to level flight position. Set altimeter to runway altitude or locally reported altimeter setting. Set heading indicator to magnetic compass.
[ ]  Comm Radio/VOR .... Set to appropriate freqs
[ ]  Beacon/Strobe .... On
[ ]  Nav Lights/Strobes .... On if required
29. ENGINE RUN-UP
[ ]  Fuel Shutoff .... On
[ ]  Mixture .... Rich (in)
[ ]  Parking brake .... Set or hold foot brakes
[ ]  Throttle .... 1,700 RPM
[ ]  Magnetos .... Check
NOTE: RPM drop should not exceed 150 RPM on either magneto. RPM difference between magnetos should not exceed 75 RPM.
[ ]  Carburetor Heat .... On
NOTE: Check for RPM drop then back to off.
[ ]  Engine instruments .... Oil pressure/temperature, suction, ammeter
NOTE: Create electrical load with landing light. Make sure no more than needle width deflection.
[ ]  Vacuum .... Check in green
[ ]  Throttle .... Idle
[ ]  Carburetor heat .... On — Make sure engine keeps running
[ ]  Throttle .... 1,000 RPM
[ ]  Throttle friction lock .... Adjust
[ ]  Alternator switch .... Off — Check low voltage light on — Switch back to on
[ ]  Flaps .... Appropriate takeoff position
[ ]  Transponder .... Set to mode C/Altitude

Normal Takeoff and Climb Procedures
[ ]  Flaps .... Full up
[ ]  Carburetor Heat .... Cold (in)
[ ]  Elevator Trim .... Takeoff position
[ ]  Heading indicator .... Calibrate against compass
[ ]  Throttle .... Full open (in)
NOTE: Engine Instruments: Check while starting roll — RPM 2600 (top of green arc); oil pressure in green; oil temperature in green; suction in green.
[ ]  Airspeed .... Building
[ ]  Elevator .... Lift nose wheel at 50 KIAS (58 MPH)
[ ]  Climb Speed .... 60–70 KIAS (69–80 MPH)

Maximum Performance Takeoff (Short Field)
[ ]  Taxi .... Maximum runway usage
NOTE: Takeoff procedure should be started using ALL available runway. Taxi to end of runway and align with centerline.
[ ]  Brakes .... Set and hold
[ ]  Flaps .... Full up
[ ]  Carburetor Heat .... Cold (in)
[ ]  Elevator Trim .... Takeoff position
[ ]  Heading indicator .... Calibrate against compass
[ ]  Throttle .... Full open (in)
NOTE: Engine Instruments: Check before starting roll — RPM 2600 (top of green arc); oil pressure in green; oil temperature in green; suction in green.
[ ]  Brakes .... Release
[ ]  Airspeed .... Building
[ ]  Elevator .... Slightly tail low
[ ]  Climb Speed .... 60 KIAS (69 MPH) with obstacles ahead

Soft Field Takeoff
[ ]  Taxi .... Keep rolling to avoid bogging down
[ ]  Flaps .... 10°
NOTE: If 10° flaps are used, with obstacles ahead, leave them extended until the obstacle is cleared and at a safe altitude. The exception is high density altitude takeoff where the climb would be marginal with flaps at 10°.
[ ]  Carburetor Heat .... Cold (in)
[ ]  Elevator Trim .... Takeoff position
[ ]  Heading indicator .... Calibrate against compass or runway heading
[ ]  Throttle .... Full open (in)
NOTE: Engine Instruments: Check as starting roll — RPM 2600 (top of green arc); oil pressure in green; oil temperature in green; suction in green.
[ ]  Airspeed .... Building
[ ]  Elevator .... Slightly tail low
NOTE: Allow the airplane to lift off as soon as possible (before reaching safe climb speed). Level off at a few feet above the ground and fly in ground effect until reaching normal climb speed.
[ ]  Climb Speed .... 60 KIAS (69 MPH) with obstacles ahead
[ ]  Flaps .... Retract at safe altitude with positive rate of climb

After Takeoff Checklist
1. CLIMBOUT
[ ]  Airspeed .... 70 Knots (80 MPH)
[ ]  Altitude .... Above 300 AGL
[ ]  Flaps .... Up (in 10° increments if more than that in use)
30. AT CRUISE ALTITUDE
[ ]  Attitude .... Level
[ ]  Airspeed .... Let build to desired cruise speed
[ ]  Throttle .... Reduce to desired cruise setting
[ ]  Heading Indicator .... Calibrate against compass
31. ABOVE 5,000 MSL
[ ]  Mixture .... Lean per POH instructions

Enroute Climb
[ ]  Normal Airspeed .... 65–75 KIAS (75–86 MPH)
[ ]  Max Performance .... See POH Climb Table in Section 5
[ ]  Throttle .... Full Open (in)
[ ]  Carburetor Heat .... Cold (in)
[ ]  Mixture .... Rich (in) below 5,000 ft. May be leaned above 5,000

Normal Approach and Landing Procedures
1. PRE-LANDING (DOWNWIND) CHECK
[ ]  Seat belts/Harnesses .... Adjust and lock
[ ]  Mixture .... Rich (In)
[ ]  Carburetor heat .... On (Out)
[ ]  Fuel Shut-off .... On
32. APPROACH AND LANDING
[ ]  Power .... Reduce to 1,500 to 1,700 RPM abeam approach end of runway
[ ]  Airspeed .... Let bleed off to less than 85 KIAS (95 MPH)
NOTE: Flaps as desired: under light (less than 10 Knots) wind conditions 10° descending on the end of the downwind leg, 20° on base, and full flaps over the threshold. In heavier winds 20° or less is good flap setting. Use minimum flap setting possible for crosswind landing.
[ ]  Airspeed — Downwind through base .... 65–70 KIAS (75–80 MPH)
[ ]  Airspeed — Final approach .... 60–65 KIAS (70–75 MPH)
NOTE: In gusty winds add 1/2 difference between gust and average wind speed to approach speed.
[ ]  Touchdown .... Just above stalling speed — main wheels first
[ ]  Landing Roll .... Lower nose wheel gently
[ ]  Braking .... Minimum required

Short Field Landing
1. PRE-LANDING (DOWNWIND) CHECK
[ ]  Seat belts/Harnesses .... Adjust and lock
[ ]  Mixture .... Rich (In)
[ ]  Carburetor heat .... On (Out)
[ ]  Fuel Shut-off .... On
33. APPROACH AND LANDING
[ ]  Power .... Reduce to 1,500 to 1,700 RPM abeam approach end of runway
[ ]  Airspeed .... Let bleed off to less than 85 KIAS (95 MPH)
NOTE: Flaps: under light (less than 10 Knots) wind conditions 10° descending on the end of the downwind leg, 20° on base, and full flaps on final.
[ ]  Airspeed — Downwind through base .... 65–70 KIAS (75–80 MPH)
[ ]  Airspeed — Final approach .... 52 KIAS (60 MPH)
NOTE: In gusty winds add 1/2 difference between gust and average wind speed to approach speed.
[ ]  Touchdown .... Just above stalling speed — power off — main wheels first. Roundout must be done much faster than usual due to low airspeed
[ ]  Landing Roll .... Lower nose wheel quickly
[ ]  Braking .... Maximum possible without sliding tires
[ ]  Flight Controls .... Flaps up. Hold full nose up elevator

Soft Field Landing
1. PRE-LANDING (DOWNWIND) CHECK
[ ]  Seat belts/Harnesses .... Adjust and lock
[ ]  Mixture .... Rich (In)
[ ]  Carburetor heat .... On (Out)
[ ]  Fuel Shut-off .... On
34. APPROACH AND LANDING
[ ]  Power .... Reduce to 1,500 to 1,700 RPM abeam approach end of runway
[ ]  Airspeed .... Let bleed off to less than 85 KIAS (95 MPH)
NOTE: Flaps: under light (less than 10 Knots) wind conditions 10° descending on the end of the downwind leg, 20° on base, and full flaps over the threshold. In heavier winds 20° or less is good flap setting. Use minimum flap setting possible for crosswind landing.
[ ]  Airspeed — Downwind through base .... 65–70 KIAS (75–80 MPH)
[ ]  Airspeed — Final approach .... 60–65 KIAS (70–75 MPH)
NOTE: In gusty winds add 1/2 difference between gust and average wind speed to approach speed.
[ ]  Touchdown .... Just above stalling speed — power off — main wheels first
[ ]  Landing Roll .... Hold nose wheel off as long as possible. Use up elevator to reduce weight on nose wheel throughout landing roll
[ ]  Braking .... As required
[ ]  Flight Controls .... Full up elevator

Balked Landing (Go Around)
[ ]  Throttle .... Full Open (in)
[ ]  Carburetor Heat .... Cold (in)
[ ]  Flaps .... To 20°
NOTE: If more than 20° of flaps were in when the go-around is initiated, retract immediately to 20°. Continue to retract flaps in 10° increments only after establishing a positive rate of climb and reaching a safe altitude.
[ ]  Airspeed .... 55 KIAS (63 MPH)

Post-Landing Checklists
1. AFTER LANDING — CLEAR OF RUNWAY
[ ]  Flaps .... Full up (visual check)
[ ]  Carburetor Heat .... Off (in)
[ ]  Elevator Trim .... Takeoff position
35. IF HARD LANDING
[ ]  ELT .... Listen for on 121.5 on communications radio
36. ENGINE SHUTDOWN
[ ]  Radios/Electrical .... All off
[ ]  Throttle .... 1,000 RPM
[ ]  Mixture .... Idle cutoff
[ ]  Ignition .... Off
[ ]  Master Switch .... Off
37. SECURING THE AIRPLANE
[ ]  Parking Brake .... Set
[ ]  Control Lock .... Install
[ ]  Tiedown .... Wings and Tail
[ ]  Pitot Cover .... Install
DOUBLE CHECK
[ ]  All electrical equipment .... Off
[ ]  Master Switch .... Off
38. CLOSE YOUR FLIGHT PLAN
[ ]  Close your Flight Plan .... Close

Before Leaving Home
1. SELF CHECK
[ ]  Feeling ok .... Yes
[ ]  Under any stress .... No more than usual
[ ]  Taking any medication .... No
[ ]  Alcohol in last 12 Hrs. .... No
39. FLIGHT PLANNING/NAVIGATION EQUIPMENT
[ ]  Current Charts
[ ]  A/FD
[ ]  POH
[ ]  Airport Guide
[ ]  E6-B
[ ]  Plotter
[ ]  Calculator
[ ]  Timer
[ ]  Custom Checklists
[ ]  Flight Plans
[ ]  Weather Reports
[ ]  Pencils
[ ]  Clipboards
40. EMERGENCY ITEMS
[ ]  Hand Compass
[ ]  Knife
[ ]  Flashlights
[ ]  Batteries
[ ]  Bulbs
[ ]  Cell Phone (Charged)
[ ]  Spare Glasses
[ ]  Sun Glasses

NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
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