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Before Starting Engine
[ ]  Preflight .... COMPLETE
[ ]  Seats, Belts .... ADJUST and LOCK
[ ]  Fuel Shutoff Valve .... ON
[ ]  Radios, Elec. Equip. .... OFF
[ ]  Brakes .... TEST and SET
[ ]  Fuses .... CHECK

Starting Engine
[ ]  Mixture .... RICH
[ ]  Carb. Heat .... COLD
[ ]  Prime .... 4 SHOTS
[ ]  Throttle .... ¼ Inch Open
[ ]  Propeller Area .... CLEAR
[ ]  Master Switch .... ON
[ ]  Magnetos .... BOTH
[ ]  Starter Handle .... PULL
[ ]  Throttle .... 1,000RPM
[ ]  Oil Pressure .... CHECK

Before Takeoff
[ ]  Parking Brake .... SET
[ ]  Cabin Doors .... CLOSED and LATCHED
[ ]  Flight Controls .... FREE and CORRECT
[ ]  Flight Instruments .... SET
[ ]  Fuel Shutoff Valve .... ON
[ ]  Mixture .... RICH
[ ]  Elevator Trim .... SET FOR TAKEOFF
[ ]  Throttle .... 1700RPM
[ ]  Magnetos .... CHECK (less than 125PRM)
[ ]  Carb. Heat .... Check (for RPM drop)
[ ]  Engine Instruments .... CHECK
[ ]  Generator Light .... OFF
[ ]  Suction Gauge .... CHECK
[ ]  Radios .... SET
[ ]  Flashing Bcn, Nav. Lights .... ON (as req’d)
[ ]  Throttle Friction Lock .... ADJUST
[ ]  Brakes .... RELEASE

Takeoff
NORMAL TAKEOFF
[ ]  Wing Flaps .... 0-10 DEGREES
[ ]  Carb. Heat .... COLD
[ ]  Throttle .... FULL OPEN
[ ]  Elevator .... LIFT NOSE at 50MPH
[ ]  Climb Speed .... 70MPH

Short-Field Takeoff
[ ]  Wing Flaps .... 10 DEGREES
[ ]  Carb. Heat .... COLD
[ ]  Brakes .... APPLY
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... RICH
[ ]  Brakes .... RELEASE
[ ]  Elevator .... SLIGHTLY TAIL LOW
[ ]  Climb Speed .... 70MPH (until Clear of obstacles)
[ ]  Wing Flaps .... RETRACT (slowly, in increments)

Enroute Climb
[ ]  Airspeed .... 70-75MPH
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... RICH (below 3000ft)

Cruise
[ ]  Power .... 1900-2550PRM (no more than 75%)
[ ]  Elevator Trim .... ADJUST
[ ]  Mixture .... LEAN (above 3000ft)

Before Landing
[ ]  Seats, Belts .... ADJUST and LOCK
[ ]  Carb. Heat .... ON

Landing
NORMAL LANDING
[ ]  Airspeed .... 70-75MPH
[ ]  Wing Flaps .... AS DESIRED (under 80MPH)
[ ]  Pitch .... for 70MPH (on final)

Short-Field Landing
[ ]  Airspeed .... 70-75MPH
[ ]  Wing Flaps .... 30 Degrees (under 80MPH)
[ ]  Airspeed .... 65MPH
[ ]  Power .... REDUCE to idle

Balked Landing
[ ]  Throttle .... FULL OPEN
[ ]  Carb. Heat .... COLD
[ ]  Wing Flaps .... RETRACT to 20 Degrees
[ ]  Airspeed .... 70MPH
[ ]  Wing Flaps .... RETRACT (slowly)

After Landing
[ ]  Wing Flaps .... UP
[ ]  Carb. Heat .... COLD

Securing Airplane
[ ]  Radios, Elec. Equip. .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magneto Switch .... OFF (key out)
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
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