Cessna 152 — c152_a152_checklist_moorabbin
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

PRE START
[ ]  Loose items stowed
[ ]  Seat adjusted
[ ]  Hatches and harnesses secure
[ ]  Fuel on
[ ]  Elevator Trim through range set to t/o
[ ]  Mixture idle cut off
[ ]  Throttle closed
[ ]  Carburetor Heat off
[ ]  Switches off
[ ]  Park Brake on
[ ]  Instruments checked and set
[ ]  Avionics off
[ ]  Master on
[ ]  Circuit breakers in
[ ]  Controls full and free, correct sense

START CHECKS
[ ]  Mixture rich
[ ]  Throttle 1 cm open
[ ]  Fuel pump on, check press & off
[ ]  Prime as required
[ ]  Check “Clear Prop”
[ ]  Magnetos start

AFTER START
[ ]  Throttle set 1000 rpm
[ ]  Oil pressure green within 30 secs
[ ]  Ammeter positive charge
[ ]  Suction within limits
[ ]  Gyro instruments erection and sync
[ ]  Annunciators test & out
[ ]  Avionics on
[ ]  Beacon on

TAXI CHECKS
[ ]  Brakes checked
[ ]  Instruments turning checks

RUN-UP CHECKS
[ ]  Park brake on
[ ]  Oil temp & pressure green arc
[ ]  Lookout all clear
[ ]  Throttle set 1700 rpm
[ ]  Oil temp & pressure green arc
[ ]  Magnetos left, both, right, both
[ ]  Carb Heat on then off
[ ]  Ammeter positive charge
[ ]  Suction 4.5” – 5.4” Hg
[ ]  Slow idle smooth running
[ ]  Throttle set 1000 rpm

PRE T/O VITAL ACTIONS
[ ]  T trims set, throttle friction adjusted
[ ]  M mixture rich
[ ]  P primer – locked
[ ]  F fuel on, contents checked
[ ]  F flaps set
[ ]  I instruments checked and set
[ ]  auto pilot checked
[ ]  S switches, as required
[ ]  C controls full & free
[ ]  H hatches & harnesses secure

PRE LINE UP CHECKS
[ ]  F fuel pump on, flaps set
[ ]  I instruments, DG to runway heading
[ ]  S switches, lights as required
[ ]  T transponder to ALT

AFTER T/O CHECKS
[ ]  Flaps retracted
[ ]  Power set as required
[ ]  Oil temp & pressure green arc

Pre manoeuvre checks
[ ]  H Height
[ ]  A Airframe
[ ]  S Security
[ ]  E Engine
[ ]  L Location
[ ]  L Lookout

PRE LANDING CHECKS
[ ]  S Speed
[ ]  U Undercarriage down
[ ]  M Mixture rich
[ ]  F Fuel contents
[ ]  H Hatches & Harnesses secure
[ ]  B Brakes, check pressure and off

AFTER LANDING CHECKS
[ ]  Flaps retract
[ ]  Carburretor heat off
[ ]  Transponder STBY
[ ]  Radio to SMC

SHUTDOWN
[ ]  Park brake on
[ ]  Throttle set 1000 rpm
[ ]  Avionics off
[ ]  Beacon off
[ ]  Magnetos check for RPM drop
[ ]  Temp and pressure green arc
[ ]  Mixture idle cut off
[ ]  Throttle closed
[ ]  Magnetos off, key out
[ ]  Master off
[ ]  Park brake release if tieing down

POST FLIGHT
[ ]  Controls secure
[ ]  Hatches secure
[ ]  Tie downs secured

AEROBATIC SPEEDS (A152 only)
[ ]  Flick roll 80 KIAS
[ ]  Barrel roll 115 KIAS
[ ]  Loop 115 KIAS
[ ]  Roll of the top 130 KIAS
[ ]  Steep turn 100 KIAS
[ ]  Chandelle & lazy eight 105 KIAS
[ ]  Spin slow deceleration

“G” LIMITS (A152 only)
[ ]  Flap up +6 -3
[ ]  Flap down +3.5

RADIO FREQUENCIES
[ ]  MB GROUND 119.9 MHz
[ ]  MB TOWER (EAST) 118.1 MHz
[ ]  MB TOWER (WEST) 123.0 MHz
[ ]  MB ATIS 398 or 120.9 MHz
[ ]  EN GROUND 121.9 MHz
[ ]  EN TOWER 125.1 MHz
[ ]  EN ATIS 356 or 119.8 MHz
[ ]  ML RAS 135.7 MHz
[ ]  ML APP 124.7 MHz
[ ]  ML DEP 118.9 or 129.4 MHz
[ ]  ML TWR 120.5 MHz
[ ]  ML SMC 121.7 MHz
[ ]  ML ACD 127.2 MHz
[ ]  ML ATIS 114.1 or 132.7 MHz

ENGINE FIRE DURING START  [EMERGENCY]
[ ]  Starter crank engine
[ ]  Mixture idle cut off
[ ]  Throttle open
[ ]  Fuel selector off
[ ]  Abandon if fire continues

ENGINE FIRE IN FLIGHT  [EMERGENCY]
[ ]  Mixture idle cut-off
[ ]  Throttle closed
[ ]  Fuel Selector off
[ ]  Heater off
[ ]  Defroster off
NOTE: Proceed with POWER OFF LANDING

ENGINE FAILURE IN FLIGHT  [EMERGENCY]
INITIAL ACTIONS:
CHECK FOR FIRE
[ ]  Throttle set 1/3 position
[ ]  Carburetor Heat on
[ ]  Mixture rich
[ ]  Fuel selector check on
ASSESS WIND
SELECT FIELD
MAKE PLAN
TROUBLE CHECKS:
[ ]  Fuel on, contents checked
[ ]  Mixture through range, set rich
[ ]  Oil temps and pressure
[ ]  Switches check magnetos
[ ]  Throttle through range set 1/3 position
MAYDAY CALL
SHUTDOWN CHECKS:
[ ]  Brakes check pressure and off
[ ]  Undercarriage down
[ ]  Switches all off, fuel off
[ ]  Hatches and harnesses secure

LOSS OF OIL PRESSURE / HIGH OIL TEMPERATURE  [EMERGENCY]
[ ]  Land as soon as possible and investigate cause.
[ ]  Prepare for power off landing

C152 / A152 (CESSNA) DATA
AIRSPEEDS
[ ]  Basic Stall Speed (VS1) 40 KIAS
[ ]  Stall with Flap (VS0) 35 KIAS
[ ]  Best Climb Angle (VX) 55 KIAS
[ ]  Best Climb Rate (VY) 65 KIAS
[ ]  Cruise Climb (Normal) 80 KIAS
[ ]  Flap Limit Speed (VFE) 85 KIAS
[ ]  Threshold 60 KIAS
[ ]  Manoeuvre Speed (VA) 93 - 104 KIAS
[ ]  (A152…108 KIAS)
[ ]  Flight Planning TAS 100 KTAS
[ ]  Maximum Cruising (VNO) 111 KIAS
[ ]  Never Exceed (VNE) 149 KIAS
[ ]  Best Glide 60 KIAS
[ ]  TOSS 54 KIAS
[ ]  Base 75 KIAS
[ ]  Final 65 KIAS
[ ]  Maximum Crosswind 15 KIAS
WEIGHT LIMITATIONS
[ ]  Max Takeoff Weight 757 Kg Lb
[ ]  Empty Weight: Refer flight manual
[ ]  Max Baggage Weight
FUEL
[ ]  Type: 100 Octane Avgas (green) or 100 LL (blue)
[ ]  Quantity: Total 98 lt, Useable 93 lt (fuel flow at 75%)
[ ]  (Long range tanks: 148 / 143 Lt)
[ ]  Typical Consumption: 23 lt per hour
[ ]  Endurance with 45 min reserve intact: 4.2 hrs
POWER SETTINGS
[ ]  Max RPM 2700 RPM
[ ]  Static RPM
ENGINE
[ ]  Avco Lycoming O-335 L2C or N2C
[ ]  4 cylinder, horizontally opposed, direct drive, air cooled, normally aspirated
[ ]  Output: 110 Hp @ 2550 rpm
OIL
[ ]  Type: Aviation grade D100
[ ]  Quantity: Max 8 US quarts, Min 6 US quarts (Company reqts)
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