Cessna 152 — c152
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Light Signals" item count differs between passes (7 vs 11); verify nothing was dropped.

Preflight Inspection
COCKPIT
[ ]  Aircraft docs .... Check
[ ]  Control wheel lock .... Remove
[ ]  Hobbs/Tach .... Check/Record
[ ]  Ignition .... Off
[ ]  Master Switch .... On
[ ]  Fuel quantity indicators .... check
[ ]  Flaps .... down
[ ]  Master Switch .... Off
[ ]  Fuel shutoff valve .... On
FUSELAGE AND EMPENAGE
[ ]  Rivets .... Check
[ ]  Rudder Gust Lock .... Remove
[ ]  Tail Tie-Down .... Disconnect
[ ]  Control surfaces .... free & secure
RIGHT WING
[ ]  Aileron .... free and secure
[ ]  Flaps .... secure
[ ]  Wing tie-down .... disconnect
[ ]  Main wheel tire .... inflated
[ ]  Brakes .... not leaking
[ ]  Fuel tank sump .... sample
[ ]  Fuel Quantity .... check
[ ]  Fuel Filler cap .... Secure
NOSE
[ ]  Engine oil level .... check
[ ]  Fuel strainer .... sample
[ ]  Propeller and spinner .... check
[ ]  Alternator belt .... check
[ ]  Air intake .... check
[ ]  Carburetor air filter .... check
[ ]  Landing lights .... check
[ ]  Nose wheel strut & tire .... check
[ ]  Nose-Tie down .... disconnect
[ ]  Static source opening .... check
LEFT WING
[ ]  Main wheel tire .... inflated
[ ]  Brakes .... not leaking
[ ]  Fuel tank sump .... sample
[ ]  Fuel Quantity .... check
[ ]  Fuel Filler cap .... Secure
[ ]  Wing tie-down .... disconnect
[ ]  Pitot tube .... uncover and check
[ ]  Stall warning .... check
[ ]  Fuel tank vent opening .... check
[ ]  Wing tie-down .... disconnect
[ ]  Aileron .... free and secure
[ ]  Flaps .... secure

Before starting engine
[ ]  Preflight inspection .... complete
[ ]  Seats, belts .... adjust and lock
[ ]  Fuel shutoff valve .... ON
[ ]  Radios & elect .... OFF
[ ]  Brakes .... test and set
[ ]  Circuit breakers .... IN

Starting Engine
[ ]  Mixture .... Rich (IN)
[ ]  Carb heat .... COLD (IN)
[ ]  Prime .... As required; locked
[ ]  Throttle .... Open ½ inch
[ ]  Propeller area .... CLEAR
[ ]  Master Switch .... ON
[ ]  Beacon .... ON
[ ]  Ignition .... START
[ ]  Throttle .... Adjust 1000 rpm
[ ]  Oil Pressure .... check normal
[ ]  Avionics .... ON
[ ]  Transponder .... Standby
[ ]  Flaps .... UP

Before Takeoff
[ ]  Parking brake .... SET
[ ]  Cabin doors .... CLOSE & LATCH
[ ]  Flight controls .... free & correct
[ ]  Instruments (4) .... SET
[ ]  Fuel Shutoff Valve .... ON
[ ]  Mixture .... RICH (IN)
[ ]  Trim .... set for TAKEOFF
[ ]  Throttle .... 1700 rpm
[ ]  Magnetos .... check
[ ]  Suction gage .... check
[ ]  Instruments .... check
[ ]  Ammeter .... check
[ ]  Carb heat .... ON
[ ]  Throttle .... IDLE -- chk
[ ]  Radios .... SET
[ ]  Beacon/lights .... ON
[ ]  Throttle friction lock .... ADJUST
[ ]  Brakes .... TEST

Engine failure  [EMERGENCY]
TAKEOFF
TAKEOFF
[ ]  Throttle .... IDLE
[ ]  Brakes .... apply
[ ]  Flaps .... UP
[ ]  Mixture .... IDLE cut-off
[ ]  Ignition .... OFF
[ ]  Master switch .... OFF

Engine failure  [EMERGENCY]
AFTER TAKEOFF
AFTER TAKEOFF
[ ]  Airspeed .... 60 KIAS
[ ]  Mixture .... Idle Cut-off
[ ]  Fuel shutoff valve .... OFF
[ ]  Ignition .... OFF
[ ]  Flaps .... as required
[ ]  Master switch .... OFF

Engine failure  [EMERGENCY]
DURING FLIGHT
DURING FLIGHT
[ ]  Airspeed .... 60 KIAS
[ ]  Carb Heat .... ON
[ ]  Primer .... IN & Locked
[ ]  Fuel Shutoff valve .... ON
[ ]  Mixture .... RICH
[ ]  Ignition .... BOTH (or START)
[ ]  Airspeed .... 60/65 (flaps)
[ ]  Mixture .... cutoff
[ ]  Fuel shutoff valve .... off
[ ]  Ignition .... off
[ ]  Flaps .... as required
[ ]  Mayday .... transmit 121.5
[ ]  Master switch .... off
[ ]  Doors .... unlatch
[ ]  Touchdown .... tail low

Carburetor Icing  [EMERGENCY]
[ ]  Throttle .... FULL
[ ]  Carb Heat .... ON (out)
[ ]  Mixture .... Adjust

Engine Roughness  [EMERGENCY]
[ ]  Magnetos .... check
[ ]  Mixture .... lean as necessary

Engine Fire during start  [EMERGENCY]
[ ]  Crank .... Continue
[ ]  Power .... 1700 RPM
[ ]  Engine .... Shut down and inspect

Engine Fire during flight  [EMERGENCY]
[ ]  Mixture .... Idle Cut-off
[ ]  Fuel shut off valve .... OFF
[ ]  Master Switch .... OFF
[ ]  Cabin head/air .... OFF
[ ]  Airspeed .... 85 KIAS

Electrical failure  [EMERGENCY]
[ ]  Load meter .... verify
[ ]  Alternator .... off
[ ]  Reduce load .... to minimum
[ ]  Breaker/alt .... chk & reset
[ ]  Alternator .... on
IF STILL NO POWER:
[ ]  Alternator .... off
[ ]  Reduce load and land

Electrical overload  [EMERGENCY]
[ ]  Master Switch .... OFF
[ ]  Master Switch .... ON
[ ]  Over-voltage light .... OFF
[ ]  or TERMINATE flight .... ASAP

Spin Recovery  [EMERGENCY]
[ ]  Ailerons .... NEUTRAL
[ ]  Throttle .... IDLE
[ ]  Rudder .... Full opposite
[ ]  Control wheel .... full forward
[ ]  Rudder control/wheel .... Neutral
[ ]  Pitch .... Level

Takeoff
[ ]  Flaps .... UP
[ ]  Carb heat .... COLD (IN)
[ ]  Transponder .... Altitude
[ ]  Trim .... set for TAKEOFF
[ ]  Throttle .... FULL
[ ]  Tach, oil, airspeed .... check
[ ]  Elevator .... Lift at 50 KIAS
[ ]  Climb .... 70-80 KIAS

Cruise
[ ]  Pitch .... Set
[ ]  Throttle .... As required
[ ]  Trim .... Set
[ ]  Mixture .... Adjust

Pre-landing checklist
[ ]  Fuel selector .... ON
[ ]  Mixture .... Rich
[ ]  Carb Heat .... ON
[ ]  Seatbelts .... Fastened

Approach
[ ]  Flight instruments .... Ckd & Set
[ ]  Radios .... Checked
[ ]  ATIS .... Checked
[ ]  Carb Heat .... ON
[ ]  Mixture .... Rich

After landing
[ ]  Flaps .... UP
[ ]  Carb Heat .... COLD (IN)
[ ]  Transponder .... Standby
[ ]  Landing light .... OFF

Parking
[ ]  Avionics .... OFF
[ ]  Electrical .... OFF
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... Cut-off
[ ]  Ignition switch .... OFF
[ ]  Master switch .... OFF

Securing the aircraft
[ ]  Control Lock .... Install
[ ]  Hobbs/Tach .... Record
[ ]  Door/Window .... Secure
[ ]  Tie-downs .... Secure

Short field take-off
[ ]  Take-off checklist .... complete
[ ]  Taxi .... max runway
[ ]  Brakes .... set and hold
[ ]  Flaps .... 10(
[ ]  Throttle .... FULL
[ ]  Brakes .... release
[ ]  Climb .... 54 KIAS
[ ]  Flaps .... retract when clear
[ ]  Airspeed .... 67 KIAS

Short field landing
[ ]  Pre-landing check .... complete
[ ]  Approach .... 54 KIAS
[ ]  Flaps .... 30(
[ ]  Throttle .... maintain glide
[ ]  Touchdown .... power off
[ ]  Flaps .... UP
[ ]  Elevator .... Full up
[ ]  Braking .... Heavy as required

Soft field take-off
[ ]  Take-off checklist .... complete
[ ]  Flaps .... 10(
[ ]  Taxi .... keep rolling
[ ]  Climb .... 54 KIAS
[ ]  Flaps .... retract
[ ]  Airspeed .... 67 KIAS

Soft field landing
[ ]  Pre-landing check .... complete
[ ]  Throttle .... 1500 RPM
[ ]  Flaps .... 10(
[ ]  Airspeed .... 60 KIAS
[ ]  Touchdown .... main first, softly
[ ]  Landing roll .... nose wheel up
[ ]  Elevator .... UP
[ ]  Braking .... as required

Go-around
[ ]  Throttle .... FULL
[ ]  Carb Heat .... Cold (IN)
[ ]  Flaps .... UP
[ ]  Airspeed .... 67 KIAS

Light Signals
LIGHT SIGNALS:
NOTE: Steady Green — On Ground: Takeoff; In Flight: Land
NOTE: Flashing Green — On Ground: Taxi; In Flight: Return to land
NOTE: Steady Red — On Ground: Stop; In Flight: Give way
NOTE: Flashing Red — On Ground: Clear runway; In Flight: Do not land
NOTE: Flashing white — On Ground: Return to ramp; In Flight: --
NOTE: Red/Green alternating — WARNING – USE CAUTION
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