Cessna 152 — Matthew_Kudija_Cessna_152_EMERGENCY_PROCEDURES
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

ENGINE FAILURES  [EMERGENCY]
ENGINE FAILURE DURING TAKEOFF:
[ ]  Throttle .... IDLE
[ ]  Brakes .... APPLY
[ ]  Flaps .... RETRACT
[ ]  Mixture .... IDLE CUTOFF
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF
ENGINE FAILURE AFTER TAKEOFF:
[ ]  Airspeed .... 60 KIAS
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Shutoff .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Flaps .... AS REQUIRED
[ ]  Master Switch .... OFF
ENGINE FAILURE DURING FLIGHT:
[ ]  Airspeed .... 60 KIAS
[ ]  Carb Heat .... ON
[ ]  Primer .... IN and LOCKED
[ ]  Fuel Shutoff .... ON
[ ]  Mixture .... RICH
[ ]  Ignition Switch .... BOTH
GENERAL:
[ ]  Airspeed .... 60
[ ]  Best Field
COCKPIT CHECKS
[ ]  Carb Heat .... ON
[ ]  Mixture
[ ]  Throttle
[ ]  Fuel Shutoff
[ ]  Oil Press/Temp
[ ]  Fuel Level

FORCED LANDINGS  [EMERGENCY]
WITHOUT ENGINE POWER:
[ ]  Airspeed .... 65 (up) 60 (dn)
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Shutoff .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Flaps .... FULL
[ ]  Master Switch .... OFF
[ ]  Doors .... UNLATCH
[ ]  Touchdown .... TAIL LOW
[ ]  Brakes .... APPLY HEAVILY
WITH ENGINE POWER:
[ ]  Airspeed .... 60 KIAS
[ ]  Flaps .... 20°
[ ]  Selected Field .... Fly Over
[ ]  Radio/Electrical .... OFF
[ ]  Flaps .... 30°
[ ]  Airspeed .... 55 KIAS
[ ]  Master Switch .... OFF
[ ]  Doors .... UNLATCH
[ ]  Touchdown .... Tail Low
[ ]  Ignition Switch .... OFF
[ ]  Brakes .... APPLY HEAVILY
DITCHING:
[ ]  Radio .... MAYDAY
[ ]  Objects .... Secure/Jettison
[ ]  Approach
[ ]  High Winds-Heavy Seas, Into wd
[ ]  Lt. Winds, Heavy Swells, Parallel
[ ]  Flaps .... 30°
[ ]  Power .... 300 FPM, 55 Kias
[ ]  Doors .... UNLATCH
[ ]  Touchdown .... LEVEL
[ ]  Face .... CUSION
[ ]  Airplane .... EVACUATE
[ ]  Vests/Raft .... INFLATE

FIRES  [EMERGENCY]
DURING START ON GROUND:
[ ]  Cranking .... CONTINUE
[ ]  Power .... 1700 RPM
[ ]  Shutdown and Inspect
ENGINE FIRE IN FLIGHT:
[ ]  Mixture .... IDLE CUTOFF
[ ]  Fuel Shutoff .... OFF
[ ]  Master Switch .... OFF
[ ]  Cabin Heat/Air .... OFF
[ ]  Airspeed .... 85 KIAS
[ ]  Forced Landing .... Execute
ELECTRICAL FIRE IN FLIGHT:
[ ]  Master Switch .... OFF
[ ]  All Switches .... OFF
[ ]  Cabin Air/Heat .... CLOSED
[ ]  Fire Ext. .... ACTIVATE
NOTE: if secure, and need electrical:
[ ]  Master Switch .... ON
[ ]  Breakers .... CHECK
[ ]  Switches .... On, one at time
[ ]  Vents .... OPEN
CABIN FIRE:
[ ]  Master Switch .... OFF
[ ]  Vents .... CLOSED
[ ]  Fire Ext. .... ACTIVATE
[ ]  LAND
WING FIRE:
[ ]  Nav. Light .... OFF
[ ]  Strobe Light .... OFF
[ ]  Pitot Heat .... OFF
[ ]  Side Slip

Flat Main Tire:  [EMERGENCY]
[ ]  Flaps .... As Desired
[ ]  Approach .... NORMAL
[ ]  Touchdown- good first

ELECTRICAL SYSTEM  [EMERGENCY]
OVER-VOLTAGE LIGHT ILLUMINATION:
[ ]  Master Switch .... OFF
[ ]  Master Switch .... ON
[ ]  Over-Voltage Light .... OFF
[ ]  Terminate Flight .... if ON
AMMETER SHOWS DISCHARGE:
[ ]  Alternator .... OFF
[ ]  Noness. Electrical .... OFF
[ ]  Flight .... TERMINATE

COMMUNICATION  [EMERGENCY]
[ ]  MAYDAY .... MAYDAY
[ ]  Name of Station
[ ]  Name of Aircraft
[ ]  Nature of Emergency
[ ]  Weather
[ ]  Intentions or Request
[ ]  Present position/ heading
[ ]  Altitude
[ ]  Fuel Remaining
[ ]  Number of people aboard
[ ]  Other Useful Info
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