Cessna 152 — TFA_Cessna_152_Checklist_2004-01
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Before Takeoff" item count differs between passes (19 vs 20); verify nothing was dropped.
content_gap: Section "Starting Engine" item count differs between passes (14 vs 15); verify nothing was dropped.

Preflight Inspection Cockpit
[ ]  A.R.O.W. Documents .... CHECK
[ ]  Hobbs Meter .... CHECK
[ ]  Control Lock .... REMOVE
[ ]  Ignition Switch .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Master (look prop is clear) .... ON
[ ]  Fuel Quantity .... CHECK
[ ]  Lights .... CHECK
[ ]  Flaps .... 30 DEGREES
[ ]  Master Switch .... OFF
[ ]  Fuel Shutoff Valve .... ON

Preflight Inspection Fuselage & Empennage
[ ]  Rudder Gust Lock .... REMOVE
[ ]  Fuselage .... CHECK
[ ]  Tail Tie Down .... UNTIE
[ ]  Elevator .... FREE & SECURE
[ ]  Rudder .... FREE & SECURE
[ ]  VOR Antennas .... CHECK
[ ]  Trim Tab .... CHECK

Preflight Inspection Right Wing
[ ]  Flap .... SECURE
[ ]  Aileron .... FREE & SECURE
[ ]  Skin/Tip/Lights .... CHECK
[ ]  Wing Tie Down .... UNTIE
[ ]  Main Wheel Tire .... INFLATED
[ ]  Brakes .... CHECK
[ ]  Fuel Tank Sump .... SAMPLE
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Filler Cap .... SECURE

Preflight Inspection Nose
[ ]  Engine Oil .... 4-6 QUARTS
[ ]  Fuel Strainer .... SAMPLE
[ ]  Belly Quick Drain .... SAMPLE
[ ]  Propeller & Spinner .... CHECK
[ ]  Air Intakes .... FREE & OPEN
[ ]  Carburetor Air Filter .... CLEAR
[ ]  Landing Light .... SECURE
[ ]  Nose Wheel & Strut .... CHECK
[ ]  Static Port .... OPEN

Preflight Inspection Left Wing
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Filler Cap .... SECURE
[ ]  Main Wheel Tire .... INFLATED
[ ]  Brakes .... CHECK
[ ]  Pitot Tube & Drain .... FREE
[ ]  Stall Warning Opening .... CHECK
[ ]  Fuel Tank Vent .... OPEN
[ ]  Wing Tie Down .... UNTIE
[ ]  Skin/Tip/Lights .... CHECK
[ ]  Aileron .... FREE & SECURE
[ ]  Flap .... SECURE
[ ]  Fuel Tank Sump .... SAMPLE

Before Starting Engine
[ ]  Preflight .... COMPLETE
[ ]  Passenger Brief .... COMPLETE
[ ]  Seat/Seat Belts .... LOCKED
[ ]  Fuel Shutoff Valve .... ON
[ ]  Electrical Equipment .... OFF
[ ]  Circuit Breakers .... IN
[ ]  Brakes .... SET & HOLD

Starting Engine
[ ]  Mixture .... RICH
[ ]  Throttle .... OPEN 1/2 INCH
[ ]  Carburetor Heat .... COLD
[ ]  Prime .... AS REQUIRED
[ ]  Beacon .... CHECK ON
[ ]  Master Switch .... ON
[ ]  Propeller Area .... CLEAR
[ ]  Ignition Switch .... START
[ ]  Throttle .... SMOOTH IDLE
[ ]  Oil Pressure .... CHECK
[ ]  Carburetor Heat .... ON or OFF FOR WX & RNWY CONDITION
[ ]  Comm.Radio/Xpdr. .... ON/STBY
[ ]  Pitot Heat .... AS REQUIRED
[ ]  Flaps .... UP & VERIFIED

Before Takeoff
[ ]  Brakes .... SET & HOLD
[ ]  Doors & Windows .... LOCKED
[ ]  Controls .... FREE & CORRECT
[ ]  Trim .... SET FOR TAKEOFF
[ ]  Flight Instr. .... SET & CHECK
[ ]  Fuel Shutoff Valve .... ON
[ ]  Mixture .... RICH
[ ]  Throttle .... 1700 RPM
[ ]  Mags .... RT/BOTH/LEFT/BOTH
NOTE: Magnetos drop should not exceed 125 RPM or 50 RPM differential between magnetos
[ ]  Carb. Heat .... ON/CHECK/OFF
[ ]  Engine Instr. .... GREEN / NORM
[ ]  Ammeter / Alternator .... CHECK
[ ]  Suction Gauge .... CHECK
[ ]  Throttle .... SMOOTH IDLE
[ ]  Carburetor Heat .... ON or OFF FOR WX & RNWY CONDITION
[ ]  Comm./Nav. Radios .... SET
[ ]  Pitot Heat .... ON AS REQUIRED
[ ]  Throttle Lock .... TIGHTEN

Taking Runway
NOTE: Do prior to or by memory
[ ]  Clearance Received .... TAKE OFF or POSITION & HOLD
[ ]  Approach End .... CLEAR
[ ]  Lights .... ON
[ ]  Camera .... TRANSPONDER ALT
[ ]  Action .... D.G. TO RNWY HDG
[ ]  Time Off .... TAKEN

Normal Take Off
[ ]  Flaps .... 0 DEGREES
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF
[ ]  Airspeed/Eng. Instr. .... CHECK
[ ]  Rotate .... 50 KIAS
[ ]  Climb Speed .... 65-75 KIAS

Soft Field Take Off
[ ]  Yoke .... FULL AFT
[ ]  Flaps .... 10 DEGREES
[ ]  Taxi .... KEEP ROLLING
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF
[ ]  Airspeed/Eng. Instr. .... CHECK
[ ]  Lift Off .... SAFE AIRSPEED
[ ]  Accelerate .... Vx = 55 or Vy = 67
[ ]  Flaps (Over Obstacle Vy+) .... UP

Short Field Take Off
[ ]  Flaps .... 10 DEGREES
[ ]  Brakes .... HOLD
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF
[ ]  Engine Instr. .... GREEN/NORM
[ ]  Brakes .... RELEASE
[ ]  Rotate .... 54 KIAS
[ ]  Climb Speed .... 54 KIAS
[ ]  Over Obstacle .... 67 KIAS & FLAPS UP

Enroute Climb
[ ]  Airspeed .... 70-80 KIAS
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... RICH OR AS REQ.

Cruise
[ ]  Airspeed .... ESTABLISHED
[ ]  Power 65% .... 2300 RPM
[ ]  Trim .... ADJUST
[ ]  Mixture .... LEAN AS REQUIRED
[ ]  Lights .... AS REQUIRED
[ ]  Flight Plan .... OPEN
[ ]  Company Freq. .... MONITOR

Descent
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON
[ ]  Throttle .... AS REQUIRED
[ ]  Landing Light .... VERIFY ON

Before Landing
[ ]  Carb. Heat .... VERIFY ON
[ ]  Gas (Fuel Valve) .... ON
[ ]  Undercarriage (Fixed) .... DOWN
[ ]  Mixture .... FULL RICH
[ ]  Primer .... IN & LOCKED
[ ]  Seatbelts / Switches .... CHECK

Normal Landings
[ ]  Airspeed .... 60-70 KIAS
[ ]  Flaps .... EXTENDED AS REQ.
[ ]  Airspeed (w/flaps) .... 55-65 KIAS
[ ]  Throttle .... AS REQ. TO RNWY
[ ]  Throttle .... TO IDLE ON RNWY
[ ]  Directional Control .... MAINTAIN

Soft Field Landing
[ ]  Airspeed .... 60-70 KIAS
[ ]  Flaps .... 30 DEGREES
[ ]  Short Final .... 54-60 KIAS
[ ]  Throttle .... AS REQUIRED
[ ]  Touchdown .... NOSE HIGH
[ ]  Nose Wheel .... HOLD OFF
[ ]  Elevator .... FULL AFT FOR TAXI

Short Field Landing
[ ]  Airspeed .... 60-70 KIAS
[ ]  Flaps .... 30 DEGREES
[ ]  Final .... MAINTAIN 54 KIAS
[ ]  Power .... REDUCE TO IDLE
[ ]  Flaps .... RETRACT
[ ]  Brakes .... APPLY HEAVILY

Go Around
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... COLD/OFF
[ ]  Flaps 20° .... IMMEDIATELY
[ ]  Airspeed .... INCREASING
[ ]  Flaps Up Increments .... 10° & 0°

After Landing
[ ]  Flaps .... UP
[ ]  Carburetor Heat .... COLD
[ ]  Transponder .... OFF
[ ]  Pitot Heat .... OFF
[ ]  Lights .... AS REQUIRED
[ ]  Taxi Clearance .... OBTAIN

Engine Shutdown & Securing Airplane
[ ]  Avionics/Avionics Master .... OFF
[ ]  Lights (except beacon) .... OFF
[ ]  Throttle .... MIN. 1000 RPM
[ ]  Mixture .... IDLE CUT OFF
[ ]  Ignition (prop stopped) .... OFF
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
[ ]  Tie Down Aircraft .... SECURELY
[ ]  Hobbs .... RECORD
[ ]  Post-flight Inspection .... DO
[ ]  Flight Plan .... CLOSE

Engine Fire During Flight  [EMERGENCY]
[ ]  Fuel Shutoff Valve [MEMORY] .... OFF
[ ]  Mixture [MEMORY] .... IDLE CUT-OFF
[ ]  Master Switch [MEMORY] .... OFF
[ ]  Cabin Heat/Air [MEMORY] .... OFF/CLOSED
[ ]  Airspeed .... 85 KIAS
NOTE: If fire is not extinguished, increase glide to an airspeed that provides an incombustible mixture
[ ]  Forced Landing .... EXECUTE

Electrical Fire In Flight  [EMERGENCY]
[ ]  Master Switch [MEMORY] .... OFF
[ ]  Switches (except Ignition) .... OFF
[ ]  Cabin Heat / Vents .... CLOSED
[ ]  Extinguisher .... ACTIVATE
[ ]  Fire Out .... VENTILATE CABIN

Engine Failure — Takeoff Run  [EMERGENCY]
[ ]  Throttle [MEMORY] .... IDLE
[ ]  Brakes .... APPLY
[ ]  Flaps .... UP
[ ]  Mixture .... IDLE CUT OFF
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF

Engine Failure — After Takeoff  [EMERGENCY]
[ ]  Best Glide [MEMORY] .... 60 KIAS
[ ]  Mixture .... IDLE CUT OFF
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Flaps .... AS REQUIRED
[ ]  Master Switch .... OFF

Engine Failure — During Flight  [EMERGENCY]
[ ]  Airspeed — Best Glide [MEMORY] .... 60 KIAS
[ ]  Best Place To Land .... TURN TO
[ ]  Carburetor Heat .... ON
[ ]  Fuel Shutoff Valve .... ON
[ ]  Mixture .... RICH
[ ]  Ignition Switch .... ON BOTH / OR START IF PROP. IS STOPPED
[ ]  Primer .... IN & LOCKED
[ ]  Trouble Shoot .... MAGS CYCLE, THROTTLE PUMP
NOTE: Unable To Re-start:
[ ]  Declare May Day .... 121.5 or ATC
[ ]  Squawk .... 7700

Forced Landing Without Engine Power  [EMERGENCY]
[ ]  Airspeed .... 65 KIAS FLAPS UP / 60 KIAS FLAP DOWN
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Mixture .... IDLE CUT OFF
[ ]  Ignition Switch .... OFF
[ ]  Doors .... UNLATCH
[ ]  Flaps .... AS REQUIRED
[ ]  Master Switch .... OFF LAST
[ ]  Touchdown .... TAIL LOW
[ ]  Brakes .... APPLY HEAVILY

Precautionary Landing w/Engine Power  [EMERGENCY]
[ ]  Airspeed .... 60 KIAS
[ ]  Selected Field .... FLY OVER
NOTE: Note any obstacles
[ ]  Electrical Equipment .... OFF
[ ]  Flaps .... 30 DEGREES
[ ]  Airspeed .... 55 KIAS
[ ]  Master Switch .... OFF
[ ]  Doors .... UNLATCH
[ ]  Touchdown .... TAIL LOW
[ ]  Ignition Switch .... OFF
[ ]  Brakes .... APPLY HEAVILY

Electrical Malfunction  [ABNORMAL]
OVER VOLTAGE CONDITION
[ ]  Alternator .... OFF
[ ]  Alternator Circuit Breaker .... PULL
[ ]  Nonessential Electrical .... OFF
[ ]  Flight .... TERMINATE as soon as practical
LOW VOLTAGE CONDITION
[ ]  Avionics / Electrical .... OFF
[ ]  Alternator Circuit Breaker .... IN
[ ]  Master .... OFF BOTH SIDES
[ ]  Master .... ON
[ ]  Voltage Light .... CHECK OFF
NOTE: If low-voltage light illuminates again
[ ]  Alternator .... OFF
[ ]  Nonessential Electrical .... OFF
[ ]  Flight .... TERMINATE as soon as practical

Wing Fire  [EMERGENCY]
[ ]  Nav Lights .... OFF
[ ]  Strobe Lights .... OFF
[ ]  Pitot Heat .... OFF
[ ]  Perform .... SIDE SLIP AWAY FROM THE FUEL TANK AND CABIN

Engine Fire During Start  [EMERGENCY]
Engine fire during start
[ ]  Cranking .... CONTINUE
NOTE: IF ENGINE STARTS
[ ]  Power .... 1700 RPM/1 MIN.
[ ]  Engine .... SHUTDOWN
[ ]  Airplane .... INSPECT
NOTE: ENGINE FAILS TO START
[ ]  Cranking .... CONTINUE
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... IDLE CUT OFF
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Master Switch .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Damage Inspection .... DO

Operating Information
BEST GLIDE 60 KIAS
VX 55 KIAS
VY 67 KIAS
VA 93-104 KIAS
VNE 149 KIAS
VNO 111 KIAS
VFE 85 KIAS
LOCAL FREQUENCIES
NOTE: All take flight aircraft are required to monitor company frequency when in range and able to do so.
NOTE: Take Flight Alaska 129.25
NOTE: Merrill ATIS 123.7
NOTE: Merrill Ground 121.7
NOTE: Merrill Tower 126.0/127.55
NOTE: Anchorage Appch. N119.1/S126.4
NOTE: Big Lake/Willow/Wasilla 122.8
NOTE: Goose Bay 122.9
NOTE: Birchwood 123.0
NOTE: Cool/Cold Engine T.F.A. Policy: Ensure either oil temp. is in the green or moving prior to engine run ups, mag. checks and prior to flight. Pre-heating a cold engine is required before starting during winter operations.
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