Cessna 172F Skyhawk — C-172FChecklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

CABIN
[ ]  Papers .... A.R.O.W.
[ ]  Control Wheel Lock .... REMOVE
[ ]  Mags .... OFF
[ ]  Avionics .... OFF
[ ]  Circuit Breakers .... IN
[ ]  Trim .... TAKEOFF
[ ]  Fuel Selector .... CHECK EACH POSITION, SET BOTH
[ ]  Prop .... CLEAR
[ ]  Master .... ON
[ ]  Fuel Gauges .... TRUE
[ ]  Flaps .... EXTEND
[ ]  Lights .... INTERIOR / EXTERIOR
[ ]  Pitot Heat .... TEST
[ ]  Stall Indicator .... TEST
[ ]  Master .... OFF
[ ]  Fuel Strainer .... PULL (4 sec)
[ ]  Baggage Door .... LOCK

EMPENNAGE
[ ]  Left Elevator .... CHECK
[ ]  Tiedown .... DISCONNECT
[ ]  Rudder .... CHECK
[ ]  Rudder and Elevator Cables .... CHECK
[ ]  Navigation Light .... SECURE
[ ]  Trim Tab Alignment .... CHECK (within ¼" of elevator)
[ ]  Right Elevator .... CHECK
[ ]  Antennas .... CHECK

RIGHT WING
[ ]  Flap .... CHECK
[ ]  Aileron .... CHECK
[ ]  Strobe/Navigation Lights .... CHECK
[ ]  Tiedown .... DISCONNECT
[ ]  Fuel Quantity .... CHECK VISUALLY
[ ]  Fuel Filler Cap .... SECURE
[ ]  Right Fuel Tank Sump .... DRAIN
[ ]  Chock .... REMOVE
[ ]  Tire .... CHECK (24 PSI)
[ ]  Brake Assembly .... CHECK

NOSE
[ ]  Chock .... REMOVE
[ ]  Nose Strut .... 1-3" EXTENSION
[ ]  Nose Tire .... CHECK (26 PSI)
[ ]  Exhaust System .... CHECK
[ ]  Air Filter .... CLEAR
[ ]  Engine Air Inlets .... CLEAR
[ ]  Prop/Spinner .... CHECK
[ ]  Oil Level .... 7 QTS (under 3 HR flight), 8 QTS (extended flight)
[ ]  Oil Cap .... SECURE
[ ]  Engine Compartment .... CHECK
[ ]  Access Door .... SECURE
[ ]  Static Port .... CLEAR

LEFT WING
[ ]  Chock .... REMOVE
[ ]  Tire .... CHECK (24 PSI)
[ ]  Brake Assembly .... CHECK
[ ]  Left Fuel Tank Sump .... DRAIN
[ ]  Fuel Quantity .... CHECK VISUALLY
[ ]  Fuel Filler Cap .... SECURE
[ ]  Pitot Tube .... CLEAR
[ ]  Fuel Vent .... CLEAR
[ ]  Tiedown .... DISCONNECT
[ ]  Landing/Taxi Lights .... CHECK
[ ]  Strobe/Navigation Lights .... CHECK
[ ]  Aileron .... CHECK
[ ]  Flap .... CHECK

START
[ ]  Hobbs Time .... RECORDED
[ ]  Passenger Brief .... COMPLETE
[ ]  Seat Track/Back .... LOCK
[ ]  Seat Belt /Harness .... FASTEN
[ ]  Brakes .... SET
[ ]  Beacon .... ON
[ ]  Navigation Lights .... AS REQUIRED
[ ]  Mixture .... RICH
[ ]  Throttle .... OPEN 1/8"
[ ]  Carb Heat .... OFF
[ ]  Prime .... AS REQUIRED
[ ]  Prop .... CLEAR
[ ]  Master .... ON
[ ]  Mags .... START
[ ]  Throttle .... 1,000 RPM
[ ]  Ammeter .... CHECK
[ ]  Oil Pressure .... CHECK
[ ]  Mixture .... LEAN

PRE-TAXI
[ ]  Flaps .... UP
[ ]  Cabin Heat & Air .... AS DESIRED
[ ]  Avionics .... ON / SET
[ ]  Transponder .... CODE / STANDBY
[ ]  Clock .... SET
[ ]  Airspeed Indicator .... CHECK
[ ]  Attitude Indicator .... SET
[ ]  Heading Indicator .... SET
[ ]  VSI .... CHECK
[ ]  ATIS/AWOS .... COPY
[ ]  Altimeter .... SET / CHECK
[ ]  Taxi Light .... AS REQUIRED

TAXI
[ ]  Brakes .... TEST
[ ]  Attitude Indicator .... CHECK
[ ]  Turn-and-Slip Indicator .... CHECK
[ ]  Heading Indicator .... CHECK
[ ]  Magnetic Compass .... CHECK

RUN-UP
[ ]  Brakes .... SET
[ ]  Mixture .... BEST POWER
[ ]  Primer .... IN & LOCKED
[ ]  Throttle .... 1,600 RPM
[ ]  Mags (R & L) .... CHECK (125 RPM max drop, 75 RPM max differential)
[ ]  Carb Heat .... TEST
[ ]  Vacuum .... CHECK
[ ]  Ammeter .... CHECK (0 to +2 needle widths)
[ ]  Oil Pressure .... CHECK
[ ]  Oil Temperature .... CHECK
[ ]  Throttle .... IDLE CHECK
[ ]  Throttle .... 1,000 RPM
[ ]  Mixture .... LEAN

TAKEOFF
[ ]  Heading Indicator .... SET
[ ]  Avionics .... SET
[ ]  Engine Gauges .... CHECK
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Selector .... BOTH
[ ]  Carb Heat .... OFF
[ ]  Mixture .... BEST POWER
[ ]  Trim .... TAKEOFF
[ ]  Flaps .... SET (0-10°)
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Doors/Window .... LOCKED
[ ]  Takeoff Brief .... COMPLETE
TAKING RUNWAY (LIGHTS, CAMERA, ACTION)
[ ]  Strobes .... ON
[ ]  Landing Light .... ON
[ ]  Transponder .... ALTITUDE
[ ]  Mixture .... BEST POWER

AFTER TAKEOFF
[ ]  Flaps .... UP
[ ]  Engine Gauges .... CHECK
[ ]  Landing Light .... AS DESIRED

CRUISE
[ ]  Landing Light .... OFF
[ ]  Throttle .... SET
[ ]  Mixture .... LEAN
[ ]  Engine Gauges .... CHECK
[ ]  Heading Indicator .... SET
[ ]  Fuel Selector .... BALANCE AS REQUIRED

FUEL MANAGEMENT ABOVE 5,000’ MSL
[ ]  When reaching cruise altitude above 5,000’ MSL, promptly switch fuel selector from BOTH to either LEFT or RIGHT and then to opposite tank to ensure both tanks are feeding.
[ ]  During cruise, use LEFT and RIGHT tank (not BOTH) as required to manage fuel balance.

APPROACH
[ ]  Mixture .... RICHEN AS REQUIRED
[ ]  Fuel Selector .... BOTH (below 5,000’ MSL)
[ ]  Carb Heat .... AS REQUIRED
[ ]  ATIS/AWOS .... COPY
[ ]  Altimeter .... SET
[ ]  Avionics .... SET
[ ]  Heading Indicator .... SET
[ ]  Engine Gauges .... CHECK
[ ]  Brakes .... PEDAL TEST
[ ]  Seatbelt/Harness .... FASTENED
[ ]  Landing Light .... ON

LANDING
[ ]  Fuel Selector .... BOTH
[ ]  Mixture .... BEST POWER
[ ]  Carb Heat .... ON
[ ]  Flaps .... AS DESIRED

AFTER LANDING
[ ]  Carb Heat .... OFF
[ ]  Mixture .... LEAN
[ ]  Flaps .... UP
[ ]  Strobes .... OFF
[ ]  Landing Light .... OFF
[ ]  Taxi Light .... AS REQUIRED
[ ]  Pitot Heat .... OFF
[ ]  Transponder .... STANDBY

SHUTDOWN
[ ]  Avionics .... OFF
[ ]  Fuel Selector .... RIGHT
[ ]  Throttle .... 1,000 RPM
[ ]  Mags .... GROUNDING CHECK
[ ]  Mixture .... FULL LEAN
[ ]  Prop .... CHECK STOPPED
[ ]  Mags .... OFF & KEY ON DASH
[ ]  Master .... OFF
[ ]  Lights .... OFF

SECURING
[ ]  Hobbs/Tach Time .... RECORDED
[ ]  Control Wheel Lock .... INSTALL
[ ]  Chocks .... INSTALL
[ ]  Tiedowns .... SECURE
[ ]  Baggage Door .... CLOSED
[ ]  Cabin Doors/Window .... CLOSED

FLOODED ENGINE  [ABNORMAL]
[ ]  Mixture .... FULL LEAN
[ ]  Throttle .... FULL OPEN
[ ]  Mags .... START (hold for several revolutions)
[ ]  Repeat START checklist beginning on step 10 (do not reprime).

GROUND BURNOUT  [ABNORMAL]
[ ]  Mixture .... RICH
[ ]  Throttle .... 2,000 RPM
[ ]  Mixture .... LEAN TO 50 RPM DROP BELOW BEST POWER
AFTER 1 MINUTE:
[ ]  Mixture .... RICH
[ ]  Mags .... RECHECK

RADIO FAILURE  [ABNORMAL]
[ ]  Volume .... CHECK
[ ]  Headset Connection .... CHECK
[ ]  Audio Controls .... CHECK
[ ]  Circuit Breakers .... CHECK
[ ]  Speaker .... ON
[ ]  Hand-Held Microphone .... CHECK
[ ]  Frequency .... SWITCH
[ ]  If IFR (or VFR in Class B, C, D airspace): Transponder .... 7600
NOTE: If failure occurs in VFR conditions, or VFR conditions are encountered after failure, continue flight under VFR and land as soon as practicable.
VFR LANDING AT A CONTROLLED FIELD:
[ ]  Remain outside or above Class D airspace until traffic flow determined.
[ ]  Transmit intentions "in the blind" advising tower of aircraft type, position, altitude, and intention to land.
[ ]  Enter pattern, report position "in the blind", and watch for light signals from tower.
NOTE: If failure occurs in IFR conditions, continue flight according to the following:
ROUTE TO FLY (IN ORDER): (AVE. F)
[ ]  A – Assigned
[ ]  V – Vectored
[ ]  E – Expected
[ ]  F – Filed
ALTITUDE (HIGHEST OF FOR THE ROUTE SEGMENT BEING FLOWN): (MEA)
[ ]  M – Minimum IFR Altitude
[ ]  E – Expected as Advised by ATC
[ ]  A – Assigned by ATC
DESCENT FOR APPROACH:
[ ]  From enroute altitude upon reaching the IAF but not before:
[ ]  Expect-further-clearance time (if given)
[ ]  ETA as calculated from filed ETE
NOTE: ATC LIGHT SIGNALS

ABORT  [EMERGENCY]
[ ]  Throttle .... IDLE
[ ]  Brakes .... AS REQUIRED

ENGINE FAILURE IMMEDIATELY AFTER TAKEOFF  [EMERGENCY]
[ ]  Airspeed [MEMORY] .... 80 MPH (flaps UP)
[ ]  Mixture [MEMORY] .... FULL LEAN
[ ]  Fuel Selector [MEMORY] .... OFF
[ ]  Flaps [MEMORY] .... DOWN (70 MPH glide)
[ ]  Master & Mags [MEMORY] .... OFF

COMPLETE ENGINE FAILURE DURING FLIGHT  [EMERGENCY]
[ ]  Airspeed [MEMORY] .... 80 MPH (flaps UP)   (Glide Ratio = 1.5 SM/1,000’ AGL)
IF AIRSTART WARRANTED:
[ ]  Carb Heat .... ON
[ ]  Mixture .... RICH
[ ]  Fuel Selector .... BOTH
[ ]  Primer .... IN & LOCKED
[ ]  Mags .... CHECK ALL
[ ]  Master .... ON

FORCED LANDING  [EMERGENCY]
[ ]  Airspeed [MEMORY] .... 80 MPH (flaps UP)
[ ]  Squawk [MEMORY] .... 7700
[ ]  Emergency [MEMORY] .... DECLARE
[ ]  ELT [MEMORY] .... ON
[ ]  Mixture [MEMORY] .... FULL LEAN
[ ]  Fuel Selector [MEMORY] .... OFF
[ ]  Seatbelt/Harness [MEMORY] .... FASTENED
[ ]  Flaps [MEMORY] .... AS REQUIRED (70 MPH with flaps full)
[ ]  Master & Mags [MEMORY] .... OFF
[ ]  Doors [MEMORY] .... UNLATCH

ENGINE ROUGHNESS  [EMERGENCY]
IF OVER 5,000’ MSL:
[ ]  Vapor In Fuel Tank .... EXECUTE
IF 5,000’ MSL OR BELOW, OR VAPOR IN FUEL TANK PROCEDURE DOESN’T CORRECT:
[ ]  Carb Heat .... ON
IF ROUGHNESS CONTINUES AFTER 1 MIN:
[ ]  Carb Heat .... OFF
[ ]  Mixture .... ADJUST FOR MAX SMOOTHNESS
[ ]  Fuel Selector .... BOTH
[ ]  Primer .... IN & LOCKED
[ ]  Engine Gauges .... CHECK
[ ]  Mags .... L then R then BOTH
[ ]  Mags .... SMOOTHEST SETTING
[ ]  Power .... REDUCE
[ ]  Mixture .... FULL RICH
[ ]  LAND AT NEAREST AIRPORT .... EXECUTE

VAPOR IN FUEL TANK (above 5,000 MSL)  [EMERGENCY]
DURING OPERATION ON A SINGLE TANK:
[ ]  Fuel Selector .... SWITCH TO OPPOSITE TANK
DURING OPERATION ON BOTH TANKS:
[ ]  Fuel Selector .... SWITCH TO A SINGLE TANK FOR 60 SECONDS
[ ]  Fuel Selector .... SWITCH TO OPPOSITE TANK

HIGH OIL TEMPERATURE  [EMERGENCY]
[ ]  Power .... REDUCE
[ ]  Mixture .... RICH
[ ]  Airspeed .... INCREASE
IF HIGH TEMP PERSISTS:
[ ]  LAND AT NEAREST AIRPORT .... EXECUTE

LOSS OF OIL PRESSURE  [EMERGENCY]
[ ]  Oil Temp .... CHECK
[ ]  Power .... REDUCE
IF OIL TEMP SHOWS RISE, ENGINE FAILURE IMMINENT:
[ ]  Forced Landing .... EXECUTE
IF OIL TEMP DOES NOT SHOW RISE:
[ ]  LAND AT NEAREST AIRPORT .... EXECUTE

ENGINE FIRE ON GROUND  [EMERGENCY]
[ ]  Mixture [MEMORY] .... FULL LEAN
[ ]  Fuel Selector [MEMORY] .... OFF
[ ]  Mags [MEMORY] .... OFF
[ ]  Master [MEMORY] .... OFF

ENGINE FIRE IN FLIGHT  [EMERGENCY]
[ ]  Mixture [MEMORY] .... FULL LEAN
[ ]  Fuel Selector [MEMORY] .... OFF
[ ]  Master & Mags [MEMORY] .... OFF
[ ]  Cabin Heat & Air [MEMORY] .... OFF
[ ]  Airspeed [MEMORY] .... 105 MPH
[ ]  Forced Landing [MEMORY] .... EXECUTE

ELECTRICAL FIRE  [EMERGENCY]
[ ]  Master [MEMORY] .... OFF

WING FIRE  [EMERGENCY]
[ ]  Landing/Taxi Lights .... OFF
[ ]  Navigation Lights .... OFF
[ ]  Strobe Lights .... OFF
[ ]  Pitot Heat .... OFF
[ ]  Sideslip .... AS REQUIRED
[ ]  Forced Landing .... EXECUTE

SMOKE AND FUMES IN COCKPIT  [EMERGENCY]
[ ]  Cabin Heat Knob .... IN
[ ]  Cabin Air Knob .... IN
[ ]  Upper Air Vents .... OPEN
[ ]  Pilot’s Window .... AS REQUIRED (below 100 MPH)

HIGH AMMETER READING (more than 2 needle widths positive deflection)  [EMERGENCY]
[ ]  Master .... OFF

NEGATIVE AMMETER READING  [EMERGENCY]
[ ]  Electrical Load .... REDUCE

VACUUM SYSTEM FAILURE  [EMERGENCY]
IF VMC:
[ ]  Attitude Indicator & Heading Indicator .... COVER
[ ]  Maintain VMC .... EXECUTE
IF IMC:
[ ]  Attitude Indicator & Heading Indicator .... COVER
[ ]  Fly using Turn-and-Slip Indicator, Altimeter, and Airspeed Indicator
[ ]  Declare EMERGENCY .... EXECUTE

INOPERATIVE TRIM  [EMERGENCY]
[ ]  Flaps .... AS REQUIRED
[ ]  Power .... AS REQUIRED

FLAP MALFUNCTION  [EMERGENCY]
[ ]  Circuit Breaker .... CHECK / RESET
IF BREAKER POPS AGAIN:
[ ]  Flaps .... LEAVE WHERE SET

STRUCTURAL ICING  [EMERGENCY]
[ ]  Pitot Heat .... ON
[ ]  Carb Heat .... ON
[ ]  Throttle .... MAX RPM
[ ]  Mixture .... BEST POWER
[ ]  Cabin Heat .... MAX DEFROST
[ ]  EXIT ICING CONDITIONS .... EXECUTE
IF LANDING WITH STRUCTURAL ICING:
[ ]  Flaps .... LEAVE UP

DOOR OR WINDOW OPENING IN FLIGHT  [EMERGENCY]
[ ]  FLY THE AIRPLANE [MEMORY] .... EXECUTE
IF WINDOW:
[ ]  Window .... CLOSE / LOCK
IF DOOR:
[ ]  LAND AS SOON AS PRACTICABLE .... EXECUTE

LANDING WITH A FLAT MAIN TIRE  [EMERGENCY]
[ ]  Approach .... NORMAL
[ ]  Flaps .... 30°
[ ]  Touchdown .... GOOD TIRE FIRST
[ ]  Hold airplane off flat tire as long as possible
[ ]  Maintain directional control using good-tire brake

LANDING WITH A FLAT NOSE TIRE  [EMERGENCY]
[ ]  Approach .... NORMAL
[ ]  Flaps .... AS REQUIRED
[ ]  Touchdown .... ON MAINS
[ ]  Hold nosewheel off ground as long as possible
[ ]  When nosewheel touches down .... FULL UP ELEVATOR

SPIN RECOVERY  [EMERGENCY]
[ ]  Power [MEMORY] .... Idle
[ ]  Ailerons [MEMORY] .... Neutral
[ ]  Rudder [MEMORY] .... Full opposite rotation direction
[ ]  Yoke [MEMORY] .... Full forward with neutral ailerons
[ ]  Rudder [MEMORY] .... Neutral when rotation stops
[ ]  Yoke [MEMORY] .... Pull smoothly from dive

INITIAL
[ ]  Wx & Density Alt
[ ]  Weight & Balance
[ ]  Performance Req
[ ]  Flight Plan - File
[ ]  Papers - A.R.O.W.
[ ]  Control Lock
[ ]  Fuel - Both
[ ]  Master - On
[ ]  Flaps - Extend
[ ]  Pitot Heat - Test
[ ]  Lights - Int/Ext
[ ]  Stall Indicator - Test
[ ]  Fuel Gauges - True
[ ]  Master - Off
[ ]  Fuel Strainer

EXTERIOR
[ ]  Fuel Quantity
[ ]  Fuel Quality
[ ]  Caps/Drains/Vents
[ ]  Engine/Oil
[ ]  Prop/Air Intake
[ ]  Exhaust System
[ ]  Surfaces & Controls
[ ]  Pitot & Static Ports
[ ]  Gear/Tires/Brakes
[ ]  Antennas
[ ]  Ties/Chocks
[ ]  Baggage Door
[ ]  Final Walk Around

INTERIOR
[ ]  Passenger Brief
[ ]  Hobbs Time
[ ]  Circuit Breakers
[ ]  Brakes - Pedal Test

START
[ ]  Seat Track/Back - Lock
[ ]  Avionics - Off
[ ]  Carb Heat - Off
[ ]  Beacon - On
[ ]  Nav Lights - As Req
[ ]  Mixture - Full Rich
[ ]  Throttle - Slight
[ ]  Prime - As Req
[ ]  Brakes
[ ]  Prop - Clear
[ ]  Master - On
[ ]  Mags - Start
[ ]  1,000 RPM
[ ]  Ammeter
[ ]  Oil Pressure
[ ]  Mixture - Lean

PRE-TAXI/TAXI
[ ]  Seat Belts/Harness
[ ]  Flaps - Up
[ ]  Heat/Vent
[ ]  Avionics - On/Set
[ ]  Transponder - Stby
[ ]  ATIS/AWOS
[ ]  Altimeter - Set
[ ]  Taxi Light - As Req
[ ]  Brakes - Test
[ ]  Attitude Indic - Test
[ ]  Turn & Slip - Test
[ ]  H.I./Compass - Test

RUN-UP
[ ]  Brakes - Set
[ ]  Fuel - Both
[ ]  Trim - Takeoff
[ ]  Flight Controls
[ ]  Instruments
[ ]  Mixture - Best Power
[ ]  Primer - In & Locked
[ ]  1600 RPM
[ ]  Mags (R&L) - Test
[ ]  Carb Heat - Test
[ ]  Vacuum
[ ]  Amps
[ ]  Oil Pressure
[ ]  Idle - Check Closed
[ ]  Mixture - Lean

TAKEOFF
[ ]  Flaps - 0-10°
[ ]  Carb Heat - Off
[ ]  Pitot Heat - As Req
[ ]  H.I. to Compass
[ ]  Doors/Window
[ ]  Takeoff Brief

TAKING RUNWAY
(LIGHTS, CAMERA, ACTION)
[ ]  Strobes - On
[ ]  Landing Light - On
[ ]  Transponder - Altitude
[ ]  Mixture - Best Power

CLIMB
[ ]  80-90 MPH
[ ]  Flaps - Up
[ ]  Power
[ ]  Mixture
[ ]  Instruments
[ ]  Landing Light - Off

CRUISE
[ ]  Power
[ ]  Mixture
[ ]  Instruments
[ ]  Fuel Selector - As Req
[ ]  H.I. To Compass

APPROACH
[ ]  Mixture - Richen
[ ]  Fuel - Both
[ ]  Carb Heat - As Req
[ ]  ATIS/AWOS
[ ]  Altimeter - Set
[ ]  Instruments
[ ]  H.I. To Compass
[ ]  Landing Light - On
[ ]  Seatbelt/Harness

LANDING
[ ]  Fuel - Both
[ ]  Mixture - Best Power
[ ]  Carb Heat - On
[ ]  Flaps - As Req

AFTER LANDING
[ ]  Flaps - Up
[ ]  Carb Heat - Off
[ ]  Mixture - Lean
[ ]  Strobes - Off
[ ]  Landing Light - Off
[ ]  Taxi Light - As Req
[ ]  Pitot Heat - Off
[ ]  Trim - Takeoff
[ ]  Transponder - Stby

SHUTDOWN
[ ]  Avionics - Off
[ ]  Fuel - Right
[ ]  Mags - Ground Check
[ ]  Mixture - Full Lean
[ ]  Mags - Off
[ ]  Master - Off
[ ]  Lights - Off

SECURING
[ ]  Hobbs/Tach Time
[ ]  Control Lock
[ ]  Chocks
[ ]  Tie Downs
[ ]  Baggage Door
[ ]  Cabin Doors/Window

AIRSPEEDS MPH IAS
[ ]  VS0   38
[ ]  VS1   44
[ ]  VR    60
[ ]  VX    66
[ ]  Short/Soft Final (40°) 70
[ ]  Normal Final (30°)     75
[ ]  VY    80
[ ]  Vmax Glide  80
[ ]  Final (0°)  80
[ ]  Base (20°)  80
[ ]  Past Abeam (10°) 90
[ ]  Cruise Climb     90
[ ]  VFE   100
[ ]  Downwind    100
[ ]  VA    122
[ ]  VNO   140
[ ]  VNE   174

DATA
[ ]  Engine: Continental O-300-D 145 HP
[ ]  Max T.O. Weight: 2300 #
[ ]  Max Bag Area:    120 #
[ ]  Fuel: 100LL (Blue)
[ ]  Usable Fuel:     36 Gal
[ ]  Oil Capacity:    8 Qts (Min 6)
[ ]  Electrical: 12-14 V 60 Amp
[ ]  Nose Tire:  26 PSI
[ ]  Main Tire:  24 PSI
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