Cessna 172L Skyhawk — c172l_abbreviated_checklist_millstone_valley
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

BEFORE STARTING ENGINE
[ ]  Exterior Preflight .... COMPLETE
[ ]  Tach/Hobbs Meter .... RECORD
[ ]  Seats, Belts, Harnesses .... ADJUST & LOCKED
[ ]  Fuel Shutoff Valve .... ON BOTH
[ ]  Radios & Electrical Equipment .... OFF
[ ]  Brakes .... TEST & SET

STARTING ENGINE
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... COLD
[ ]  Master Switch .... ON
[ ]  Prime .... AS REQUIRED
[ ]  Throttle .... OPEN ¼ INCH
[ ]  Propeller Area .... CLEAR
[ ]  Ignition Switch .... START (release when engine starts)
[ ]  Oil Pressure .... CHECK

BEFORE TAKEOFF
[ ]  Cabin Doors .... LATCHED
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Elevator Trim .... TAKEOFF POSITION
[ ]  Fuel Shutoff Valve .... ON BOTH
[ ]  Brakes .... SET
[ ]  Throttle .... 1700 RPM
[ ]  Magnetos .... CHECK — 125 MAX DROP / 50 MAX DIFF
[ ]  Carburetor Heat .... CHECK FOR RPM DROP
[ ]  Engine Instruments and Ammeter .... CHECK
[ ]  Suction Gauge .... CHECK
[ ]  Flight Instruments and Radio .... SET
[ ]  Throttle Friction Lock .... ADJUST
[ ]  Wing Flaps .... AS REQUIRED

TAKE-OFF
NORMAL TAKEOFF
[ ]  Wing Flaps .... UP (0)
[ ]  Carburetor Heat .... COLD
[ ]  Throttle .... FULL OPEN
[ ]  Elevator Control .... LIFT NOSE WHEEL AT 65 MPH
[ ]  Climb Speed .... 80 - 90 MPH
MAXIMUM PERFORMANCE TAKEOFF
[ ]  Wing Flaps .... 10 DEGREES
[ ]  Carburetor Heat .... COLD
[ ]  Brakes .... HOLD
[ ]  Throttle .... FULL OPEN
[ ]  Brakes .... RELEASE
[ ]  Elevator Control .... SLIGHTLY TAIL LOW
[ ]  Climb Speed .... 68 MPH (with obstacles ahead)

ENROUTE CLIMB
[ ]  Airspeed .... 80 – 100 MPH
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... RICH (Unless engine is rough)

CRUISE
[ ]  Power .... 2200 to 2500 (No more than 75%)
[ ]  Elevator Trim .... ADJUST
[ ]  Mixture .... RICH BELOW 3000

BEFORE LANDING
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON (apply before closing throttle)
[ ]  Airspeed .... 70-80 MPH (flaps up)
[ ]  Wing Flaps .... AS DESIRED (below 100 MPH)
[ ]  Airspeed .... 60-70 MPH (flaps down)

BALKED LANDING  [ABNORMAL]
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... COLD
[ ]  Wing Flaps .... RETRACT TO 20
[ ]  Airspeed .... 84 MPH
[ ]  Wing Flaps .... RETRACT (slowly)

NORMAL LANDING
[ ]  Touchdown .... MAIN WHEELS FIRST
[ ]  Landing Roll .... LOWER NOSE WHEEL GENTLY
[ ]  Braking .... MINIMUM REQUIRED

AFTER LANDING
[ ]  Wing Flaps .... UP
[ ]  Carburetor Heat .... COLD
[ ]  Unnecessary Equipment .... OFF

SECURING AIRCRAFT
[ ]  Parking Brake .... SET (Normally Not Used)
[ ]  Radios, Electrical Equipment .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
[ ]  Tach/Hobbs Meter .... RECORD

C172L Airspeeds (MPH Indicated)
[ ]  Vr .... 65
[ ]  Vx .... 68
[ ]  Vy .... 84
[ ]  Va .... 111
[ ]  Vs .... 54
[ ]  Vso .... 47
[ ]  Vfe .... 97
[ ]  Vno .... 147
[ ]  Vne .... 184
[ ]  Best Glide .... 75
[ ]  Demonstrated X-Wind .... 15 Knots
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