Cessna 172N _ 172M Skyhawk — jochman-clc172
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

ENGINE FAILURE DURING TAKEOFF  [EMERGENCY]
[ ]  Throttle .... IDLE
[ ]  Brakes .... APPLY
[ ]  Wing Flaps .... RETRACT
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF

ENGINE FAILURE AFTER TAKEOFF  [EMERGENCY]
[ ]  Airspeed (flaps UP) .... 65 KIAS
[ ]  Airspeed (flaps DOWN) .... 60 KIAS
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Wing Flaps .... AS REQUIRED
[ ]  Master Switch .... OFF

ENGINE FAILURE DURING FLIGHT  [EMERGENCY]
[ ]  Airspeed .... 65 KIAS
[ ]  Carburetor Heat .... ON
[ ]  Fuel Selector Valve .... BOTH
[ ]  Mixture .... RICH
[ ]  Ignition Switch .... BOTH or START
[ ]  Primer .... IN & LOCKED

EMERGENCY LANDING  [EMERGENCY]
[ ]  Airspeed (flaps UP) .... 65 KIAS
[ ]  Airspeed (flaps DOWN) .... 60 KIAS
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Wing Flaps .... AS REQUIRED
[ ]  Master Switch .... OFF
[ ]  Doors .... UNLATCH PRIOR TO TOUCHDOWN
[ ]  Touchdown .... SLIGHTLY TAIL LOW
[ ]  Brakes .... APPLY HEAVILY

PRECAUTIONARY LANDING  [EMERGENCY]
[ ]  Wing Flaps .... 20(
[ ]  Airspeed .... 60 KIAS
[ ]  Select field .... SUITABLE
[ ]  Avionics Power Switch .... OFF
[ ]  Electrical Switches .... OFF
[ ]  Wing Flaps (on final approach) .... 30(
[ ]  Airspeed .... 60 KIAS
[ ]  Master Switch .... OFF
[ ]  Doors .... UNLATCH PRIOR TO TOUCHDOWN
[ ]  Touchdown .... SLIGHTLY TAIL LOW
[ ]  Ignition Switch .... OFF
[ ]  Brakes .... APPLY HEAVILY

CABIN
[ ]  Pilot’s Operating Handbook .... AVAILABLE
[ ]  Aircraft Documents .... AVAILABLE
[ ]  Control Wheel Lock .... REMOVE
[ ]  Ignition Switch .... OFF
[ ]  Avionics Power Switch .... OFF
[ ]  Master Switch .... ON
[ ]  Fuel Quanity Indicators .... CHECK QUANTITY
[ ]  Flaps .... DOWN
[ ]  Master Switch .... OFF

EMPENNAGE
[ ]  Rudder Gust Lock .... REMOVE
[ ]  Tail Tie-Down .... DISCONNECT
[ ]  Control Surfaces .... CHECK FREE

RIGHT WING
[ ]  Aileron .... CHECK FREE
[ ]  Wing Tie-Down .... DISCONNECT
[ ]  Main Wheel Tire .... CHECK
[ ]  Fuel Tank Sump .... SAMPLE
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Filler Cap .... SECURE

NOSE
[ ]  Engine Oil Level .... CHECK
[ ]  Fuel Strainer .... DRAIN
[ ]  Propeller and Spinner .... CHECK
[ ]  Landing Light .... CHECK
[ ]  Carburetor Air Filter .... CHECK
[ ]  Nose Wheel Strut and Tire .... CHECK
[ ]  Nose Tie-Down .... DISCONNECT
[ ]  Static Source Opening .... CHECK

LEFT WING
[ ]  Main Wheel Tire .... CHECK
[ ]  Fuel Tank Sump .... SAMPLE
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Filler Cap .... SECURE
[ ]  Pitot Tube Cover .... REMOVE
[ ]  Fuel Tank Vent Opening .... CHECK
[ ]  Stall Warning Opening .... CHECK
[ ]  Wing Tie-Down .... DISCONNECT
[ ]  Aileron .... CHECK FREE

BEFORE STARTING ENGINE
[ ]  Preflight Inspection .... COMPLETE
[ ]  Seats, Belts, Shoulder Harnesses .... ADJUST & LOCK
[ ]  Fuel Selector Valve .... BOTH
[ ]  Avionics Power Switch .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Brakes .... TEST & SET
[ ]  Circuit Breakers .... CHECK IN

STARTING ENGINE
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... COLD
[ ]  Master Switch .... ON
[ ]  Prime .... AS REQUIRED
[ ]  Throttle .... OPEN ¼ INCH
[ ]  Propeller Area .... CLEAR
[ ]  Ignition Switch .... START
[ ]  Throttle .... 1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Flashing Beacon, Nav. Lights .... ON
[ ]  Avionics Power Switch .... ON
[ ]  Radios .... ON
[ ]  Transponder .... STANDBY

BEFORE TAXI
[ ]  Wing Flaps .... UP
[ ]  Parking Brake .... RELEASE
[ ]  Brakes .... TEST
[ ]  Area .... CLEAR

BEFORE TAKEOFF
[ ]  Parking Brake .... SET
[ ]  Cabin Doors and Windows .... CLOSED & LOCKED
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Flight Instruments .... SET
[ ]  Fuel Selector Valve .... BOTH
[ ]  Mixture (Below 3000’) .... RICH
[ ]  Elevator Trim .... TAKEOFF
[ ]  Rudder Trim (if installed) .... TAKEOFF
[ ]  Throttle .... 1700 RPM
[ ]  Magnetos .... CHECK
[ ]  Carburetor Heat .... CHECK
[ ]  Engine Instruments .... CHECK
[ ]  Ammeter .... CHECK
[ ]  Suction Guage .... CHECK
[ ]  Throttle .... 1000 RPM
[ ]  Radios .... SET
[ ]  Transponder .... ON-ALT

NORMAL TAKEOFF
[ ]  Wing Flaps .... 0( - 10(
[ ]  Carburetor Heat .... COLD
[ ]  Throttle .... FULL OPEN
[ ]  Elevator Control .... LIFT NOSE AT 55 KIAS
[ ]  Climb Speed .... BEST RATE

SHORT FIELD TAKEOFF
[ ]  Wing Flaps .... 10(
[ ]  Carburetor Heat .... COLD
[ ]  Brakes .... APPLY
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... LEAN above 3000’, RICH below 3000’
[ ]  Brakes .... RELEASE
[ ]  Elevator Control .... SLIGHTLY TAIL LOW
[ ]  Climb Speed (Until Obstacles Cleared) .... BEST ANGLE

ENROUTE CLIMB
[ ]  Airspeed .... BEST RATE or HIGHER
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... LEAN above 3000’, RICH below 3000’

CRUISE
[ ]  Power .... 75% or LESS
[ ]  Elevator Trim .... ADJUST
[ ]  Rudder Trim (if installed) .... ADJUST
[ ]  Mixture .... LEAN

DESCENT
[ ]  Fuel Selector Valve .... BOTH
[ ]  Mixture .... ADJUST
[ ]  Power .... AS DESIRED
[ ]  Carburetor Heat .... FULL AS REQUIRED

BEFORE LANDING
[ ]  Seats, Belts, Shoulder Harnesses .... SECURE
[ ]  Fuel Selector Valve .... BOTH
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON

BALKED LANDING
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... COLD
[ ]  Wing Flaps (immediately) .... 20(
[ ]  Climb Speed .... BEST ANGLE
[ ]  Wing Flaps .... 10(
[ ]  Wing Flaps (after safe alt. and 60 KIAS) .... RETRACT

AFTER LANDING
[ ]  Wing Flaps .... UP
[ ]  Carburetor Heat .... COLD
[ ]  Transponder .... STANDBY

SECURING AIRPLANE
[ ]  Parking Brake .... SET
[ ]  Avionics Power Switch .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
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