Cessna 172N — Normal Procedures (independently worded)
NOT FOR FLIGHT — source fidelity: not_applicable | operational review: none | completeness: normal_only | 1 unresolved safety defect(s)
safety_defect: Contains no airspeeds, power settings, fuel quantities or other limitations. It cannot be used as a working checklist as it stands.
content_gap: Normal procedures only. No emergency or abnormal sections.
content_gap: 172N airframes differ in equipment. Verify each item exists on the specific aircraft before use.

Before Start
[ ]  Preflight inspection .... COMPLETE
[ ]  Seats and belts .... ADJUSTED AND SECURE
[ ]  Brakes .... TESTED AND HELD
[ ]  Electrical equipment .... OFF
[ ]  Fuel selector .... BOTH
[ ]  Radios and avionics .... OFF

Engine Start
[ ]  Mixture .... RICH
[ ]  Carburetor heat .... COLD
[ ]  Master switch .... ON
[ ]  Beacon .... ON
[ ]  Primer .... AS REQUIRED
[ ]  Throttle .... OPEN SLIGHTLY
[ ]  Call "CLEAR PROP" and confirm the propeller arc is clear
[ ]  Ignition switch .... START, RELEASE ON START
[ ]  Oil pressure .... IN GREEN WITHIN 30 SECONDS
CAUTION: If oil pressure does not reach the green arc, shut the engine down and investigate before the next start attempt.
[ ]  Throttle .... SET IDLE RPM
[ ]  Ammeter .... CHARGING

Before Takeoff
[ ]  Parking brake .... SET
[ ]  Flight controls .... FREE AND CORRECT
[ ]  Flight instruments .... SET AND CROSS-CHECKED
[ ]  Altimeter .... SET TO FIELD SETTING
[ ]  Fuel selector .... BOTH
[ ]  Mixture .... RICH
[ ]  Elevator trim .... SET FOR TAKEOFF
[ ]  Throttle .... SET FOR RUN-UP
[ ]  Magnetos .... CHECK EACH, DROP AND DIFFERENTIAL WITHIN POH LIMITS
The permitted maximum drop and maximum difference between magnetos are POH figures for this aircraft and are not stated in this file.
[ ]  Carburetor heat .... CHECK FOR RPM DROP, THEN COLD
[ ]  Engine instruments .... IN RANGE
[ ]  Suction gauge .... IN RANGE
[ ]  Throttle .... IDLE, THEN CHECK IDLE RPM
[ ]  Flaps .... SET FOR TAKEOFF
[ ]  Doors and windows .... CLOSED AND LATCHED
[ ]  Lights .... AS REQUIRED
[ ]  Takeoff briefing .... COMPLETE
[ ]  Parking brake .... RELEASED

Cruise
[ ]  Power .... SET PER POH CRUISE TABLE
[ ]  Elevator trim .... ADJUSTED
[ ]  Mixture .... LEANED PER POH
[ ]  Engine instruments .... MONITORED
[ ]  Fuel selector and quantity .... CHECKED

Before Landing
[ ]  Seats and belts .... SECURE
[ ]  Fuel selector .... BOTH
[ ]  Mixture .... RICH
[ ]  Carburetor heat .... AS REQUIRED
[ ]  Landing light .... AS REQUIRED
[ ]  Flaps .... AS REQUIRED
[ ]  Approach speed .... SET PER POH

Go Around  [ABNORMAL]
[ ]  Throttle [MEMORY] .... FULL
[ ]  Carburetor heat [MEMORY] .... COLD
[ ]  Flaps [MEMORY] .... RETRACT PROGRESSIVELY
[ ]  Climb attitude and speed .... ESTABLISHED
[ ]  Trim .... ADJUSTED

Shutdown and Securing
[ ]  Parking brake .... SET
[ ]  Throttle .... IDLE
[ ]  Avionics and electrical equipment .... OFF
[ ]  Mixture .... IDLE CUTOFF
[ ]  Ignition switch .... OFF AND KEY REMOVED
[ ]  Master switch .... OFF
[ ]  Control lock and tiedowns .... INSTALLED

NOT FOR FLIGHT — source fidelity: not_applicable | operational review: none | completeness: normal_only | 1 unresolved safety defect(s)
Source: authored — no source document
Rights: original_expression CC-BY-4.0
Checklist hash: a507c8e9ba3192529dfdf11ad884e8fc7278e52e023fd1f6630396d9e9951a0b
Verify against the aircraft's own approved documentation before use.
