Cessna 172P Skyhawk — C172p-checklist_selkirk_college
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "ELECTRICAL FIRE IN FLIGHT" item count differs between passes (13 vs 12); verify nothing was dropped.
content_gap: Section "ELECTRICAL MALFUNCTION" item count differs between passes (5 vs 4); verify nothing was dropped.
content_gap: Section "ENGINE START" item count differs between passes (8 vs 7); verify nothing was dropped.
content_gap: Section "PRECAUTIONARY LANDING WITH POWER" item count differs between passes (18 vs 16); verify nothing was dropped.

PRE-START
[ ]  HOBBS .... NOTED
[ ]  PASSENGER BRIEFING .... COMPLETED (IF REQUIRED)
[ ]  DISPATCH LOG .... COMPLETED
[ ]  LOGS & DOCUMENTS .... ON BOARD & VALID
[ ]  SEATS & BELTS .... LOCKED & SECURE*
[ ]  CONTROLS .... FREE & CORRECT
[ ]  PARKING BRAKE .... SET
[ ]  CIRCUIT BREAKERS .... ALL IN
[ ]  ELECTRICS .... OFF
[ ]  RADIO MASTER .... OFF
[ ]  MASTER .... ON
[ ]  RADIO FAN .... ON
[ ]  BEACON .... ON
[ ]  LOW VOLTAGE LIGHT .... ON
[ ]  AMMETER .... CHECKED
[ ]  FUEL .... QUANTITY CHECKED, ON LEFT
[ ]  FLAPS .... UP

ENGINE START
[ ]  MIXTURE .... FULL RICH
[ ]  PRIMER .... PRIMED & LOCKED
[ ]  THROTTLE .... SET
[ ]  ENGINE (START) .... STARTED
[ ]  OIL PRESSURE .... NORMAL
[ ]  AMMETER .... CHECKED
[ ]  SUCTION .... CHECKED
NOTE: *BOTH PILOTS RESPOND

POST - START
[ ]  RADIO MASTER .... ON
[ ]  ELECTRICS .... ON (AS REQUIRED)
[ ]  ELT .... CHECKED
[ ]  INSTRUMENT PANEL .... PANEL CHECKED
[ ]  RADIOS .... RADIOS CHECKED
[ ]  FUEL SELECTOR .... QUANTITY CHECKED, ON RIGHT

TAXI
[ ]  BRAKES .... CHECKED
[ ]  INSTRUMENTS .... CHECKED

RUN - UP
[ ]  PARKING BRAKE .... SET
[ ]  THROTTLE .... 1000
[ ]  FUEL SELECTOR .... QUANTITY CHECKED, ON BOTH
[ ]  ENGINE GAUGES .... NORMAL
[ ]  THROTTLE .... 1700
[ ]  ENGINE GAUGES .... NORMAL
[ ]  SUCTION .... NORMAL
[ ]  MIXTURE .... CHECKED
[ ]  CARB HEAT .... CHECKED
[ ]  MAGNETOS .... CHECKED
[ ]  THROTTLE .... IDLE CHECKED, 1000, CARB HEAT COLD

PRE - TAKEOFF
[ ]  SEAT & BELTS .... LOCKED & SECURE*
[ ]  CONTROLS .... FREE
[ ]  TRIMS .... ____SET
[ ]  FUEL SELECTOR .... QUANTITY CHECKED, ON BOTH
[ ]  FLAPS .... SET FOR TAKEOFF
[ ]  ALTERNATE STATIC .... CHECKED & OFF
[ ]  MIXTURE .... FULL RICH
[ ]  THROTTLE TENSION .... SET
[ ]  CARB HEAT .... COLD
[ ]  CIRCUIT BREAKERS .... ALL IN
[ ]  PRIMER .... LOCKED
[ ]  ENGINE GAUGES .... NORMAL
[ ]  ALTIMETER .... ____SET
[ ]  CLOCK .... ______CHECKED
[ ]  HEADING INDICATOR .... CHECKED & SET
[ ]  IFR CLEARANCE .... CLEARANCE REVIEWED
[ ]  CREW BRIEFING .... BRIEFING COMPLETED
[ ]  DOORS & WINDOWS .... CLOSED & LOCKED*
[ ]  PITOT HEAT .... ON (IF REQUIRED)
[ ]  LANDING LIGHT .... ON (IF REQUIRED)
[ ]  STROBES .... ON (IF EQUIPPED)
[ ]  PULSE LIGHT .... ON
[ ]  TRANSPONDER .... ON ALT_______
[ ]  TIME .... NOTED
[ ]  HEADING INDICATOR .... CHECKED ON RUNWAY

POST - TAKEOFF
[ ]  FLAPS .... UP
[ ]  ENGINE GAUGES .... NORMAL
[ ]  LANDING LIGHT .... OFF

PRE - LANDING
[ ]  SEATS & BELTS .... LOCKED & SECURE*
[ ]  BRAKES .... CHECKED & OFF
[ ]  FUEL SELECTOR .... QUANTITY CHECKED, ON BOTH
[ ]  MIXTURE .... FULL RICH
[ ]  CARB HEAT .... HOT
[ ]  ELECTRICS .... ON (AS REQUIRED)
[ ]  MAGNETOS .... ON BOTH
[ ]  LANDING LIGHT .... ON (IF REQUIRED)

POST - LANDING
[ ]  FLAPS .... UP
[ ]  CARB HEAT .... COLD
[ ]  TRANSPONDER .... STANDBY
[ ]  MINIMUM ELECTRICS .... SET

SHUT - DOWN
[ ]  PARKING BRAKE .... SET
[ ]  THROTTLE .... 1000
[ ]  ELT .... CHECKED
[ ]  ELECTRICS .... OFF
[ ]  MASTER .... OFF
[ ]  THROTTLE .... IDLE
[ ]  LIVE MAG .... CHECKED
[ ]  MIXTURE .... IDLE CUT OFF
[ ]  MAGNETOS .... OFF
[ ]  FUEL SELECTOR .... ON LEFT

EMERGENCY PROCEDURES  [EMERGENCY]
NOTE: * ITEMS MUST BE PERFORMED BY MEMORY

ENGINE FAILURE DURING TAKEOFF RUN  [EMERGENCY]
[ ]  THROTTLE [MEMORY] .... IDLE
[ ]  BRAKES [MEMORY] .... APPLY
[ ]  WING FLAPS [MEMORY] .... RETRACT
[ ]  MIXTURE [MEMORY] .... IDLE CUT OFF
[ ]  IGNITION SWITCH [MEMORY] .... OFF
[ ]  MASTER SWITCH [MEMORY] .... OFF

ENGINE FAILURE IMMEDIATELY AFTER TAKEOFF  [EMERGENCY]
[ ]  AIRSPEED [MEMORY] .... 65K (FLAPS UP) 60K (FLAPS DOWN)
[ ]  MIXTURE [MEMORY] .... IDLE CUT OFF
[ ]  FUEL SELECTOR VALVE [MEMORY] .... OFF
[ ]  IGNITION SWITCH [MEMORY] .... OFF
[ ]  WING FLAPS [MEMORY] .... AS REQUIRED
[ ]  MASTER SWITCH [MEMORY] .... OFF

ENGINE FAILURE IN FLIGHT  [EMERGENCY]
[ ]  AIRSPEED [MEMORY] .... 65KTS
[ ]  CARBURETOR HEAT [MEMORY] .... HOT
[ ]  FUEL SELECTOR [MEMORY] .... BOTH
[ ]  MIXTURE [MEMORY] .... RICH
[ ]  IGNITION SWITCH [MEMORY] .... BOTH (OR START)
[ ]  PRIMER [MEMORY] .... IN AND LOCKED
[ ]  GLIDE AIRSPEED .... 65K FLAPS UP 60K FLAPS DOWN
[ ]  RADIO .... MAYDAY CALLED
[ ]  PASSENGERS .... BRIEFED FOR ROUGH LANDING
[ ]  EVACUATION NOTICE .... ISSUED
[ ]  CABIN .... SECURED
[ ]  RESTART .... UNSUCCESSFUL
NOTE: IF RESTART IS UNSUCCESSFUL CONTINUE WITH CHECKLIST BELOW
[ ]  MIXTURE .... IDLE CUT OFF
[ ]  FUEL SELECTOR VALVE .... OFF
[ ]  IGNITION SWITCH .... OFF
[ ]  WING FLAPS .... AS REQUIRED
[ ]  MASTER SWITCH .... OFF
[ ]  DOORS .... UNLATCH BEFORE LANDING
[ ]  BRAKES .... APPLY HEAVILY

PRECAUTIONARY LANDING WITH POWER  [EMERGENCY]
NOTE: *ITEMS MUST BE PERFORMED BY MEMORY
LANDING OFF AERODROME
[ ]  WING FLAPS .... 20 DEGREES
[ ]  AIRSPEED .... 60K OR HIGHER IF REQUIRED
[ ]  RADIO CALL .... CONTACT FSS, ATC OR OTHER AIRCRAFT. REPORT POSITION, CONDITIONS AND INTENTIONS.
[ ]  PASSENGERS .... BRIEF FOR LANDING
[ ]  CABIN .... SECURE FOR LANDING
[ ]  SELECTED FIELD .... FLY OVER NOTING TERRAIN AND OBSTRUCTIONS
[ ]  OVERSHOOT .... RETRACT FLAPS UPON REACHING SAFE ALTITUDE AND AIRSPEED
[ ]  RADIO MASTER .... OFF
[ ]  ELECTRICS .... OFF
[ ]  FLAPS .... 30 ON FINAL
[ ]  AIRSPEED .... 60 KIAS
[ ]  MASTER SWITCH .... OFF
[ ]  DOORS .... UNLATCH PRIOR TO LANDING
[ ]  TOUCHDOWN .... SLIGHTLY TAIL LOW
[ ]  IGNITION SWITCH .... OFF
[ ]  BRAKES .... APPLY AS REQUIRED

ELECTRICAL FIRE IN FLIGHT  [EMERGENCY]
NOTE: * ITEMS MUST BE PERFORMED BY MEMORY
[ ]  MASTER [MEMORY] .... OFF
[ ]  RADIO MASTER [MEMORY] .... OFF
[ ]  ELECTRICAL SWITCHES [MEMORY] .... OFF
[ ]  VENTS/CABIN AIR/HEAT .... CLOSED
[ ]  FIRE EXTINGUISHER .... ACTIVATE IF REQUIRED
WARNING: AFTER DISCHARGING A FIRE EXTINGUISHER VENTILATE THE CABIN
NOTE: IF ELECTRIC POWER IS NOT REQUIRED - LEAVE MASTER OFF AND LAND AT A SUITABLE AERODROME.
[ ]  MASTER .... ON
[ ]  CIRCUIT BREAKERS .... CHECK-DO NOT RESET
[ ]  RADIO SWITCHES .... OFF
[ ]  RADIO MASTER .... ON
[ ]  RADIO AND ELECTRICAL SWITCHES .... ON ONE AT A TIME, WITH DELAY UNTIL SHORT IS LOCALIZED

CABIN FIRE  [EMERGENCY]
[ ]  MASTER [MEMORY] .... OFF
[ ]  VENTS/CABIN AIR/HEAT [MEMORY] .... CLOSED
[ ]  FIRE EXTINGUISHER .... ACTIVATE, IF REQUIRED
WARNING: AFTER DISCHARGING A FIRE EXTINGUISHER VENTILATE THE CABIN
[ ]  LAND ASAP .... INSPECT FOR DAMAGE

WING FIRE  [EMERGENCY]
[ ]  NAVIGATION LIGHTS .... OFF
[ ]  PITOT HEAT .... OFF
[ ]  STROBES .... OFF
NOTE: PERFORM A SIDESLIP TO KEEP FLAMES AWAY FROM THE FUEL TANK
[ ]  LAND .... AS SOON AS POSSIBLE
WARNING: USE FLAPS ONLY AS REQUIRED FOR LANDING

ELECTRICAL MALFUNCTION  [ABNORMAL]
NOTE: * ITEMS MUST BE PERFORMED BY MEMORY
[ ]  ALTERNATOR [MEMORY] .... OFF
[ ]  ALTERNATOR CIRCUIT BREAKER .... PULL
[ ]  NONESSENTIAL ELECTRIC EQUIPMENT .... OFF
[ ]  FLIGHT .... END AS SOON AS PRACTICAL

LOW VOLTAGE LIGHT ILLUMINATES DURING FLIGHT  [ABNORMAL]
[ ]  RADIO MASTER .... OFF
[ ]  ALTERNATOR CIRCUIT BREAKER .... CHECK IN
[ ]  MASTER .... OFF-BOTH SIDES
[ ]  MASTER .... ON-AFTER 3 SECONDS
[ ]  LOW VOLTAGE LIGHT .... CHECK OFF
[ ]  RADIO MASTER .... ON
NOTE: IF LOW-VOLTAGE LIGHT ILLUMINATES AGAIN
[ ]  ALTERNATOR .... OFF
[ ]  NONESSENTIAL ELECTRICS .... OFF
[ ]  FLIGHT .... END AS SOON AS PRACTICAL

FIRES  [EMERGENCY]
NOTE: *ITEMS MUST BE PERFORMED BY MEMORY

FIRE DURING START ON GROUND  [EMERGENCY]
[ ]  CRANKING [MEMORY] .... CONTINUE
IF ENGINE STARTS:
[ ]  POWER [MEMORY] .... 1700 RPM
[ ]  ENGINE .... SHUTDOWN AND INSPECT
IF ENGINE FAILS TO START:
[ ]  THROTTLE [MEMORY] .... FULL OPEN
[ ]  MIXTURE [MEMORY] .... IDLE CUT-OFF
[ ]  CRANKING [MEMORY] .... CONTINUE
[ ]  FIRE EXTINGUISHER .... OBTAIN
[ ]  MASTER .... OFF
[ ]  MAGNETOS .... OFF
[ ]  FUEL SELECTOR .... OFF
[ ]  PASSENGERS .... EVACUATE
[ ]  FIRE .... EXTINGUISH, IF SAFE
[ ]  FIRE DAMAGE .... INSPECT

ENGINE FIRE IN FLIGHT  [EMERGENCY]
[ ]  MIXTURE [MEMORY] .... IDLE CUT OFF
[ ]  FUEL SELECTOR VALVE [MEMORY] .... OFF
[ ]  MASTER [MEMORY] .... OFF
[ ]  CABIN HEAT AND AIR [MEMORY] .... OFF
[ ]  AIRSPEED [MEMORY] .... 100 KIAS SEE NOTE
NOTE: IF FIRE NOT EXTINGUISHED INCREASE GLIDE TO FIND AN INCOMBUSTIBLE MIXTURE
[ ]  FORCED LANDING [MEMORY] .... EXECUTE
NOTE: REFER TO ENGINE FAILURE IN FLIGHT ITEMS 7 - 19

DITCHING  [EMERGENCY]
[ ]  RADIO .... TRANSMIT MAYDAY
[ ]  TRANSPONDER .... SQUAWK 7700
[ ]  CABIN .... SECURE FOR ROUGH LANDING - JETTISON HEAVY OBJECTS
[ ]  PASSENGERS .... BRIEF FOR ROUGH LANDING
[ ]  PASSENGERS .... BRIEF ESCAPE PROCEDURE
NOTE: EVACUATE THROUGH CABIN DOORS- IF NECESSARY OPEN WINDOW AND FLOOD CABIN TO EQUALIZE PRESSURE SO DOORS CAN BE OPENED.
[ ]  APPROACH .... HIGH WINDS HEAVY SWELLS: INTO WIND; LIGHT WINDS HEAVY SWELLS: PARALLEL
[ ]  FLAPS .... 20 TO 30 DEGREES
NOTE: IF NO POWER IS AVAILABLE, APPROACH AT 65KIAS WITH FLAPS UP OR 60 KIAS WITH FLAPS 10 DEGREES
[ ]  CABIN DOOR .... UNLATCH
[ ]  TOUCHDOWN .... LEVEL ATTITUDE AT ESTABLISHED RATE OF DESCENT
[ ]  FACE .... CUSHION BEFORE TOUCHDOWN WITH FOLDED COAT
[ ]  AIRPLANE .... EVACUATE
[ ]  LIFE VESTS AND RAFT .... INFLATE
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