Cessna 172P Skyhawk — TFA_Cessna_172P_Checklist_2004-01
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Before Takeoff" item count differs between passes (19 vs 21); verify nothing was dropped.
content_gap: Section "Cruise" item count differs between passes (8 vs 11); verify nothing was dropped.
content_gap: Section "Preflight Inspection" item count differs between passes (56 vs 58); verify nothing was dropped.
content_gap: Section "Short Field Take Off" item count differs between passes (11 vs 12); verify nothing was dropped.

V Speed Review
[ ]  Max Cross Wind .... 15 KIAS
[ ]  Vso .... 33 KIAS
[ ]  Vs1 .... 44 KIAS
[ ]  Vx .... 60 KIAS
[ ]  Best Glide .... 65 KIAS
[ ]  Vy .... 76 KIAS
[ ]  Va .... 82-99 KIAS
[ ]  Vfe 20° & + .... 85 KIAS
[ ]  Vfe 10° .... 110 KIAS
[ ]  Vno .... 127 KIAS
[ ]  Vne .... 158 KIAS

Preflight Inspection
CABIN
[ ]  A.R.O.W.& Mtc. Docs. .... CHECK
[ ]  Hobbs Meter .... CHECK
[ ]  Control Lock .... REMOVE
[ ]  Ignition Switch .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Master (look prop is clear) .... ON
[ ]  Avionics Power .... ON/FAN/OFF
[ ]  Fuel Quantity Indicators .... CHECK
[ ]  Lights & Pitot Heat .... CHECK
[ ]  Flaps .... 30°
[ ]  Master Switch .... OFF
[ ]  Alternate Static .... OFF
[ ]  Fuel Selector Valve .... BOTH
[ ]  Baggage Door .... CHECK
EMPENNAGE
[ ]  Rudder Gust Lock .... REMOVE
[ ]  Fuselage .... CHECK
[ ]  Tail Tie Down .... UNTIE
[ ]  Elevator .... FREE & SECURE
[ ]  Rudder .... FREE & SECURE
[ ]  VOR Antennas .... CHECK
[ ]  Trim Tab .... CHECK
RIGHT WING
[ ]  Flap .... SECURE
[ ]  Aileron .... FREE & SECURE
[ ]  Skin/Tip/Lights .... CHECK
[ ]  Wing Tie Down .... UNTIE
[ ]  Main Wheel Tire .... INFLATED
[ ]  Brakes .... CHECK
[ ]  Fuel Tank Sump .... SAMPLE
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Filler Cap .... CHECK SECURE
NOSE
[ ]  Engine Oil .... 5-7 Qts. Min/Max (N63022 6-8 Qts. Min/Max)
[ ]  Fuel Strainer .... SAMPLE
[ ]  Belly Quick Drain .... SAMPLE (N52950 No Belly Quick Drain Avail.)
[ ]  Propeller & Spinner .... CHECK
[ ]  Air Intakes .... FREE & OPEN
[ ]  Carburetor Air Filter .... CLEAR
[ ]  Landing Light .... SECURE
[ ]  Nose Wheel & Strut .... CHECK
[ ]  Static Port .... OPEN
LEFT WING
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Filler Cap .... CHECK SECURE
[ ]  Main Wheel Tire .... INFLATED
[ ]  Brakes .... CHECK
[ ]  Fuel Tank Sump .... SAMPLE
[ ]  Pitot Tube & Drain .... FREE
[ ]  Stall Warning Opening .... CHECK
[ ]  Fuel Tank Vent .... OPEN
[ ]  Wing Tie Down .... UNTIE
[ ]  Aileron .... FREE & SECURE
[ ]  Flap .... SECURE
[ ]  Skin/Tip/Lights .... CHECK

Before Starting Engine
[ ]  Preflight .... COMPLETE
[ ]  Passenger Brief .... COMPLETE
[ ]  Seat/Seat Belts .... LOCKED
[ ]  Fuel Selector Valve .... BOTH
[ ]  Avionics Power .... OFF
[ ]  Circuit Breakers .... IN
[ ]  Electrical Equipment .... OFF
[ ]  Brakes .... SET & HOLD

Starting Engine
[ ]  Mixture .... RICH
[ ]  Throttle .... OPEN ¼ INCH
[ ]  Carburetor Heat .... COLD
[ ]  Prime .... AS REQ
[ ]  Beacon .... ON
[ ]  Master Switch .... ON
[ ]  Propeller Area .... CLEAR
[ ]  Ignition Switch .... START
[ ]  Throttle .... SMOOTH IDLE
[ ]  Oil Pressure .... CHECK
[ ]  Carburetor Heat .... AS REQ
[ ]  Flaps .... UP & VERIFIED
[ ]  Pitot Heat .... AS REQ
[ ]  Avionics Master / Avionics .... ON

Before Takeoff
[ ]  Brakes .... SET & HOLD
[ ]  Doors & Windows .... LOCKED
[ ]  Controls .... FREE & CORRECT
[ ]  Trim .... SET FOR TAKEOFF
[ ]  Flight Instr. .... SET & CHECK
[ ]  Fuel Selector Valve .... BOTH
[ ]  Mixture .... RICH
[ ]  Throttle .... 1700 RPM
[ ]  Mags .... RT/BOTH/LEFT/BOTH; Max 125 Drop & 50 Diff.
[ ]  Carb. Heat .... ON/CHECK/OFF
[ ]  Engine Instr. .... GREEN/NORM
[ ]  Ammeter/Alternator .... CHECK
[ ]  Suction Gauge .... CHECK
[ ]  Throttle .... SMOOTH IDLE
[ ]  Carburetor Heat .... AS REQ (FOR WX & RNWY COND.)
[ ]  Comm./Nav. Radios .... SET
[ ]  Strobe Lights (if installed) .... ON
[ ]  Throttle Lock .... ADJUST
[ ]  Flaps .... SET FOR TAKEOFF

Taking Runway
NOTE: MEMORY ITEMS – CALCAT
[ ]  Clearance .... RECEIVED T.O. or P.& H.
[ ]  Approach End .... CLEAR
[ ]  Lights .... ON
[ ]  Camera .... TRANSPONDER ALT
[ ]  Action .... D.G. TO RNWY HDG
[ ]  Time .... OFF TAKE

Normal Takeoff
[ ]  Flaps .... 0° - 10°
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF/COLD
[ ]  Airspeed .... ALIVE
[ ]  Eng. Instr. .... GREEN/NORM.
[ ]  Lift Nose Wheel .... 55 KIAS
[ ]  Climb Speed .... 70 – 80 KIAS

Soft Field Take Off
[ ]  Elevator Control .... FULL AFT
[ ]  Flaps .... 10°
[ ]  Taxi .... KEEP ROLLING
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF/COLD
[ ]  Airspeed .... ALIVE
[ ]  Eng. Instr. .... GREEN/NORM.
[ ]  Lift Off .... AS SOON AS PRACTICAL
[ ]  Accelerate In Ground Effect .... TO Vx OR Vy
[ ]  Flaps (Over Obstacle & Vy+) .... UP

Short Field Take Off
[ ]  Flaps .... 10°
[ ]  Brakes .... HOLD
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF/COLD
[ ]  Mixture .... RICH (above 3000’ Lean Max RPMs)
[ ]  Engine Instr. .... GREEN/NORM
[ ]  Brakes .... RELEASE
[ ]  Airspeed .... ALIVE
[ ]  Lift Nose .... APPROX. 55 KIAS
[ ]  Climb Speed .... 56 KIAS
[ ]  Over Obstacle .... ACCELERATE TO Vy & THEN FLAPS UP

Enroute Climb
[ ]  Airspeed .... 70 – 85 KIAS
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... RICH OR AS REQ.

Cruise
[ ]  Attitude .... ESTABLISH
[ ]  Power .... ADJUST 65% 2400 RPM (upon reaching desired airspeed)
[ ]  Trim .... ADJUST
[ ]  Carb Heat .... AS REQ (ON WHENEVER IN RAIN, SNOW, OR VISIBLE MOISTURE)
[ ]  Mixture .... LEAN AS REQ (50° Less Peak EGT If Installed)
[ ]  Lights .... AS REQ
[ ]  Flight Plan .... OPEN
[ ]  Co. Frequency .... MONITOR 129.25 WHENEVER ABLE

Descent
[ ]  Landing Light .... ON
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... ON/HOT
[ ]  Throttle .... AS REQ

Before Landing
NOTE: ALOUD ALL TRAINING FLIGHTS SOLO OR DUAL SEVERAL TIMES
[ ]  Carb. Heat .... VERIFIED ON
[ ]  Gas (Fuel Valve) .... BOTH
[ ]  Undercarriage (Fixed) .... DOWN
[ ]  Mixture .... FULL RICH
[ ]  Primer .... IN & LOCKED
[ ]  Seatbelts / Switches .... CHECK

Normal Landings
[ ]  Airspeed .... 65-75 KIAS
[ ]  Flaps .... AS REQ
[ ]  Airspeed (with flaps) .... 60-70 KIAS
[ ]  Throttle .... AS REQ
[ ]  Braking .... MIN REQ

Soft Field Landing
[ ]  Airspeed .... 65-75 KIAS
[ ]  Flaps .... 30°
[ ]  Short Final .... 61 KIAS
[ ]  Touchdown .... NOSE HIGH
[ ]  Throttle .... IF/OR AS REQ
[ ]  Nose Wheel .... HOLD OFF
[ ]  Elevator .... FULL AFT FOR TAXI
[ ]  Throttle .... AS REQ/RNWY COND.

Short Field Landing
[ ]  Airspeed .... 65 - 75 KIAS
[ ]  Flaps .... 30°
[ ]  Airspeed .... MAINTAIN 61 KIAS (Until Flare)
[ ]  Clearing Obstacle .... THROTTLE REDUCE TO IDLE AT TOUCHDOWN
[ ]  Flaps .... RETRACT
[ ]  Brakes .... APPLY HEAVILY

Go Around
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... COLD/OFF
[ ]  Flaps 20° .... IMMEDIATELY
[ ]  Airspeed .... INCREASING
[ ]  Flaps .... RETRACT SLOWLY

After Landing
[ ]  Flaps .... UP
[ ]  Carburetor Heat .... COLD
[ ]  Transponder .... OFF/1200
[ ]  Pitot Heat .... OFF
[ ]  Lights .... AS REQ
[ ]  Taxi Clearance .... OBTAIN

Securing Airplane
[ ]  Avionics/Avionics Master .... OFF
[ ]  Lights/Switches (Ex. Beacon) .... OFF
[ ]  Throttle .... MIN. 1000 RPM
[ ]  Mixture .... IDLE CUT OFF
[ ]  Ignition (verify prop stopped) .... OFF
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
[ ]  Hobbs .... RECORD
[ ]  Tie Down Aircraft .... SECURELY
[ ]  Post-flight Inspection .... DO
[ ]  Flight Plan .... CLOSE WITH FSS

Emergency Checklist — Fires  [EMERGENCY]
ENGINE FIRE DURING START
[ ]  Cranking .... CONTINUE
IF ENGINE STARTS
[ ]  Power .... 1700 RPM/1 MIN.
[ ]  Engine .... SHUTDOWN/INSPECT
ENGINE FAILS TO START
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... IDLE CUT OFF
[ ]  Cranking .... CONTINUE
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Master Switch .... OFF
[ ]  Ignition Switch .... OFF
[ ]  Fire Extinguisher .... OBTAIN/EXT.
[ ]  Fire Damage .... INSPECT
ENGINE FIRE DURING FLIGHT
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Master Switch .... OFF
[ ]  Cabin Heat & Air .... OFF (except overhead vents)
[ ]  Airspeed .... 100 KIAS
NOTE: If fire is not extinguished, increase airspeed to an incombustible mixture.
[ ]  Forced Landing .... EXECUTE
WING FIRE
[ ]  Nav/Strobe/Landing Lights .... OFF
[ ]  Pitot Heat .... OFF
[ ]  Perform .... SIDE SLIP AWAY FROM THE FUEL TANK AND CABIN
ELECTRICAL FIRE IN FLIGHT
[ ]  Master Switch .... OFF
[ ]  Switches (except Ignition) .... OFF
[ ]  Vents/Cabin Air/Heat .... CLOSED
[ ]  Extinguisher .... ACTIVATE
[ ]  Fire Out .... VENTILATE CABIN
NOTE: IF FIRE OUT & ELECTRIC IS NECESSARY FOR CONTINUED FLIGHT (i.e. I.F.R.& I.M.C.) THEN:
[ ]  Master .... ON
[ ]  Circuit Breakers .... CHK/NO RESET
[ ]  All Radio Switches .... OFF
[ ]  Avionics Power Switch .... ON
[ ]  Radio/Elect. Switches .... ON ONE AT A TIME, WITH DELAY UNTIL FAULT FOUND

Engine Failure Takeoff Run  [EMERGENCY]
[ ]  Throttle .... IDLE
[ ]  Brakes .... APPLY
[ ]  Flaps .... UP
[ ]  Mixture .... IDLE CUT OFF
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF

Engine Failure After Takeoff  [EMERGENCY]
[ ]  Best Glide .... 60 KIAS
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Mixture .... IDLE CUT OFF
[ ]  Ignition Switch .... OFF
[ ]  Flaps .... AS REQ
[ ]  Master Switch .... OFF

Engine Failure During Flight  [EMERGENCY]
[ ]  Airspeed Best Glide .... 65 KIAS
[ ]  Best Place To Land .... TURN TO
[ ]  Carburetor Heat .... ON
[ ]  Fuel Shutoff Valve .... BOTH
[ ]  Mixture .... RICH
[ ]  Ignition Switch .... CHECK BOTH/OR START IF PROP IS STOPPED
[ ]  Primer .... IN & LOCKED
[ ]  Trouble Shoot .... MAGS CYCLE THROTTLE PUMP
UNABLE TO RE-START:
[ ]  Declare May Day .... ATC or 121.5
[ ]  Squawk .... 7700

Forced Landing Without Engine Power  [EMERGENCY]
[ ]  Airspeed .... 65 KIAS FLAPS UP; 60 KIAS FLAP DOWN
[ ]  Fuel Shutoff Valve .... OFF
[ ]  Mixture .... IDLE CUT OFF
[ ]  Ignition Switch .... OFF
[ ]  Doors .... UNLATCH
[ ]  Flaps .... AS REQ
[ ]  Master Switch .... OFF LAST
[ ]  Touchdown .... TAIL LOW
[ ]  Brakes .... APPLY HEAVILY

Precautionary Landing With Engine Power  [EMERGENCY]
[ ]  Airspeed .... 60 KIAS
[ ]  Electrical Equipment .... OFF
[ ]  Flaps .... 20°
[ ]  Master Switch .... OFF
[ ]  Doors .... UNLATCH
[ ]  Touchdown .... TAIL LOW
[ ]  Ignition Switch .... OFF
[ ]  Brakes .... APPLY HEAVILY

Electrical Malfunction  [EMERGENCY]
OVER VOLTAGE CONDITION
[ ]  Alternator .... OFF
[ ]  Alternator Circuit Breaker .... PULL
[ ]  Nonessential electrical equip .... OFF
[ ]  Flight .... TERMINATE AS SOON AS PRACTICAL
LOW VOLTAGE CONDITION
[ ]  Avionics / Electrical .... OFF
[ ]  Alternator Circuit Breaker .... IN
[ ]  Master Switch .... OFF
[ ]  Master Switch .... ON
[ ]  Low Voltage Light .... CHECK OFF
[ ]  Avionics Power Switch .... ON
NOTE: If low voltage light illuminates again:
[ ]  Alternator .... OFF
[ ]  Nonessential elect. equip .... OFF
[ ]  Flight .... TERMINATE AS SOON AS PRACTICAL

Cold & Cool Weather Ops
NOTE: A preheated engine is required before starting during cool, cold, or winter operations. Ensure oil temp. is in the green or is moving before engine run-up and mag checks are attempted.
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