Cessna 172RG Skyhawk — Sam_Dawson_C172RG_InFlight_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Balked Landing" item count differs between passes (7 vs 8); verify nothing was dropped.
content_gap: Section "In Range-Descent" item count differs between passes (13 vs 18); verify nothing was dropped.

Final Before Take Off
[ ]  Heading .... Check w/ Runway
[ ]  Altimeter .... Field Elevation
[ ]  Transponder .... Alt
[ ]  Time .... Noted
[ ]  Exterior Lights .... On

Climb
[ ]  Fuel Selector .... BOTH
[ ]  Cowl Flaps .... OPEN as required
[ ]  Flaps .... Up
[ ]  Power .... 25”/ 2500 RPM
[ ]  Mixture .... Lean
[ ]  Airspeed .... 85-95 KIAS

Cruise
[ ]  Fuel Selector .... As Required
[ ]  Elevator and Rudder Trim .... Adjust
[ ]  Cowl Flaps .... CLOSED
[ ]  Power .... 15-25”/ 2100-2700 RPM
[ ]  Mixture .... Lean
[ ]  Landing Light .... Off
[ ]  Heading Indicator .... Align w/ Compass

In Range-Descent
[ ]  ATIS/AWOS/ASOS .... Received
[ ]  Altimeter .... Set
[ ]  Seats & Seat Belts .... Upright & Secured
[ ]  Fuel Selector .... BOTH
[ ]  Cowl Flaps .... CLOSED
[ ]  Mixture .... ENRICHEN as required
[ ]  Power .... As Required
[ ]  Carburetor Heat .... FULL as required
[ ]  Landing Light .... On
[ ]  Avionics .... Set
[ ]  Approach Briefing .... Complete
TURN-TIME-TWIST-THROTTLE-TALK
NOTE: Vx-67, Vy-84, Va- 89/98/106, Vref-60-70, Vshort-63

Approach Brief (boxed items VFR)
[ ]  -Approach
[ ]  -Frequency .... Set, ID
[ ]  Final Approach Course .... CDI Set
[ ]  FAF
[ ]  DH/MDA
[ ]  Approach Lights/PAPI/VASI
[ ]  TDZE, HAT/HAA
[ ]  MAP
[ ]  Missed Approach
[ ]  Notes
[ ]  -Runway exit/taxi plan
[ ]  -Terrain, obstacles
[ ]  Heading Indicator .... Align w/ Compass

Before Landing
[ ]  Landing Gear .... DOWN (below 140)
[ ]  Seats, Seat Belts, Shoulder Harnesses .... SECURE
[ ]  Fuel Selector .... BOTH
[ ]  Mixture .... Set
[ ]  Carburetor Heat .... As Required
[ ]  Flaps .... As Desired

SHORT FINAL
[ ]  Landing Gear .... CHECK
[ ]  Propeller .... HIGH RPM
[ ]  Auto Pilot .... OFF

After Landing
[ ]  Trim .... Set for Takeoff
[ ]  Flaps .... Up
[ ]  Transponder .... Sby
[ ]  Mixture .... Lean
[ ]  Exterior Lights .... As Required
[ ]  Carburetor Heat .... Cold
[ ]  Cowl Flaps .... OPEN

Balked Landing  [EMERGENCY]
[ ]  Power .... FULL THROTTLE, 2700 RPM
[ ]  Carburetor Heat .... COLD
[ ]  Cowl Flaps .... OPEN
[ ]  Wing Flaps .... RETRACT to 20°
[ ]  Climb Speed .... 55 KIAS
[ ]  Wing Flaps .... RETRACT after 65 KIAS
NOTE: Vx-67, Vy-84, Va- 89/98/106, Vref-60-70, Vshort- 63
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