Cessna 172RG Skyhawk — TFA_Cessna_172RG_Checklist_Emergency_2004-02
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "EMERGENCY LANDING WITHOUT ENGINE POWER" item count differs between passes (13 vs 11); verify nothing was dropped.
content_gap: Section "ENGINE FAILURE DURING FLIGHT" item count differs between passes (8 vs 7); verify nothing was dropped.
content_gap: Section "ENGINE FAILURE IMMEDIATELY AFTER TAKE-OFF" item count differs between passes (7 vs 6); verify nothing was dropped.
content_gap: Section "LANDING GEAR FAILS TO RETRACT" item count differs between passes (7 vs 6); verify nothing was dropped.
content_gap: Section "PRECAUTIONARY LANDING WITH ENGINE POWER" item count differs between passes (15 vs 14); verify nothing was dropped.

ENGINE FAILURE DURING TAKEOFF RUN  [EMERGENCY]
[ ]  THROTTLE .... IDLE
[ ]  BRAKES .... APPLY
[ ]  WING FLAPS .... RETRACT
[ ]  MIXTURE .... IDLE
[ ]  IGNITION SWITCH .... OFF
[ ]  MASTER SWITCH .... OFF

ENGINE FAILURE IMMEDIATELY AFTER TAKE-OFF  [EMERGENCY]
[ ]  AIRSPEED .... 70 KIAS
NOTE: 65 KIAS Flaps down
[ ]  MIXTURE .... IDLE
[ ]  FUEL VALVE .... OFF
[ ]  IGNITION SWITCH .... OFF
[ ]  FLAPS .... AS REQ (30° rec)
[ ]  MASTER SWITCH .... OFF

ENGINE FAILURE DURING FLIGHT  [EMERGENCY]
[ ]  AIRSPEED .... 75 KIAS
[ ]  CARB HEAT .... ON
[ ]  FUEL VALVE .... BOTH
[ ]  MIXTURE .... RICH
[ ]  AUX FUEL PUMP .... ON
NOTE: If fuel press is below .5 psi
[ ]  IGNITION SWITCH .... BOTH
[ ]  PRIMER .... IN & LOCKED

EMERGENCY LANDING WITHOUT ENGINE POWER  [EMERGENCY]
[ ]  SEATBELTS .... SECURE
[ ]  AIRSPEED .... 75 KIAS
NOTE: 65 KIAS Flaps down
[ ]  MIXTURE .... IDLE
[ ]  FUEL VALVE .... OFF
[ ]  IGNITION SWITCH .... OFF
[ ]  LANDING GEAR .... DOWN
NOTE: (UP FOR SOFT TERRAIN)
[ ]  WING FLAPS .... AS REQ
[ ]  MASTER SWITCH .... OFF
[ ]  DOORS .... UNLATCHED
[ ]  TOUCHDOWN .... TAIL LOW
[ ]  BRAKES .... HEAVILY

PRECAUTIONARY LANDING WITH ENGINE POWER  [EMERGENCY]
[ ]  SEATBELTS .... SECURE
[ ]  WING FLAPS .... 20°
[ ]  AIRSPEED .... 65 KIAS
[ ]  FIELD .... FLY OVER
[ ]  ELECT SWITCHES .... OFF
[ ]  LANDING GEAR .... DOWN
NOTE: (UP FOR SOFT TERRAIN)
[ ]  WING FLAPS .... 30° FINAL
[ ]  AIRSPEED .... 65 KIAS
[ ]  DOORS .... UNLATCH
[ ]  AVIONICS MASTER .... OFF
[ ]  MASTER SWITCH .... OFF
[ ]  TOUCHDOWN .... TAIL LOW
[ ]  IGNITION SWITCH .... OFF
[ ]  BRAKES .... HEAVILY

DURING START ON GROUND  [EMERGENCY]
[ ]  CRANKING .... CONTINUE
IF ENGINE STARTS:
[ ]  POWER .... 1700 RPM
[ ]  ENGINE .... SHUT DOWN
NOTE: (Inspect for damage)
IF ENGINE FAILS TO START:
[ ]  THROTTLE .... FULL OPEN
[ ]  MIXTURE .... IDLE
[ ]  CRANKING .... CONTINUE
[ ]  FIRE EXT .... OBTAIN
[ ]  ENGINE .... SECURE
[ ]  MASTER SWITCH .... OFF
[ ]  IGN. SWITCH .... OFF
[ ]  FUEL VALVE .... OFF
[ ]  FIRE .... EXTINGUISH
[ ]  DAMAGE .... INSPECT

ENGINE FIRE IN FLIGHT  [EMERGENCY]
[ ]  MIXTURE .... IDLE
[ ]  FUEL VALVE .... OFF
[ ]  MASTER SWITCH .... OFF
[ ]  CABIN HEAT/AIR .... OFF
[ ]  AIRSPEED .... 105 KIAS
NOTE: If fire is not extinguished, increase glide to an airspeed that provides an incombustible mixture.
[ ]  FORCED LAND .... EXECUTE

CABIN FIRE  [EMERGENCY]
[ ]  MASTER SWITCH .... OFF
[ ]  VENTS .... CLOSED
[ ]  FIRE EXT .... ACTIVATE
[ ]  CABIN .... VENTILATE
[ ]  LAND .... ASAP

ELECTRICAL FIRE IN FLIGHT  [EMERGENCY]
[ ]  MASTER SWITCH .... OFF
[ ]  AVIONICS PWR SW .... OFF
[ ]  ELECTRICAL SWS .... OFF
[ ]  VENTS .... CLOSED
[ ]  EXTINGUISHER .... ACTIVATE
[ ]  CABIN .... VENTILATE
[ ]  MASTER SWITCH .... ON
[ ]  C/BREAKERS .... CHECK
[ ]  RADIO SWITCHES .... OFF
[ ]  AVIONICS PWR SW .... ON
[ ]  ELECTRICAL SWITCHES .... ON ONE AT A TIME
[ ]  VENTS .... OPEN

WING FIRE  [EMERGENCY]
[ ]  NAV LIGHTS .... OFF
[ ]  STROBE LIGHTS .... OFF
[ ]  PITOT HEAT SWITCH .... OFF

LANDING WITH FLAT MAIN TIRE  [ABNORMAL]
[ ]  APPROACH .... NORMAL
[ ]  TOUCHDOWN .... GOOD WHEEL FIRST

LANDING GEAR FAILS TO RETRACT  [ABNORMAL]
[ ]  MASTER SWITCH .... ON
[ ]  GEAR LEVER .... CHECK UP
[ ]  CIRCUIT BREAKERS .... IN
[ ]  GEAR UP LIGHT .... CHECK
[ ]  GEAR LEVER .... RECYCLE
[ ]  GEAR MOTOR .... CHECK
NOTE: (ammeter and noise)

LANDING GEAR FAILS TO EXTEND  [ABNORMAL]
[ ]  MASTER SWITCH .... ON
[ ]  GEAR LEVER .... DOWN
[ ]  CIRCUIT BREAKERS .... IN
[ ]  AIRSPEED .... 100 KIAS/LESS
[ ]  EMERGENCY PUMP .... PUMP
[ ]  GEAR DOWN LIGHT .... ON
[ ]  PUMP HANDLE .... STOW

GEAR UP LANDING  [EMERGENCY]
[ ]  GEAR LEVER .... UP
[ ]  CIRCUIT BREAKERS .... IN
[ ]  RUNWAY .... SELECT
[ ]  FLAPS .... 30° ON FINAL
[ ]  AIRSPEED .... 65 KIAS
[ ]  DOORS .... UNLATCHED
[ ]  AVIONICS PWR. SW .... OFF
[ ]  MASTER SWITCH .... OFF
[ ]  TOUCH DWN .... TAIL LOW
[ ]  MIXTURE .... IDLE
[ ]  IGNITION SWITCH .... OFF
[ ]  FUEL VALVE .... OFF
[ ]  AIRPLANE .... EVACUATE

LANDING WITHOUT POSITIVE INDICATION OF GEAR LOCKING  [ABNORMAL]
[ ]  B4 LAND CHECK .... DO
[ ]  APPROACH .... NORMAL
[ ]  CIRCUIT BREAKERS .... IN
[ ]  LANDING .... TAIL LOW
[ ]  BRAKING .... MINIMUM
[ ]  TAXI .... SLOWLY
[ ]  ENGINE .... SHUTDOW

LANDING WITH DEFECTIVE NOSE GEAR  [ABNORMAL]
[ ]  MOVABLE LOAD X-FR. .... TO BAGGAGE AREA
[ ]  PASSENGER .... MOVE TO REAR SEAT
[ ]  B4 LAND CHECK .... DO
[ ]  RUNWAY .... HARD/SMOOTH
[ ]  FLAPS .... 30 DEGREES
[ ]  CABIN DOORS .... UNLATCH
[ ]  AVIONICS PWR SW .... OFF
[ ]  MASTER SWITCH .... OFF
[ ]  LAND .... TAIL LOW
[ ]  MIXTURE .... IDLE
[ ]  IGNITION SWITCH .... OFF
[ ]  FUEL SELECTOR .... OFF
[ ]  HOLD NOSE UP .... HOLD
[ ]  AIRPLANE .... EVACUATE

LOW VOLTAGE LIGHT DURING FLIGHT  [ABNORMAL]
AMMETER INDICATES DISCHARGE
[ ]  AVIONICS PWR SW .... OFF
[ ]  ALTERNATOR C/B .... CHECK IN
[ ]  MASTER SWITCH .... OFF
[ ]  MASTER SWITCH .... ON
[ ]  LOW-VOLT LIGHT .... OFF
[ ]  AVIONICS PWR SW .... ON
IF LOW-VOLTAGE LIGHT ILLUMINATES AGAIN:
[ ]  ALTERNATOR .... OFF
[ ]  ESSENTIAL RADIOS ONLY .... USE
[ ]  FLIGHT .... TERMINATE

AMMETER EXCESSIVE RATE OF CHARGE  [ABNORMAL]
FULL SCALE DEFLECTION
[ ]  ALTERNATOR .... OFF
[ ]  ALTERNATOR C/B .... PULL
[ ]  ONLY ESSENTIAL RADIOS .... USE
[ ]  FLIGHT .... TERMINATE

DITCHING  [EMERGENCY]
[ ]  RADIO MAYDAY .... ON 121.5
[ ]  XPONDER .... SQUAWK 7700
[ ]  HEAVY OBJECTS .... SECURE OR JETISON
[ ]  LANDING GEAR .... UP
[ ]  FLAPS .... 20° to 30°
[ ]  SEATBELTS .... SECURE
[ ]  AIRSPEED .... 60 KIAS
[ ]  DESCENT RATE .... 300 FT/MIN
NOTE: IF NO POWER AVAILABLE, 70 KIAS FLAPS UP OR 65 KIAS WITH 10 DEGREES FLAPS
APPROACH:
NOTE: HIGH WINDS HEAVY SEAS: INTO WIND
NOTE: LIGHT WINDS & HEAVY SWELLS: PARALLEL TO SWELLS
[ ]  DOORS .... UNLATCH
[ ]  TOUCHDOWN .... LEVEL
[ ]  FACE .... CUSHION
[ ]  AIRPLANE .... EVACUATE
[ ]  VESTS & RAFT .... INFLATE
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