Cessna 172RG Skyhawk — TFA_Cessna_172RG_Checklist_Normal_2004-02
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Before Takeoff" item count differs between passes (20 vs 21); verify nothing was dropped.
content_gap: Section "Radio Frequencies" item count differs between passes (10 vs 9); verify nothing was dropped.

Speeds
[ ]  BEST GLIDE .... 73 KIAS
[ ]  Vr .... 55 KIAS
[ ]  Vx .... 67 KIAS
[ ]  Vy .... 84 KIAS
[ ]  Vne .... 164 KIAS
[ ]  Vno .... 145 KIAS
[ ]  Vso .... 42 KIAS
[ ]  Vlo .... 140 KIAS
[ ]  Vle .... 164 KIAS
[ ]  Va .... 89-106 KIAS
[ ]  Vfe .... 130-100 KIAS
[ ]  Max Crosswind .... 15 KIAS

Radio Frequencies
[ ]  Take Flight .... 129.25
NOTE: (monitor when able)
[ ]  Merrill ATIS .... 123.70
[ ]  Merrill Ground .... 121.70
[ ]  Merrill Tower .... 126.00
[ ]  Anch Appch .... N 119.1/S 126.4
[ ]  Elmendorf Tower .... 127.2
[ ]  Big Lake/Willow/Wasilla .... 122.8
[ ]  Goose Bay .... 122.9
[ ]  Birchwood .... 123.0

Cold Weather Ops
NOTE: Ensure oil temp is in the green or moving before engine run-up/mag check and prior to flight. Preheating a cold engine is required before starting during winter operations.

Preflight Inspection - Cabin
[ ]  AROW/100hr/Mtc .... CHECK
[ ]  Landing Gear Lever .... DOWN
[ ]  Hobbs Meter .... CHECK
[ ]  Control Lock .... REMOVE
[ ]  Ignition Switch .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Master Switch .... ON
[ ]  Fuel Qty .... CHECK
[ ]  Landing Gear Light .... ON
[ ]  Av. Cooling Fan .... CHECK
[ ]  Lights .... CHECK
[ ]  Flaps .... 30(
[ ]  Master Switch .... OFF
[ ]  Fuel Selector Valve .... BOTH
[ ]  Alt Static Source .... OFF
[ ]  Baggage Door .... CHECK

Preflight Inspection - Empennage
[ ]  Rudder Gust Lock .... REMOVE
[ ]  Tail Tie Down .... REMOVE
[ ]  Elevator & Rudder .... CHECK

Preflight Inspection - Right Wing
[ ]  Aileron & Flap .... CHECK
[ ]  Skin/Tip/Lights .... CHECK
[ ]  Tie Down .... REMOVE
[ ]  Strut/Tire/Brake .... CHECK
[ ]  Fuel Tank Sump .... SAMPLE
[ ]  Fuel Qty .... CHECK
[ ]  Fuel Filler Cap .... SECURE

Preflight Inspection - Nose
[ ]  Static Source (both) .... CHECK
[ ]  Engine Oil .... 6 to 8 QUARTS
[ ]  Fuel Strainer .... DRAIN & SAMPLE
[ ]  Fuel Selector/Belly Drain .... SAMPLE
[ ]  Prop & Spinner .... CHECK
[ ]  Landing Light .... CHECK
[ ]  Nose Gear Doors .... CHECK
[ ]  Nose Wheel & Strut .... CHECK

Preflight Inspection - Left Wing
[ ]  Fuel Tank Sump .... SAMPLE
[ ]  Fuel Qty .... CHECK
[ ]  Fuel Filler Cap .... SECURE
[ ]  Strut/Tire/Brake .... CHECK
[ ]  Pitot Tube & Drain .... CHECK
[ ]  Stall Warning .... CHECK
[ ]  Fuel Tank Vent .... CHECK
[ ]  Tie Down .... REMOVE
[ ]  Aileron & Flap .... CHECK

Before Starting Engine
[ ]  Preflight .... COMPLETE
[ ]  Passenger Brief .... COMPLETE
[ ]  Seat Belts .... SECURE
[ ]  Fuel Selector Valve .... BOTH
[ ]  Avionics Pwr. Switch .... OFF
[ ]  Avionics Circuit Breakers .... IN
[ ]  Circuit Breakers .... CHECK IN
[ ]  Elec. Equip./Autopilot .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Landing Gear Lever .... DOWN
[ ]  Brakes .... SET HOLD

Starting Engine
[ ]  Beacon .... ON
[ ]  Mixture .... RICH
[ ]  Propeller .... HIGH RPM
[ ]  Throttle .... 1/4 INCH
[ ]  Carb Heat .... OFF
[ ]  Prime .... AS REQ.
[ ]  Master Switch .... ON
[ ]  Propeller Area .... CLEAR
[ ]  Ignition Switch .... START
[ ]  Oil Pressure .... CHECK
[ ]  Avionics Pwr. Switch .... ON
[ ]  Lights .... AS REQIRED
[ ]  Flaps .... UP

Before Takeoff
[ ]  Brakes .... TEST/SET
[ ]  Doors .... CLOSED/LOCKED
[ ]  Seat Belts .... FASTENED
[ ]  Controls .... FREE & CORRECT
[ ]  Trim .... SET
[ ]  Flight Instruments .... CHECK
[ ]  Fuel Selector Valve .... BOTH
[ ]  Mixture .... RICH
[ ]  Aux Fuel Pump .... ON/OFF
[ ]  Throttle .... 1800 RPM
[ ]  a. Magnetos .... CHECK
[ ]  b. Prop .... CYCLE
[ ]  c. Carb Heat .... CHECK
[ ]  d. Engine Inst .... CHECK
[ ]  e. Ammeter .... CHECK
[ ]  f. Suction Gg. .... CHECK
[ ]  Throttle .... 800-1000 RPM
[ ]  Radios .... CHECK
[ ]  Autopilot .... RECHECK OFF
[ ]  Throttle Friction .... ADJUST

Taking Runway
[ ]  Clearance Rec’vd .... TO/P&H
[ ]  Approach End .... CLEAR
[ ]  Lights .... ON
[ ]  Camera .... Transponder Alt
[ ]  Action .... D.G. Runway Hdg
[ ]  Time Off .... Record

Normal Takeoff
[ ]  Flaps .... 0(
[ ]  Carb Heat .... OFF
[ ]  Throttle .... FULL OPEN
[ ]  Airspeed/Eng Inst .... CHECK
[ ]  Rotate .... 55 KIAS
[ ]  Climb Speed .... 70-80 KIAS
[ ]  Brakes .... APPLY
[ ]  Landing Gear .... RETRACT

Short Field Takeoff
[ ]  Flaps .... 0 or 10 DEGREES
NOTE: (Zero if within 100lbs. of Gross)
[ ]  Brakes .... HOLD
[ ]  Throttle .... FULL OPEN
[ ]  Carburetor Heat .... OFF
[ ]  Engine Instr. .... GREEN/NORM
[ ]  Brakes .... RELEASE
[ ]  Rotate .... 55 KIAS
[ ]  Climb Speed .... 63 KIAS
[ ]  Over Obstacle .... 84 KIAS & FLAPS UP

Enroute Climb
[ ]  Airspeed .... 85-95 KIAS
[ ]  Power .... 25 in Hg & 2500 rpm
[ ]  Mixture .... AS REQ
[ ]  Cowl Flaps .... OPEN

Cruise
[ ]  Power .... 15-25 in Hg / 2100-2700 RPM
[ ]  Elev/Rudder .... TRIM
[ ]  Cowl Flaps .... CLOSED
[ ]  Mixture .... AS REQ
[ ]  Lights .... AS REQ
[ ]  Flight Plan .... OPEN
[ ]  Company Freq .... MONITOR

Descent
[ ]  Fuel Selector .... BOTH
[ ]  Mixture .... RICH
[ ]  Carb Heat .... ON AS REQ
[ ]  Cowl Flaps .... CLOSED
[ ]  Throttle .... AS REQ
[ ]  Landing Light .... ON
[ ]  Wing Flaps .... AS REQ

Before Landing
[ ]  Carb Heat .... ON
[ ]  Cowl Flaps .... CLOSED
[ ]  Gas (fuel selector) .... BOTH
[ ]  Undercarriage .... DOWN
[ ]  Mixture .... RICH
[ ]  Propeller .... HIGH RPM
[ ]  Seat Belts .... SECURE
NOTE: ON FINAL CALL OUT & VERIFY AGAIN:
NOTE: “FINAL UMP’s CHECK…….
[ ]  Undercarriage .... Green/Down & Locked
[ ]  Mixture .... RICH
[ ]  Prop .... HIGH

Normal Landing
[ ]  Airspeed .... 65-75 KIAS
[ ]  Flaps .... AS REQ
[ ]  Airspeed .... 60-70 KIAS
[ ]  Throttle .... AS REQ
[ ]  Braking .... MIN REQ

Short Field Landing
[ ]  Airspeed .... 65-75 KIAS
[ ]  Flaps .... 30 DEGREES
[ ]  Short Final .... 63 KIAS
[ ]  Throttle .... AS REQ
[ ]  Brakes .... APPLY HEAVILY
[ ]  Flaps .... RETRACT

Go Around Procedure With Full Flaps
[ ]  Throttle .... FULL OPEN
[ ]  Carb Heat .... COLD
[ ]  Flaps .... 20(
[ ]  Airspeed .... INCREASING
[ ]  Altitude .... INCREASING
[ ]  Flaps .... 10(
[ ]  Vy 87 KIAS .... OBTAIN
[ ]  Flaps .... 0(
[ ]  Cowl Flaps .... OPEN

After Landing
[ ]  Flaps .... UP
[ ]  Carb Heat .... COLD
[ ]  Cowl Flaps .... OPEN
[ ]  Transponder .... OFF
[ ]  Lights .... OFF
[ ]  Taxi Clearance .... OBTAIN

Securing Airplane
[ ]  Avionics Pwr Sw .... OFF
[ ]  Electrical Equip .... OFF
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... IDLE CUT OFF
[ ]  Throttle .... Close as rpm drops
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF
[ ]  Cowl Flaps .... (winter) CLOSED
[ ]  Control Lock .... INSTALL
[ ]  Hobbs .... RECORD
[ ]  Flight Plan .... CLOSE
[ ]  Tie Down .... SECURE
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