Cessna 172S Skyhawk — JetStream_172S_N101GV Front Checklist 4.8.05
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Run Up" item count differs between passes (22 vs 25); verify nothing was dropped.

Before Start
[ ]  Preflight Inspection .... Complete
[ ]  Pass, Briefing .... Complete
[ ]  Seats / Seatbelts .... Adjust, Lock
[ ]  Brakes .... Set
[ ]  Circuit Breakers .... Check In
[ ]  Electrical and Avionics .... Off

Normal Engine Start
[ ]  Fuel Select Valve .... Both
[ ]  Fuel Shutoff Valve .... In (On)
[ ]  Mixture .... Idle Cutoff
[ ]  Throttle .... Open 1/4 inch
[ ]  Master Switch .... On
[ ]  Rotating Beacon .... On
[ ]  Aux Fuel Pump .... On
[ ]  Mixture .... Full Rich 3-5 GPH, then idle
[ ]  Aux Fuel Pump .... Off
[ ]  Area .... Clear
[ ]  Ignition Switch .... Engage, Release
when engine fires
[ ]  Mixture .... Smoothly full rich
[ ]  Oil Pressure .... Check
[ ]  Taxi, Nav. Lights .... As Required
[ ]  Avionics Master .... On
[ ]  Flaps .... Retract

Taxi
[ ]  Mixture .... Lean for Taxi
[ ]  Brakes .... Release, Check
[ ]  Instruments .... Check

Run Up
[ ]  Brakes .... Set
[ ]  Seats / Seatbelts .... Check Secure
[ ]  Doors .... Closed, Locked
[ ]  Flight Controls .... Free and Correct
[ ]  Flight Instruments .... Check and Set
[ ]  Radios / Navigation .... Set for Departure
[ ]  Navigation / GPS .... Set for Departure
[ ]  Fuel Selector .... Both
[ ]  Throttle .... 1800 rpm
[ ]  Mixture .... Set for Altitude
[ ]  Magnetos .... Left, Right, Both
[ ]  Engine Instruments .... Check
[ ]  Vacuum .... Check
[ ]  Ammeter .... Check with load
[ ]  Annunciator panel .... Test, Clear
[ ]  Throttle .... 1000 RPM
[ ]  Autopilot .... Off
[ ]  Throttle friction lock .... Set
[ ]  Elevator Trim .... Set for takeoff
[ ]  Flaps .... Set for takeoff
[ ]  Emergency, dep. brief .... Perform
[ ]  Brakes .... Release

Before Takeoff
[ ]  Landing light, strobes .... On
[ ]  Transponder .... Set to altitude
[ ]  Area .... Clear

Normal Takeoff
[ ]  Throttle .... Full Open
[ ]  Mixture .... Adjust smooth
[ ]  Elevator control .... Lift nose at 55 KIAS
[ ]  Climb Speed .... 75 KIAS

Climb (above 1000' AGL)
[ ]  Climb speed .... 75 KIAS
[ ]  Engine instruments .... Green
[ ]  Taxi, landing lights .... Off

Cruise
[ ]  Power .... 2100-2700 rpm
[ ]  Elevator trim .... Adjust
[ ]  Mixture .... Lean for altitude

Descent
[ ]  Fuel Selector .... Both
[ ]  Mixture .... Set
[ ]  Power .... Set
[ ]  Altimeter .... Set
[ ]  Nav/GPS .... Set

Before Landing
[ ]  Seats / Seatbelts .... Check Secure
[ ]  Fuel Selector .... Both
[ ]  Autopilot .... Off
[ ]  Taxi, landing lights .... On

Normal Landing
[ ]  Airspeed .... 65-75 KIAS flaps up
[ ]  Flaps .... As required
[ ]  Airspeed .... 60-70 KIAS flaps down

After Landing
[ ]  Flaps .... Retract
[ ]  Transponder .... Standby
[ ]  Land, Strobe lights .... Off
[ ]  Trim .... Takeoff

Shutdown and Securing
[ ]  Avionics and Switches .... Off
[ ]  Throttle .... Idle
[ ]  Mixture .... Idle Cutoff
[ ]  Mags .... Off
[ ]  Master .... Off
[ ]  Control Lock .... In
[ ]  Hobbs and Tach .... Record
[ ]  Tie Downs .... Attached
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