Cessna 172S Skyhawk — Sam_Dawson_C172S_Ground
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

172S BEFORE STARTING ENGINE
[ ]  Preflight Inspection .... Complete
[ ]  CRM/Passenger Briefing .... Complete
[ ]  Seats and Seat Belts .... Adjust & Lock
[ ]  Brakes .... Test & Set
[ ]  Fuel Selector .... Both
[ ]  Fuel Shutoff .... On (In)
[ ]  Throttle .... Open ¼ “
[ ]  Mixture .... Idle Cutoff
[ ]  Avionics Master Switch .... Off
[ ]  Electrical Equipment .... Off
[ ]  Circuit Breakers .... Check In

STARTING ENGINE
[ ]  Master Switch .... On
[ ]  Lights .... As Required
[ ]  Auxiliary Fuel Pump .... On
[ ]  Mixture .... Full Rich, then off after fuel flow
[ ]  Auxiliary Fuel Pump .... Off
[ ]  Propeller Area .... Clear
[ ]  Ignition Switch .... Start
[ ]  Mixture .... Advance
[ ]  Oil Pressure / Ammeter .... Check

BEFORE TAXI
[ ]  Flaps .... Retract to takeoff setting
[ ]  Mixture .... Lean
[ ]  Throttle .... 1000 RPM
[ ]  Avionics Master Switch (Radios) .... On
[ ]  ATIS / AWOS .... Receive
[ ]  Clearance .... Obtain
[ ]  MFD & GPS .... Initialize
[ ]  Avionics / Transponder .... Set / SBY
[ ]  Flight Instruments .... Check & Set
[ ]  Engine Instruments .... Check

TAXI
[ ]  Brakes & Steering .... Check
[ ]  Flight Instruments .... Check
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BEFORE TAKEOFF
[ ]  Cabin Doors .... Closed & Locked
[ ]  Seats / Seat Belts .... Upright & Secured
[ ]  Flight Controls .... Free & Correct
[ ]  Clock .... Set
[ ]  Fuel Quantity .... Check
[ ]  Engine Instruments .... Check
[ ]  Flight Instruments .... Check & Set
[ ]  MFD & GPS .... Set
[ ]  Radios / Avionics .... Set for Departure
[ ]  NAV / GPS Switch .... Set
[ ]  Autopilot .... Test / Off
[ ]  Fuel Selector .... Both
[ ]  Fuel Shutoff .... On (In)
[ ]  Electric Trim / Elevator Trim .... Check / Set
[ ]  Flaps .... Set for Takeoff
[ ]  Mixture .... Enrichen
[ ]  Throttle .... 1800 RPM
[ ]  Mixture .... Lean for Takeoff
[ ]  Magnetos .... Check
[ ]  Engine Instruments / Ammeter .... Check
[ ]  Vacuum .... Green Arc
[ ]  Annunciator Panel .... Clear
[ ]  Throttle .... Idle / 1000 RPM
[ ]  Throttle Friction Lock .... Adjust
[ ]  Departure Briefing .... Complete

Shutdown and Securing
[ ]  Avionics Master .... Off
[ ]  Exterior Lights (except beacon) .... Off as Required
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... Idle Cut Off
[ ]  Magneto Switch .... Off
[ ]  Battery and Alternator .... Off
[ ]  Fuel Selector Valve .... Left or Right
[ ]  Gust Lock .... Install
[ ]  Post Flight Inspection .... Accomplish
[ ]  Internal and External Covers .... Install
[ ]  Tiedowns and Chocks .... Install
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