Cessna 177 Cardinal — C177_checklist_N29655 new
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

BEFORE STARTING ENGINE
[ ]  Preflight Inspection .... COMPLETE
[ ]  Seats Belts .... ADJUST AND LATCH
[ ]  Fuel Selector Valve .... ON BOTH
[ ]  Fuel Shutoff Valve .... ON
[ ]  Electrical Equipment .... OFF
[ ]  Avionics Master .... OFF
[ ]  Brakes .... TEST & SET
[ ]  Circuit Breakers .... CHECK IN

STARTING THE ENGINE
[ ]  Mixture .... RICH
[ ]  Carburetor Heat .... COLD
[ ]  Prime .... AS REQUIRED
[ ]  Throttle .... OPEN 1/8 INCH
[ ]  Propeller Area .... CLEAR
[ ]  Master Switch .... ON
[ ]  Ignition Switch .... START
[ ]  Oil Pressure .... CHECK
[ ]  Throttle .... 1000 RPM

TAXI CHECK
[ ]  Avionics Master .... ON
[ ]  Radios .... ON AS REQUIRED
[ ]  Beacon Light .... ON
[ ]  Flaps .... UP
[ ]  Call Pax Clearance Delivery .... 135.2
[ ]  Call Pax Ground for taxi .... 120.6
[ ]  Brakes .... CHECK

BEFORE TAKE-OFF
[ ]  Parking Brake .... SET
[ ]  Flight Controls .... FREE AND CORRECT
[ ]  Fuel Shutoff Valve .... ON
[ ]  Fuel Selector Valve .... ON BOTH
[ ]  Mixture .... RICH (BELOW 3000 FEET)
[ ]  Elevator Trim .... TAKE-OFF

BEFORE TAKE-OFF Continued
[ ]  Throttle Setting .... 1700 RPM
[ ]  Engine Instruments and Ammeter .... CHECK
[ ]  Carburetor Heat .... CHECK
[ ]  Magnetos .... CHECK, MAX DROP 150 RPM, MAX DIFFERENTIAL 50 RPM
[ ]  Aux Fuel Pump .... CHECK
[ ]  Suction Gage .... CHECK 4.6 IN HG – 5.4 IN HG
[ ]  Throttle .... IDLE
[ ]  Flight Instruments .... SET
[ ]  Radios .... SET
[ ]  NAV Lights .... AS REQUIRED
[ ]  Strobe Lights .... AS REQUIRED
[ ]  Throttle Friction Lock .... ADJUST
[ ]  Cabin Doors & Windows .... CLOSED
[ ]  Call Pax Tower for take-off .... 123.7
[ ]  Transponder .... ON ALT

NORMAL TAKE-OFF
[ ]  Wing Flaps .... 1/4 DOWN
[ ]  Carburetor Heat .... COLD
[ ]  Throttle .... FULL OPEN
[ ]  Elevator Control .... LIFT NOSE AT 60 MPH
[ ]  Climb Speed .... 75 TO 90 MPH

CLIMB
[ ]  Cruise Climb .... 90 TO 100 MPH
[ ]  Vx .... 67 MPH
[ ]  Vy .... 88 MPH
[ ]  Throttle .... FULL OPEN
[ ]  Mixture .... FULL RICH (BELOW 3000 FEET)

CRUISING
[ ]  Power .... 65% CRUISE RPM
[ ]  Trim Tab .... ADJUST
[ ]  Mixture .... LEAN

BEFORE LANDING
[ ]  Seats Belts .... ADJUST AND LATCH
[ ]  Mixture .... RICH
[ ]  Fuel Selector .... BOTH
[ ]  Carburetor Heat .... ON APPLY FULL HEAT BEFORE CLOSING THROTTLE

NORMAL LANDING
[ ]  Airspeed .... 80–75 MPH (FLAPS UP)
[ ]  Wing Flaps .... 1/4 BELOW 130 MPH
[ ]  Wing Flaps .... AS DESIRED (BELOW 105 MPH)
[ ]  Airspeed .... 70-80 MPH (FLAPS DOWN)
[ ]  Touchdown .... MAIN WHEELS FIRST
[ ]  Landing Roll .... LOWER NOSE WHEEL GENTLY
[ ]  Braking .... MINIMUM REQUIRED

AFTER LANDING
[ ]  Wing Flaps .... UP
[ ]  Carburetor Heat .... COLD
[ ]  Strobe Lights .... OFF

SECURING AIRCRAFT
[ ]  Parking Brake .... SET
[ ]  Radios & Electrical Equipment .... OFF
[ ]  Avionics Master .... OFF
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Ignition & Master Switch .... OFF
[ ]  Control Lock .... INSTALLED
[ ]  Windshield Sun Reflector .... INSTALLED
[ ]  Cowl & Tail Plugs .... INSTALLED
[ ]  Pitot Tube Cover .... INSTALLED
[ ]  Refuel Airplane .... AS REQUIRED
[ ]  Chock & Tie-down Airplane .... CHOCK & TIE-DOWN
[ ]  Record Hobbs, Tach & Gas .... RECORD
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