Cessna 182RG Skylane — Paul_Yust_cessna_c182RG_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "ENGINE FIRE – GROUND" item count differs between passes (8 vs 6); verify nothing was dropped.

PREFLIGHT - COCKPIT
[ ]  W&B / I’M SAFE .... CHECK
[ ]  AROW Documents .... ON BOARD
[ ]  Hobbs/Tach Time .... RECORD
[ ]  Key .... INSERTED
[ ]  Master .... ON
[ ]  Fuel Gauges/Fuel Valve .... CHECK
[ ]  Lights/Flaps .... CHECK
[ ]  Landing Gear Light .... GREEN
[ ]  Master .... OFF

PREFLIGHT - EXTERNAL
[ ]  Tie Downs & Chocks .... REMOVE
[ ]  Fuel Sumps (1st Flight) .... SAMPLE
[ ]  Fuel Quantity .... VISUAL CHECK
[ ]  Oil Level .... 5-8 QTS
[ ]  Windshield .... CLEAN
[ ]  Antennas/Static Ports .... CHECK
[ ]  Wings/ Ailerons/Flaps .... CHECK
[ ]  Rudder/Elevator .... CHECK
[ ]  Pitot Tube & Stall Vane .... CHECK
[ ]  Main Gear/Brakes (50 psi) .... CHECK
[ ]  Nose Gear (68 psi) .... CHECK
[ ]  Propeller & Spinner .... CHECK
[ ]  Baggage Door .... SECURE

ENGINE START
[ ]  Passenger Brief .... COMPLETE
[ ]  Seats & Belts .... SECURE
[ ]  Avionics/Electrics .... OFF
[ ]  Fuel Selector .... BOTH
[ ]  Cowl Flaps .... OPEN
[ ]  Master .... ON
[ ]  Beacon (Always On) .... ON
[ ]  Carb Heat .... OFF
[ ]  Mixture & Prop .... FULL FORWARD
[ ]  Prime (2-6 Strokes) .... AS REQ
[ ]  Throttle .... PUMP then ¼” OPEN
[ ]  Aux Fuel Pump (Check Press.) .... ON/OFF
[ ]  Prop Area .... CLEAR
[ ]  Brakes .... HOLD
[ ]  Mags .... START
[ ]  Throttle .... 1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Mixture .... LEAN
[ ]  Avionics/Electrics .... ON & SET
[ ]  Ground ATC .... CLEARENCE
[ ]  Parking Brake .... OFF
[ ]  Taxi Checks .... BRAKES, TC, AI, & DG

V-SPEEDS (KIAS @ Max Wt)
[ ]  VGLIDE .... 80
[ ]  VX .... 65
[ ]  VA .... 112
[ ]  VS0 .... 39
[ ]  VY .... 88
[ ]  VNO .... 158
[ ]  VS .... 41
[ ]  VFE 20° .... 95
[ ]  VNE .... 181
[ ]  VR .... 50
[ ]  VFE 10° .... 140
[ ]  VLO .... 140

RUNUP & TAKEOFF
[ ]  Mixture (<3000’) .... RICH
[ ]  Engine Run-Up .... 1700 RPM
[ ]  -  Mags 175/50, Prop, Carb., Engine Inst. .... CHECK
[ ]  Flight Controls .... FREE & CORRECT
[ ]  Flight Instruments .... SET
[ ]  Elevator & Rudder Trim .... SET
[ ]  Flaps (Short/Soft 20o) .... SET
[ ]  Autopilot .... CHECK & OFF
[ ]  Seats/Belts/Doors/Windows .... SECURE
[ ]  Tower & Traffic .... CLEARENCE
[ ]  Lights & Pitot Heat .... SET
[ ]  Power (Throttle/Prop/Mix) .... ALL FWD
[ ]  Climb Speed .... 88 KTS
[ ]  Gear/Flaps .... UP
[ ]  Landing light .... OFF

CRUISE
[ ]  Cowl Flaps .... CLOSED
[ ]  Power .... AS REQ
[ ]  Mixture .... LEAN BELOW 75% PWR

LANDING
[ ]  ATIS/AWOS .... OBTAIN
[ ]  IFR Approach Brief .... COMPLETE
[ ]  GUMPS Check .... COMPLETE
[ ]  Flaps .... SET
[ ]  Landing Light .... ON
[ ]  Approach Speed .... 70-80 KTS

MISSED APPROACH
[ ]  Cram .... FULL THROTTLE
[ ]  Climb (100 KTS) .... PITCH +6o on AI
[ ]  Cleanup .... GEAR & FLAPS
[ ]  Cool .... COWL FLAPS OPEN
[ ]  Call .... TRAFFIC/TOWER

AFTER LANDING
[ ]  Flaps .... UP
[ ]  Elevator & Rudder Trim .... SET
[ ]  Cowl Flaps .... OPEN
[ ]  Carb Heat .... OFF
- READY FOR TOUCH & GO
[ ]  Mixture .... LEAN
[ ]  Transponder .... STANDBY
[ ]  Pitot Heat, Strobe .... OFF

SHUTDOWN
[ ]  S  Switches/Avionics .... OFF
[ ]  L  Lean Mixture .... IDLE-CUTOFF
[ ]  I   Ignition Mags .... OFF
[ ]  M Master .... OFF
[ ]  Hobbs/Tach Time .... RECORD
[ ]  Gust Lock .... SECURE
[ ]  Flight Plan .... CLOSED

EMERGENCY LANDING  [EMERGENCY]
[ ]  Pitch For Best Glide .... 80 KTS
[ ]  Landing field .... SELECTED
TIME PERMITTING:
[ ]  Aux Fuel Pump .... ON
[ ]  Fuel Tank Selector .... BOTH
[ ]  Mixture .... RICH
[ ]  Mags .... BOTH
[ ]  Radio (121.5 or Tower) .... MAYDAY
[ ]  Transponder .... 7700
[ ]  ELT .... ON
[ ]  Seats & Belts .... READY
[ ]  Door .... AJAR
[ ]  Mixture/Fuel Valve .... OFF
[ ]  Gear/Flaps .... AS REQ
[ ]  Mags/Master .... OFF
[ ]  Short Final (full-no flaps) .... 65-70 KTS

RESTART ENGINE – IN FLIGHT  [EMERGENCY]
[ ]  Airspeed .... 80 KTS
[ ]  Fuel Selector .... BOTH
[ ]  Carb Heat .... HOT
[ ]  Throttle .... ¼” OPEN
[ ]  Mixture & Prop .... FULL FORWARD
[ ]  Mags .... BOTH
[ ]  Aux Fuel Pump (If no pressure) .... ON
[ ]  Mixture (If no restart) .... CYCLE

MANUAL GEAR EXTENSION  [EMERGENCY]
[ ]  Gear Light/Circuit Breaker .... CHECK
[ ]  Airspeed .... 100 KTS
[ ]  A/P (if available) .... ENGAGE
[ ]  Gear Pump Breaker .... PULL OUT
[ ]  Gear Lever .... DOWN
[ ]  Gear Hand Pump .... EXTEND/PUMP 20+
[ ]  Gear Hand Pump .... STOW
[ ]  Gear Pump Breaker .... PUSH IN

GEAR RETRACT FAILURE  [ABNORMAL]
[ ]  Master .... ON
[ ]  Gear Lever .... VERIFY UP
[ ]  Gear & Pump Breakers .... CHECK IN
[ ]  Gear Lever .... CYCLE
[ ]  Gear Motor (amps & noise) .... VERIFY

ENGINE FIRE – GROUND  [EMERGENCY]
[ ]  Mags .... CONTINUE CRANKING
IF ENGINE STARTS WITHOUT FIRE:
[ ]  Power .... 1700 RPM FOR 3 MINS
IF ENGINE DOES NOT START:
[ ]  Throttle .... FULL OPEN
[ ]  Mixture/Fuel Valve .... OFF
[ ]  Mags/Master .... OFF
[ ]  Exit Plane .... ASAP

ENGINE FIRE – IN FLIGHT  [EMERGENCY]
[ ]  Mixture/Fuel Valve .... OFF
[ ]  Mags/Master .... OFF
[ ]  Vents/Window .... OPEN if smoke enters
[ ]  Airspeed (blow out fire) .... 100+ KTS
[ ]  Land .... ASAP

ELECTRICAL FIRE – IN FLIGHT  [EMERGENCY]
[ ]  Master/Avionics .... OFF
[ ]  Vents/Window .... OPEN if smoke enters
[ ]  Extinguisher .... ACTIVATE
IF ELECTRICS REQUIRED:
[ ]  Circuit Breakers .... CHECK
[ ]  All Electric Switches .... OFF
[ ]  Master .... ON
[ ]  Electrical Switches .... 1 AT TIME

AMMETER SHOW DISCHARGE  [ABNORMAL]
[ ]  Alternator (Left Side Master) .... OFF
[ ]  Nonessential Electrics .... OFF

OVER VOLTAGE LIGHT ON  [ABNORMAL]
[ ]  Avionics Master .... OFF
[ ]  Alternator (Left Side Master) .... OFF/ON
[ ]  Avionics Master .... ON

ICING CONDITIONS  [ABNORMAL]
[ ]  Pitot Heat .... ON
[ ]  Direction and/or Altitude .... CHANGE
[ ]  Cabin Heat & Defrost .... ON
[ ]  Carb Heat .... AS REQ
[ ]  Airspeed .... FASTER THAN NORMAL

IFR APPROACH @ ~ 95 KTS
Turn-Time-Twist-Throttle-Talk
[ ]  Level flight approaching FAF .... ~16”, Prop IN, Gear UP, Flaps UP
[ ]  500 FPM ILS precision decent .... ~15”, Prop IN, Gear DN, Flaps 10°
[ ]  700 FPM VOR non-precision decent .... ~13”, Prop IN, Gear DN, Flaps 10°
[ ]  Level flight circle to land .... ~20”, Prop IN, Gear DN, Flaps 10°

WEIGHT & BALANCE (LBS)
[ ]  Gross Weight .... 3100 LBS
[ ]  Empty Weight .... 1886 LBS
[ ]  Useful Load .... 1214 LBS
[ ]  Payload (65 gals @ neck*) .... 824 LBS
[ ]  Payload (88 gals @ full) .... 686 LBS
NOTE: To the bottom filler neck
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