Cessna 182S Skylane — JetStream_C182 Front Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Before Start
[ ]  Preflight Inspection .... Complete
[ ]  Passenger Briefing .... Complete
[ ]  Seats / Seatbelts .... Adjust, Lock
[ ]  Fuel Selector Valve .... Both
[ ]  Cowl Flaps .... Open
[ ]  Brakes .... Set
[ ]  Avionics, Electrical .... Off
[ ]  Circuit Breakers .... Check In

Normal Engine Start
[ ]  Mixture .... Rich
[ ]  Propeller .... High RPM
[ ]  Power .... 1/2 Inch
[ ]  Carburetor Heat .... Cold
[ ]  Prime .... 1-6 as req'd
[ ]  Rotating Beacon .... On
[ ]  Master Switch .... On
[ ]  Area .... Clear
[ ]  Ignition Switch .... Engage
[ ]  Mixture .... Lean
[ ]  Engine Instruments .... Check
[ ]  Taxi, Nav. Lights .... As Required
[ ]  Avionics Master .... On
[ ]  Flaps .... Retract

Taxi
[ ]  Weather info/ATIS .... Obtain
[ ]  Avionics and Flight Instruments .... Check/Set
[ ]  Brakes .... Release, Check

Run Up
[ ]  Doors .... Closed, Locked
[ ]  Parking Brake .... Set
[ ]  Flight Controls .... Free and Correct
[ ]  Flight Instruments .... Check and Set
[ ]  Fuel Selector .... Both
[ ]  Trim .... Set for takeoff
[ ]  Power .... 1700 rpm
[ ]  Mixture .... Set
[ ]  Magnetos .... Left, Right, Both
[ ]  Propeller .... Cycle
[ ]  Carb Heat .... Check
[ ]  Engine Instruments .... Check
[ ]  Vacuum .... Check
[ ]  Ammeter .... Check with load
[ ]  Throttle .... Idle, then 1000 RPM
[ ]  Throttle friction lock .... Set
[ ]  Flaps .... Set for takeoff
[ ]  Emergency, dep. brief .... Perform
[ ]  Radios .... Set for Departure
[ ]  Navigation / GPS .... Set for Departure
[ ]  Brakes .... Release

Before Takeoff
[ ]  Landing light, strobes .... On
[ ]  Transponder .... Set to altitude
[ ]  Area .... Clear

Normal Takeoff (to 1000' AGL)
[ ]  Power/Prop .... Full
[ ]  Mixture .... Adjust smooth
[ ]  Elevator control .... Lift nose at 50 KIAS
[ ]  Climb Speed .... 80 KIAS

Climb (above 1000' AGL)
[ ]  Climb speed .... 90-100 KIAS
[ ]  Power/Prop .... Top of the Green
[ ]  Mixture .... Adjust
[ ]  Lights .... As required

Cruise
[ ]  Power/Prop .... 15-23 in., 2100-2450 RPM
[ ]  Elevator/Rudder trim .... Adjust
[ ]  Mixture .... Lean for altitude
[ ]  Cowl Flaps .... Closed/As Req'd

Descent
[ ]  Approach Briefing .... Complete
[ ]  Lights .... On
[ ]  Fuel Selector .... Both
[ ]  Cowl Flaps .... Closed
[ ]  Mixture .... Set
[ ]  Power/Prop .... Set

Before Landing
[ ]  Seats / Seatbelts .... Check Secure
[ ]  Fuel Selector .... Both
[ ]  Carb Heat .... On
[ ]  Propeller .... Full forward

Normal Landing
[ ]  Airspeed .... 70-80 KIAS flaps up
[ ]  Flaps .... As required
[ ]  Airspeed .... 65-75 KIAS flaps down

After Landing
[ ]  Cowl Flaps .... Open
[ ]  Trim .... Takeoff
[ ]  Flaps .... Retract
[ ]  Carb Heat .... Off
[ ]  Land, Strobe lights .... Off
[ ]  Transponder .... Standby

Shutdown and Securing
[ ]  Power .... Idle
[ ]  Avionics and Switches .... Off
[ ]  Mixture .... Idle Cutoff
[ ]  Mags .... Off
[ ]  Master .... Off
[ ]  Control Lock .... In
[ ]  Hobbs and Tach .... Record
[ ]  Tie Downs .... Attached
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