Cessna 182S Skylane — N358ME_CESSNA_182_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

BEFORE STARTING ENGINE
[ ]  Preflight inspection .... COMPLETE
[ ]  Seats, Seat Belts, and Shoulder Harnesses .... ADJUST and LOCK
[ ]  Brakes .... TEST
[ ]  Circuit Breakers .... CHECK IN
[ ]  Electrical Equipment .... OFF
[ ]  Avionics Master Switch .... OFF
[ ]  Autopilot .... OFF
[ ]  Cowl Flaps .... OPEN
[ ]  Fuel Selector Valve .... BOTH
[ ]  Avionics Circuit Breakers .... CHECK IN

STARTING ENGINE
[ ]  Throttle .... OPEN 1/4"
[ ]  Propeller .... HIGH RPM
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Propeller Area .... CLEAR
[ ]  Master Switch .... ON
[ ]  Flashing Beacon .... ON
[ ]  Auxiliary Fuel Pump .... ON
[ ]  Mixture .... ADVANCE until fuel flow just starts to rise, then return to IDLE CUT-OFF position
[ ]  Auxiliary Fuel Pump .... OFF
[ ]  Ignition Switch .... START (release when engine starts)
[ ]  Mixture .... Advance smoothly to RICH when engine fires
[ ]  Throttle .... 1000 RPM
[ ]  Oil pressure .... CHECK
[ ]  Mixture .... LEAN one inch for taxi
[ ]  Flaps .... UP
[ ]  Navigation, Cockpit, and Taxi Lights .... ON as required
[ ]  Avionics Master Switch .... ON
NOTE: Communication Radios: DVT / SDL / FFZ; ATIS 126.5 / 118.6 / 118.25; Ground 121.8 / 121.6 / 121.3; Tower S: 118.4 / 119.9 / 124.6, N: 120.2; Practice area 122.75 (north), 122.85 (south)
[ ]  Altimeter .... SET to setting given by ATC
[ ]  Annunciator Panel .... TEST
[ ]  GPS .... Confirm self-test and altimeter setting
[ ]  Transponder .... TEST, then STANDBY
[ ]  Autopilot .... enter altimeter setting
[ ]  Taxiing .... CHECK brakes immediately after airplane begins moving

DURING TURNS WHILE TAXIING
[ ]  Turn Coordinator .... Indicates skidding turn in proper direction
[ ]  Heading Indicator .... Turns in proper direction
[ ]  Magnetic Compass .... Turns in proper direction, bowl full of fluid

BEFORE TAKEOFF
[ ]  Passenger Seat Backs .... MOST UPRIGHT POSITION
[ ]  Seats & Seat Belts .... CHECK SECURE
[ ]  Cabin Doors .... CLOSED and LATCHED
[ ]  Flight controls .... FREE and CORRECT
[ ]  Fuel Quantity .... CHECK
[ ]  Fuel Selector Valve .... RECHECK BOTH
[ ]  Mixture .... FULL RICH
[ ]  Throttle .... 1800 RPM
[ ]  Magnetos .... CHECK (max drop 150 RPM, max diff. 50 RPM)
[ ]  Propeller .... CYCLE from high to low to high RPM
[ ]  Vacuum .... Normal operating range
[ ]  Ammeter .... CHECK
[ ]  Engine Instruments .... CHECK
[ ]  Annunciator Panel .... No warnings illuminated
[ ]  Throttle .... CHECK IDLE
[ ]  Throttle .... 1000 RPM
[ ]  Throttle Friction Lock .... ADJUST
[ ]  Flight instruments .... SET
[ ]  Attitude Indicator .... Check, Set for level flight
[ ]  Vertical Speed Indicator .... Note indication of 0 fpm climb
[ ]  Altimeter .... Should read within 75 ft of field elevation
[ ]  Airspeed Indicator .... indicates 0
[ ]  Pitot heat .... CHECK
[ ]  Elevator & Rudder Trim .... SET for TAKEOFF
[ ]  Communication Radio .... Tower or CTAF
[ ]  Navigation Radios .... SET if flying cross-country
[ ]  NAV/GPS HIS Switch .... SET
[ ]  Autopilot .... OFF
[ ]  Strobe and Landing Lights .... ON
[ ]  Windows .... CLOSED
[ ]  Parking Brake .... OFF
[ ]  Transponder .... ALT

NORMAL TAKEOFF
[ ]  Flaps .... 0°
[ ]  Throttle .... FULL OPEN
[ ]  Airspeed Indicator .... Indicates increasing speed
[ ]  Elevator Control .... Rotate at 60 KIAS

SHORT FIELD TAKEOFF
[ ]  Flaps .... 20°
[ ]  Brakes .... HOLD
[ ]  Throttle .... FULL OPEN
[ ]  Brakes .... RELEASE
[ ]  Climb Speed .... 58 KIAS until obstacles cleared, then as appropriate
[ ]  Flaps .... RETRACT after reaching 70 KIAS

NORMAL CLIMB
[ ]  Airspeed .... 85-95 KIAS
[ ]  Power .... 23" or FULL THROTTLE (whichever is less)
[ ]  RPM .... REDUCE to 2400 RPM
[ ]  Mixture .... 15 GPH or FULL RICH (whichever is less)

CRUISE
[ ]  Power .... 15-23", 2000-2400 RPM (no more than 80% is recommended)
[ ]  Elevator Trim .... ADJUST
[ ]  Mixture .... lean to peak EGT minus 125° F
[ ]  Cowl Flaps .... CLOSED

BEFORE LANDING
[ ]  Passenger Seat Backs .... MOST UPRIGHT POSITION
[ ]  Seats & Seat Belts .... SECURED & LOCKED
[ ]  Fuel Selector Valve .... BOTH
[ ]  Mixture .... RICH
[ ]  Propeller .... HIGH RPM
[ ]  Strobe and Landing Lights .... ON
[ ]  Autopilot .... OFF

NORMAL LANDING
[ ]  Airspeed .... 70-80 KIAS (flaps UP)
[ ]  Flaps .... 0-10° < 140 KIAS, 10°-20° < 120 KIAS, FULL < 100 KIAS
[ ]  Airspeed .... 60-70 KIAS (flaps DOWN)

SHORT OR SOFT FIELD LANDING
[ ]  Flaps .... FULL DOWN (below 100 KIAS)
[ ]  Airspeed .... 60 KIAS

BALKED LANDING
[ ]  Throttle .... FULL OPEN
[ ]  Flaps .... RETRACT TO 20° (immediately)
[ ]  Airspeed .... 55 KIAS (until obstacles are cleared)
[ ]  Flaps .... RETRACT (after reaching a safe altitude and 70 KIAS)
[ ]  Cowl Flaps .... OPEN

AFTER LANDING
[ ]  Flaps .... RETRACT
[ ]  Cowl Flaps .... OPEN
[ ]  Transponder .... STANDBY

SHUTDOWN
[ ]  Call for fuel .... on 130.65 @ DVT
[ ]  Avionics Master Switch .... OFF
[ ]  Electrical Equipment .... OFF (except flashing beacon)
[ ]  Throttle .... IDLE
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Ignition Switch .... OFF (after propeller stops turning)
[ ]  Flashing Beacon .... OFF
[ ]  Master Switch .... OFF
[ ]  Control Lock .... INSTALL
[ ]  Vents .... CLOSED
[ ]  Tiedowns .... SECURED
[ ]  Flight Plan .... CLOSED
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