Cessna 206H Stationair — Sam_Dawson_206_ground_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Before Takeoff" item count differs between passes (22 vs 26); verify nothing was dropped.

Before Starting Engine
[ ]  Preflight Inspection .... Complete
[ ]  CRM/Passenger Briefing .... Complete
[ ]  Seats and Seat Belts .... Adjust & Lock
[ ]  Brakes .... Test & Set
[ ]  Fuel Selector .... FULLEST TANK
[ ]  Cowl Flaps .... OPEN
[ ]  Mixture .... RICH
[ ]  Propeller .... HIGH RPM
[ ]  Avionics Master Switch .... OFF
[ ]  Electrical Equipment .... OFF
[ ]  Circuit Breakers .... Check In

Starting Engine
[ ]  Master Switch .... ON
[ ]  Exterior Lights .... As Required
[ ]  Mixture .... RICH
[ ]  Throttle .... CLOSED
[ ]  Auxiliary Fuel Pump .... LO
[ ]  Propeller Area .... CLEAR
[ ]  Ignition Switch .... START
[ ]  Throttle .... ADVANCE slowly
[ ]  Ignition Switch .... RELEASE after start
[ ]  Throttle .... RESET to idle speed
[ ]  Auxiliary Fuel Pump Switch .... OFF
[ ]  Oil Pressure .... Check

Before Taxi
[ ]  Flaps .... Take Off Position
[ ]  Throttle .... 1000 RPM
[ ]  Avionics Master (Radios) .... On
[ ]  ATIS / AWOS .... Receive
[ ]  Clearance .... Obtain
[ ]  Avionics / Transponder .... Set / SBY
[ ]  Flight Instruments .... Check & Set
[ ]  Engine Instruments .... Check

Taxi
[ ]  Brakes & Steering .... Check
[ ]  Flight Instruments .... Check

Before Takeoff
[ ]  Brakes .... SET
[ ]  Cabin Doors .... Closed & Locked
[ ]  Seats / Seat Belts .... Upright & Secured
[ ]  Flight Controls .... Free & Correct
[ ]  Clock .... Check
[ ]  Fuel Quantity .... Check
[ ]  Fuel Selector .... FULLEST TANK
[ ]  Cowl Flaps .... FULL OPEN
[ ]  Elevator and Rudder Trim .... SET for takeoff
[ ]  Flaps .... SET for Takeoff
[ ]  Flight Instruments .... Check & Set
[ ]  Radios / Avionics .... Set for Departure
[ ]  Mixture .... Enrichen
[ ]  Throttle .... 1700 RPM
[ ]  Mixture .... LEAN for takeoff
[ ]  Magnetos .... Check (drop <150, 50 differential)
[ ]  Propeller .... CYCLE
[ ]  Engine Instruments / Ammeter .... CHECK
[ ]  Vacuum Gage .... CHECK
[ ]  Throttle .... Idle / 1000 RPM
[ ]  Autopilot .... OFF
[ ]  Departure Briefing .... Complete- Type T/O Vr-60 Vy- 100 (-1MPH/1000’) Vx- 78 Power Heading Altitude

Shutdown and Securing
[ ]  Avionics Master Switch .... Off
[ ]  Exterior Lights (except beacon) .... Off
[ ]  Throttle .... 1000 RPM
[ ]  Mixture .... Idle Cut Off
[ ]  Ignition Switch .... Off
[ ]  Battery and Alternator .... Off
[ ]  Gust Lock .... Install
[ ]  Post Flight Inspection .... Accomplish
[ ]  Tie downs and Chocks .... Install
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