Cessna 210_210B Centurion — jochman-clc210b
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Maximum Performance Take-Off" item count differs between passes (9 vs 10); verify nothing was dropped.

Aircraft Performance Speeds
NOTE: VS0 – Landing configuration stall at gross weight, power off     57 MPH
NOTE: VS1 – Cruise configuration stall at gross weight, power off      65 MPH
NOTE: VR       60 MPH
NOTE: VX – Best Angle of Climb Speed       69 MPH
NOTE: VY – Best Rate of Climb Speed        105 MPH
NOTE: VFE – Max. Flap Extension 0-10º      160 MPH
NOTE: VFE – Max. Flap Extension 10-40º     110 MPH
NOTE: VLE – Max. Landing Gear Extension    160 MPH
NOTE: VA – Maneuvering Speed    132 MPH
NOTE: VNO – Top of Green Arc    190 MPH
NOTE: VNE – Red Line – Never Exceed        225 MPH
NOTE: VL/D     95 MPH

Aircraft Specifications
NOTE: Maximum Gross Weight     3000 LBS
NOTE: Basic Empty Weight (N4345X)   1832 LBS
NOTE: Useful Load (N4345X)     1168 LBS
NOTE: Fuel Capacity (useable)  80 GALS
NOTE: Fuel Consumption 75%@2500’    14.3 GPH
NOTE: Oil Capacity   9-12 QTS
NOTE: Tire Pressure – Nose      45 PSI
NOTE: Tire Pressure – Mains     42 PSI

Before Starting Engine
[ ]  Preflight .... Complete
[ ]  Seats and Seat Belts .... Adjust and Lock
[ ]  Brakes .... Test and Set
[ ]  Cowl Flaps .... Open
[ ]  Fuel Selector .... Fullest Tank
[ ]  Lights .... OFF
[ ]  Circuit Breakers .... Check
[ ]  Clock .... Set
[ ]  Altimeter .... Set
[ ]  Controls .... Free & Correct
[ ]  Flaps .... Check
[ ]  Trim .... Set for T/O
[ ]  Radios and Electrical Equipment .... OFF
[ ]  Master Switch .... ON
[ ]  Landing Gear .... Handle Neutral
[ ]  Green DN Light .... ON
[ ]  Landing Gear Lights, Horn .... Press to Test

Starting Engine (COLD)
[ ]  Anti-collision Light .... ON
[ ]  Mixture .... Full Rich
[ ]  Propeller .... High RPM
[ ]  Throttle .... Full Open
[ ]  Propeller Area .... CLEAR
[ ]  Aux. Fuel Pump Switch .... High for 5 Sec.
[ ]  Aux. Fuel Pump Switch .... OFF
[ ]  Throttle .... 50%
[ ]  Ignition Key .... Start
[ ]  Throttle .... Reduce to Idle
[ ]  Oil Pressure .... Check
[ ]  Radios .... ON, Check 121.5
[ ]  Transponder .... Standby
[ ]  Fuel Selector .... Switch Tanks for Taxi
[ ]  Brakes .... OFF
[ ]  Toe Brakes .... Check

Starting Engine (HOT)
[ ]  Anti-collision Light .... ON
[ ]  Mixture .... Idle-Cutoff
[ ]  Propeller .... High RPM
[ ]  Throttle .... Closed
[ ]  Propeller Area .... CLEAR
[ ]  Aux. Fuel Pump Switch .... High for 5 Sec.
[ ]  Throttle .... Open 1”
[ ]  Ignition Key .... Start
[ ]  Mixture .... Push to Full Rich
[ ]  Throttle .... Set to Idle
[ ]  Oil Pressure .... Check
[ ]  Aux. Fuel Pump Switch .... OFF
[ ]  Radios .... ON, Check 121.5
[ ]  Transponder .... Standby
[ ]  Fuel Selector .... Switch Tanks for Taxi
[ ]  Brakes .... OFF
[ ]  Toe Brakes .... Check

Before Take-Off
[ ]  Parking Brake .... SET
[ ]  Cowl Flaps .... Check FULL
[ ]  Flight Controls .... Free and Correct
[ ]  Elevator and Rudder Trim .... TAKE OFF
[ ]  Fuel Selector .... Fullest Tank
[ ]  Throttle Setting .... 1700 RPM
[ ]  Engine Instruments .... Check
[ ]  Ammeter .... Check
[ ]  Suction Gauge .... Check (4.6 to 5.4")
[ ]  Oil Pressure .... Check
[ ]  Oil Temperature .... Check
[ ]  Alternator .... Check
[ ]  Annunciator Panel .... Check
[ ]  Fuel Flow .... Check
[ ]  Magnetos .... Check (50 RPM Max diff.)
[ ]  Propeller .... Cycle
[ ]  Throttle .... Check Idle
[ ]  Flight Instruments and Radios .... SET
[ ]  Autopilot or Wing Leveler .... OFF
[ ]  Cabin Doors, Window .... Closed and Locked
[ ]  Seat Belts/Harness .... Buckled
[ ]  Transponder .... ON ALT, Code Set

Normal Take-Off
[ ]  Wing Flaps .... 0º - 10º
[ ]  Power .... Full Throttle and 2850 RPM
[ ]  Mixture .... Lean for Field Elevation
[ ]  Elevator Control .... Lift nose at 60-70 MPH
[ ]  Climb Speed .... 70 MPH
[ ]  Brakes .... Apply (when airborne)
[ ]  Landing Gear .... Retract (in climb out)
[ ]  Wing Flaps .... Retract (obstacles cleared)

Maximum Performance Take-Off
[ ]  Wing Flaps .... 10º
[ ]  Brakes .... APPLY
[ ]  Power .... Full Throttle and 2850 RPM
[ ]  Mixture .... Lean for Field Elevation
[ ]  Brakes .... RELEASE
[ ]  Elevator Control .... Slightly Tail Low
[ ]  Climb Speed .... 64 MPH
[ ]  Landing Gear and Wing Flaps .... RETRACT (after obstacles are cleared and 90)
NOTE: Note: Do not reduce power until wing flaps and landing gear have been retracted.

Normal Climb
[ ]  Airspeed .... 120 to 140 MPH
[ ]  Power .... 25" and 2550 RPM
[ ]  Mixture .... Lean as Necessary
[ ]  Cowl Flaps .... Open as Required

Maximum Performance Climb
[ ]  Airspeed .... 105 MPH (sea level) to 100 MPH (10,000')
[ ]  Power .... Full Throttle and 2700 RPM
[ ]  Mixture .... Lean for Altitude
[ ]  Cowl Flaps .... Full Open

Cruise
[ ]  Power .... 15-25" of MP, 2200-2550 RPM
[ ]  Power .... no more than 75%
[ ]  Cowl Flaps .... Open as Required
[ ]  Elevator and Rudder Trim .... Adjust
[ ]  Mixture .... Lean for Cruise

Let-Down
[ ]  Power .... As Desired
[ ]  Mixture .... Lean for Smoothness
[ ]  Use Full Mixture for Idle Power
[ ]  Cowl Flaps .... Closed

Before Landing
[ ]  Fuel Selector .... Fullest Tank
[ ]  Landing Gear Level .... DOWN (160 MPH)
[ ]  Landing Gear Light .... GREEN
[ ]  Mixture .... RICH
[ ]  Propeller .... HIGH RPM
[ ]  Wing Flaps .... DOWN
[ ]  0º-10º .... below 160 MPH
[ ]  10º-30º .... below 110 MPH
[ ]  Airspeed .... 85-95 MPH (flaps retracted)
[ ]  Airspeed .... 75-85 MPH (flaps extended)
[ ]  Elevator Trim .... Adjust

Balked Landing (Go Around)
[ ]  Power .... Full Throttle and 2850 RPM
[ ]  Wing Flaps .... Retract to 20º
[ ]  Upon reaching an airspeed of 90 MPH .... retract flaps slowly

Normal Landing
[ ]  Touchdown .... Main Wheels First
[ ]  Landing Roll .... Lower Nose Wheel Gently
[ ]  Braking .... Minimum Required

After Landing
[ ]  Cowl Flaps .... OPEN
[ ]  Wing Flaps .... RETRACT
[ ]  Transponder .... OFF

Securing Aircraft, Stopping Engines
[ ]  Parking Brake .... SET
[ ]  Radios and Electrical Equipment .... OFF
[ ]  Mixture .... Idle Cut-Off
[ ]  Ignition and Master Switch .... OFF
[ ]  Control Lock .... Installed
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