Cessna 401 — Louis_Janos_401_Emergency1_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "ALTERNATOR FAILURE" item count differs between passes (12 vs 10); verify nothing was dropped.
content_gap: Section "ALTERNATOR FAILURE DUAL" item count differs between passes (14 vs 12); verify nothing was dropped.
content_gap: Section "ENGINE INOPERATIVE PROCEDURES" item count differs between passes (22 vs 21); verify nothing was dropped.

ENGINE INOPERATIVE PROCEDURES  [EMERGENCY]
DURING TAKEOFF
[ ]  Throttles .... Closed
[ ]  Brakes .... As Required
AFTER TAKEOFF
[ ]  Mixtures .... Rich
[ ]  Props .... Forward
[ ]  Throttles .... Forward (34.5" MP)
[ ]  Gear .... Up
[ ]  Inoperative Propeller .... Feather
INOPERATIVE ENGINE –SECURE:
[ ]  Throttle .... Close
[ ]  Mixture .... Idle Cutoff
[ ]  Prop .... Feather
[ ]  Fuel Selector .... Off
[ ]  Aux fuel pump .... Off
[ ]  Magnetos .... Off
[ ]  Alternator .... Off
[ ]  Cowl flap .... close
DURING FLIGHT
[ ]  Inoperative Engine .... Secure
[ ]  Operative Engine .... Adjust
[ ]  Electrical Load .... Reduce

LANDING GEAR EMERGENCY  [EMERGENCY]
[ ]  Landing Gear Motor C/B .... Pull
[ ]  Landing Gear Switch .... Neutral (center)
[ ]  Pilot's Seat .... Tilt Aft
[ ]  Hand Crank .... Extend and Lock
[ ]  Rotate Crank .... Clockwise four turns past the point where gear-down  lights come on (approximately 54 turns)
[ ]  Gear .... Check Down
[ ]  Gear Warning Horn .... Check
[ ]  Hand Crank .... Push Button and Stow

OBSTRUCTION/ICING OF STATIC SOURCE  [EMERGENCY]
[ ]  Alternate Static Source .... Open
[ ]  Maintain Altitude and Airspeed

AIR INLET/FILTER ICING  [EMERGENCY]
[ ]  Alternate Air Control .... Pull Out
[ ]  Props .... Increase (2550 RPM)
[ ]  Mixture .... Lean as required

ENGINE DRIVEN INJECTOR PUMP FAILURE  [EMERGENCY]
[ ]  Fuel Selector .... Main Tank
[ ]  Auxiliary Fuel Pump .... High
[ ]  Cowl Flap .... Open
[ ]  Mixture .... Full Rich
[ ]  Land .... As Soon As Practical

ALTERNATOR FAILURE  [ABNORMAL]
indicated by illumination of failure light
[ ]  Reduce load
IF CIRCUIT BREAKER IS TRIPPED
[ ]  Shut off affected alternator.
[ ]  Reset affected alternator circuit breaker .
[ ]  Turn on affected alternator switch.
[ ]  If circuit breaker reopens, turn off alternator.
IF CIRCUIT BREAKER DOES NOT TRIP
[ ]  Select affected alternator on ammeter and monitor output.
[ ]  If output is normal and failure light remains on, disregard fail indication and have indicator checked after landing.
[ ]  If output is insufficient turn off alternator and reduce electrical load to one alternator capacity.
[ ]  If complete loss of alternator output occurs check field fuse and replace if necessary.
[ ]  If an intermittent light indication accompanied by ammeter fluctuation is observed - shut off affected alternator and reduce load to one alternator capacity.

ALTERNATOR FAILURE DUAL  [ABNORMAL]
[ ]  Reset over-voltage protector if out
[ ]  If still inoperative, switch to number 2 regulator
IF STILL INOPERATIVE:
[ ]  Shut off both alternator switches
[ ]  Shut off battery master switch
[ ]  Reduce electrical load to a minimum
[ ]  Turn on emergency power switch
[ ]  Turn on left alternator switch
[ ]  Turn on right alternator switch
IF STILL INOPERATIVE:
[ ]  Turn off emergency power switch
[ ]  Turn off both alternator switches
[ ]  Turn on battery master switch
[ ]  Prepare to terminate flight

AIRCRAFT FIRE ON GROUND  [EMERGENCY]
[ ]  Throttles .... Close
[ ]  Brakes .... As Required
[ ]  Mixtures .... Idle Cutoff
[ ]  Battery .... Off
[ ]  Evacuate Aircraft

IN FLIGHT CABIN FIRE OR SMOKE  [EMERGENCY]
[ ]  Electrical Load .... Reduce
[ ]  Isolate Source .... Attempt
[ ]  Wemacs .... Open
[ ]  Cabin Air Controls .... Open
[ ]  Land .... Evacuate Aircraft

IN FLIGHT WING OR ENGINE FIRE  [EMERGENCY]
[ ]  Auxiliary fuel pumps .... Off
[ ]  Appropriate Engine .... Secure
[ ]  Cabin Heater .... Off
[ ]  Evacuate .... As Soon As Possible
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