Cessna 401 — Louis_Janos_401_Normal_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "AFTER TAKEOFF" item count differs between passes (5 vs 6); verify nothing was dropped.
content_gap: Section "BEFORE TAKEOFF" item count differs between passes (9 vs 8); verify nothing was dropped.
content_gap: Section "CRUISE" item count differs between passes (5 vs 7); verify nothing was dropped.
content_gap: Section "TAKEOFF" item count differs between passes (4 vs 5); verify nothing was dropped.

BEFORE START
[ ]  Preflight Inspection .... COMPLETE
[ ]  Cabin Door .... LATCHED
[ ]  Gear Switch .... DOWN
[ ]  Alternate Air Controls .... FULL IN
[ ]  Alternators and Battery .... ON
[ ]  Control Lock .... REMOVED
[ ]  Flight Controls .... FREE AND CORRECT
[ ]  Cowl Flaps .... OPEN
[ ]  Throttles .... OPEN ONE INCH
[ ]  Props .... FORWARD
[ ]  Mixtures .... RICH
[ ]  Fuel Selectors .... MAIN/TIP TANKS

ENGINE START
[ ]  Magnetos .... ON
[ ]  Left Starter .... PRESS
[ ]  Prime Switch .... APPROPRIATE ENGINE
[ ]  Auxiliary Fuel Pump .... LOW
[ ]  Throttle .... 1000 - 1200 RPM
[ ]  Vacuum System .... CHECK
[ ]  Right Engine .... REPEAT 1 THROUGH 6
[ ]  Lights .... ON
[ ]  Radios .... ON

BEFORE TAKEOFF
[ ]  Trim Tabs .... CHECK MOVEMENT, SET FOR TAKEOFF
[ ]  Controls .... FREE AND CORRECT
[ ]  Cowl Flaps .... OPEN
[ ]  Wing Flaps .... UP
[ ]  Engine Instruments .... NORMAL
[ ]  Instruments and Radios .... CHECK/SET
[ ]  Engine Runup .... CHECK
[ ]  Voltammeter, Vacuum System, Magnetos
[ ]  Feather

TAKEOFF
[ ]  Auxiliary Fuel Pumps .... LOW
[ ]  Landing Lights .... ON
[ ]  Transponder .... ALT
[ ]  Engine Power .... 34.5" MP/2700 RPM, CHECK FUEL FLOW IN WHITE ARC

AFTER TAKEOFF
[ ]  Landing Gear .... UP
[ ]  Engine Power .... 29.5" MP/2450 RPM (1000 FT AGL CHECK FUEL FLOW ON BLUE 75% MARK)
[ ]  Auxiliary Fuel Pumps .... OFF OR AS REQUIRED
[ ]  Fuel selector
[ ]  Voltammeter

CRUISE
[ ]  Engine Power .... 27.0" MP/2300 RPM
[ ]  Mixtures .... LEAN, USE EGT BELOW 75% POWER, SET 100º ROP
[ ]  Cowl Flaps .... CLOSED
[ ]  Fuel Selectors .... AUXILIARY - ONE AT A TIME (AFTER THERE IS ROOM IN THE TIP TANK)
[ ]  Landing Lights .... OFF

DESCENT
[ ]  ATIS
[ ]  Altimeter .... SET
[ ]  Reduce M.P. 1" per minute .... CHECK

APPROACH
[ ]  Fuel Selectors .... MAINS/OUTBOARD TANKS
[ ]  Alternate Air .... CHECK IN
[ ]  Mixtures .... RICH OR AS REQUIRED
[ ]  Auxiliary Fuel Pumps .... LOW
[ ]  Heater .... OFF
[ ]  Landing Lights .... ON
[ ]  Cowl Flaps .... CLOSED
[ ]  Flaps .... DOWN 15º BELOW 180 MPH
[ ]  Gear .... DOWN

BEFORE LANDING
[ ]  Flaps .... DOWN 45º BELOW 160 MPH
[ ]  Gear .... CHECK DOWN
[ ]  Props .... FORWARD

AFTER LANDING
[ ]  Auxiliary Fuel Pumps .... LOW
[ ]  Cowl Flaps .... OPEN
[ ]  Flaps .... UP
[ ]  Transponder .... STBY
[ ]  Trim .... SET FOR TAKEOFF
[ ]  Heater .... CHECK OFF
[ ]  Landing Lights .... OFF

SHUTDOWN
[ ]  Auxiliary Fuel Pumps .... OFF
[ ]  Radios .... OFF
[ ]  Throttles .... IDLE
NOTE: Engine cool 3 min. before shutdown
[ ]  Props .... FORWARD
[ ]  Left Mixture .... IDLE CUTOFF
[ ]  Vacuum System .... CHECK
[ ]  Right Mixture .... IDLE CUTOFF
[ ]  Magnetos .... OFF
[ ]  Battery and Alternators .... SET
[ ]  Parking Brake .... SET
[ ]  Control Lock .... INSTALL
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