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Preflight Inspection
1.
[ ]  Control Lock .... REMOVE and STOW
[ ]  Parking Brake .... N/A
[ ]  All Switches .... OFF
[ ]  Landing Gear Switch .... DOWN
[ ]  Battery Switch .... ON
[ ]  Fuel Gages .... CHECK QUANTITY and OPERATION
[ ]  Flaps .... EXTEND
[ ]  Battery Switch .... OFF
[ ]  Left Fuel Selector .... LEFT MAIN (feel for detent)
[ ]  Right Fuel Selector .... RIGHT MAIN (feel for detent)
[ ]  Trim Tab Controls (3) .... NEUTRAL
[ ]  N/A .... N/A
2.
[ ]  Battery Compartment Cover .... SECURE
[ ]  Wing Locker Baggage Door .... SECURE
[ ]  Flap .... CHECK SECURITY and ATTACHMENT
[ ]  Wing Locker Sump .... DRAIN
[ ]  Control Surface Lock .... REMOVE
[ ]  Aileron and tab .... CHECK CONDITION and FREEDOM OF MOVEMENT
[ ]  Fuel Sump (Main Tank) .... DRAIN
[ ]  Fuel Vent and Sniffle Valve .... CLEAR
[ ]  Fuel Quantity (Main Tank) .... CHECK, CAP SECURE
[ ]  Stall Warning Vane .... CHECK FREEDOM OF MOVEMENT
[ ]  Wing Tie Down .... REMOVE
[ ]  Fuel Quantity (Auxiliary Tank) .... CHECK, CAP SECURE
[ ]  Fuel Sump (Auxiliary Tank and Wing Locker Transfer Line) .... DRAIN
[ ]  Fuel Vent (Wing Locker Tank) .... CLEAR, CAP SECURE
3.
[ ]  Fuel Strainer .... DRAIN
[ ]  Cowl Flap .... SECURE
[ ]  Engine Compartment General Condition .... CHECK
[ ]  Oil Level .... CHECK, MINIMUM 9 QUARTS
[ ]  Propeller and Spinner .... EXAMINE FOR NICKS, SECURITY and OIL LEAKS
[ ]  Cowl Flap .... SECURE
[ ]  Main Gear, Strut, Doors and Tire .... CHECK
[ ]  Leading Edge Air Intake .... CLEAR
[ ]  Cross Feed Line .... DRAIN
4.
[ ]  Baggage Door .... SECURE
[ ]  Nose Gear, Strut, Doors and Tire .... CHECK
[ ]  Pitot Cover (If Installed) .... REMOVE, Pitot Tube - CLEAR
[ ]  Tie Down .... REMOVE
[ ]  Heater Inlet .... CLEAR
[ ]  Baggage Door .... SECURE
5.
[ ]  Crossfeed Line .... DRAIN
[ ]  Leading Edge Air Intake .... CLEAR
[ ]  Main Gear, Strut, Doors and Tire .... CHECK
[ ]  Cowl Flap .... SECURE
[ ]  N/A .... N/A
[ ]  Oil Level .... CHECK, MINIMUM 9 QUARTS
[ ]  Engine Compartment and General Condition .... CHECK
[ ]  Propeller and Spinner .... EXAMINE FOR NICKS, SECURITY and OIL LEAKS
[ ]  Cowl Flap .... SECURE
[ ]  Fuel Strainer .... DRAIN
6.
[ ]  Fuel Vent (Wing Locker Tank) .... CLEAR
[ ]  Fuel Sump (Auxiliary Tank and Wing Locker Transfer Line) .... DRAIN
[ ]  Fuel Quantity (Auxiliary Tank) .... CHECK, CAP SECURE
[ ]  Wing Tie Down .... REMOVE
[ ]  Fuel Quantity (Main Tank) .... CHECK, CAP SECURE
[ ]  Fuel Vent and Sniffle Valve .... CLEAR
[ ]  Fuel Sump (Main Tank) .... DRAIN
[ ]  Aileron .... CHECK CONDITION and FREEDOM of MOVEMENT
[ ]  Control Surface Lock .... REMOVE
[ ]  Flaps .... CHECK SECURITY and ATTACHMENT
[ ]  Nacelle Baggage Door .... SECURE
7.
[ ]  Static Port .... CLEAR
[ ]  Control Surface Lock .... REMOVE
[ ]  Tie Down .... REMOVE
[ ]  Static Port .... CLEAR
[ ]  Cabin Door, General Condition and Security Check

NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
Source: Cessna/401/Louis_Janos_401A_Preflight_checklist.txt
Rights: licensed
Checklist hash: 0ff05bcb9ebef74236ad0470e55a9deca353d603b9b6db9381ae3c3eff71661f
Verify against the aircraft's own approved documentation before use.
