Cirrus SR20 — alexbruzzano_sr20_arnav_checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Preflight — Cabin
[ ]  AROW .... COMPLETED
[ ]  CAPS SAFETY PIN .... REMOVED
[ ]  FIRE EXTINGUISHER .... AVAILABLE
[ ]  EGRESS HAMMER .... AVAILABLE
[ ]  HOBBS METER .... NOTE TIME
[ ]  CIRCUIT BREAKERS .... IN
[ ]  TURN COORDINATOR .... NORMAL
[ ]  AVIONICS POWER .... OFF
[ ]  BATTERY MASTER SWITCH .... ON
[ ]  ANNUNCIATOR LIGHTS .... TEST
[ ]  STANDBY VACUUM .... VERIFY OPS
[ ]  FLAPS .... 100%
[ ]  FUEL QUANTITY .... CHECK
[ ]  FUEL SELECTOR .... FULLEST
[ ]  LIGHTS & PITOT HEAT .... CHECK
[ ]  BATTER MASTER SWITCH .... OFF

Preflight — Left Fuselage
[ ]  COMM 1 & 2 ANTENNA .... CONDITION
[ ]  WING/FUSELAGE FARING .... CHECK
[ ]  BAGGAGE DOOR .... LOCKED
[ ]  STATIC PORT .... CLEAR
[ ]  PARACHUTE COVER .... CONDITION

Preflight — Empennage
[ ]  TIE DOWN .... REMOVED
[ ]  HORIZ/VERT STAB .... CONDITION
[ ]  ELEVATOR .... CONDITION
[ ]  RUDDER .... CONDITION

Preflight — Right Fuselage
[ ]  STATIC PORT .... CLEAR
[ ]  PARACHUTE COVER .... CONDITION
[ ]  WING/FUSELAGE FARING .... CHECK

Preflight — Right Wing
[ ]  FLAP .... CONDITION
[ ]  AILERON .... CONDITION
[ ]  WINGTIP .... CONDITION
[ ]  STROBE/NAV LIGHT .... CONDITION
[ ]  FUEL VENT .... CLEAR
[ ]  LEADING EDGE/STALL STRIPS .... CONDITION
[ ]  FUEL CAP .... QUANTITY/SECURE
[ ]  STALL WARNING .... CLEAR/TEST
[ ]  CABIN AIR VENT .... CLEAR
[ ]  GEAR FARINGS .... CONDITION
[ ]  TIRE (53 psi) .... CONDITION
[ ]  FUEL DRAINS .... SUMP
[ ]  WHEEL BRAKES .... CONDITION
[ ]  CHOCKS .... REMOVE
[ ]  TIE DOWN ROPES .... REMOVE

Preflight — Nose
[ ]  COWLING .... SECURE
[ ]  EXHAUST PIPES .... CONDITION
[ ]  TRANSPONDER ANTENNA .... CONDITION
[ ]  FUEL DRAIN .... SUMP
[ ]  TOW BAR .... REMOVE
[ ]  STRUT .... CONDITION
[ ]  GEAR FARING .... CONDITION
[ ]  TIRE (40 psi) .... CONDITION
[ ]  PROPELLER .... CONDITION
[ ]  SPINNER .... CONDITION/OIL LEAKS
[ ]  AIR INLETS .... CLEAR
[ ]  ALTERNATOR BELT .... CONDITION/TENSION
[ ]  LANDING LIGHT .... CONDITION
[ ]  ENGINE OIL .... CHECK/SECURE
[ ]  EXTERNALN POWER DOOR .... SECURE

Preflight — Left Wing
[ ]  CABIN AIR VENT .... LEAR
[ ]  GEAR FARINGS .... CONDITION TIRE (53 psi)
[ ]  CONDITION .... CONDITION
[ ]  FUEL DRAINS .... SUMP
[ ]  WHEEL BRAKES .... CONDITION
[ ]  CHOCKS .... REMOVE
[ ]  TIE DOWN ROPES .... REMOVE
[ ]  LEADING EDGE/STALL STRIPS .... CONDITION
[ ]  FUEL CAP .... QUANTITY/SECURE
[ ]  FUEL VENT .... CLEAR
[ ]  PITOT TUBE .... CLEAR
[ ]  STROBE/NAV LIGHT .... CONDITION
[ ]  AILERON .... CONDITION
[ ]  FLAP .... CONDITION

Before Starting Engines
[ ]  PREFLIGHT .... COMPLETE
[ ]  PASSENGERS .... BRIEFED
[ ]  SEATS & BELTS .... SECURE
[ ]  BRAKES .... SET
[ ]  STATIC SOURCE .... NORMAL
[ ]  EXTERNAL POWER .... AS REQ

Starting Engine
[ ]  PROPELLER AREA .... CLEAR
[ ]  DOORS .... LATCHED
[ ]  BATTERY MASTER SWITCH .... ON
[ ]  STROBE LIGHTS .... ON
[ ]  MIXTURE .... FULL RICH
[ ]  THROTTLE .... FULL FWD
[ ]  FUEL PUMP .... PRIME THEN BOOST
[ ]  THROTTLE .... IDLE
[ ]  IGNITION SWITCH .... START
[ ]  THROTTLE .... 1000 RPM
[ ]  OIL PRESSURE .... CHECK
[ ]  VACUUM GAUGE .... CHECKED
[ ]  ALTERNATOR .... ON
[ ]  AVIONICS SWITCH .... ON
[ ]  VACUUM ANNUNCIATOR .... OUT
[ ]  AMMETER .... CHECKED
[ ]  ENGINE GAUGES .... CHECKED
[ ]  FUEL PUMP .... OFF
[ ]  EXTERNAL POWER .... DISCONN
[ ]  VACUUM SYSTEM CB .... IN

Cold Start
Cold start
[ ]  MIXTURE .... FULL RICH
[ ]  THROTTLE .... FULL FWD
[ ]  FUEL PUMP .... PRIME 10 SEC THEN BOOST
[ ]  THROTTLE .... OPEN ¼ INCH
[ ]  IGNITION SWITCH .... START
NOTE: continue with normal checklist

Hot Start
Hot start
[ ]  MIXTURE .... FULL RICH
[ ]  THROTTLE .... OPEN ¼ INCH
[ ]  FUEL PUMP .... BOOST
[ ]  IGNITION switch .... START
NOTE: continue with normal checklist

Before Taxi
[ ]  AUTOPILOT .... TEST
[ ]  FLAPS .... UP
[ ]  CABIN HEAT/DEFROST .... SET
[ ]  RADIOS/AVIONICS .... SET
[ ]  LIGHTS .... AS REQUIRED
[ ]  PARKING BRAKE .... RELEASE

Taxi
[ ]  BRAKES & STEERING .... CHECKED
[ ]  INSTRUMENTS .... CHECKED

Before Takeoff
[ ]  BRAKES .... SET
[ ]  SEATS & BELTS .... SECURE
[ ]  DOORS .... LATCHED
[ ]  TRIM .... SET T/OFF
[ ]  FLIGHT CONTROLS .... CHECKED
[ ]  HEADING INDICATOR .... CHECK/SLAVE
[ ]  MIXTURE .... FULL RICH
[ ]  FUEL PUMP .... BOOST
[ ]  FUEL QUANTITY .... CONFIRM
[ ]  FUEL TANK .... SWITCH
[ ]  PROPELLER .... CHECK
NOTE: Oil temp minimum 100°
NOTE: Increase to detent: note 2000 RPM then drop
[ ]  THROTTLE .... 1700 RPM
[ ]  VACUUM GAUGE .... CHECK
[ ]  ENGINE INSTRUMENTS .... CHECK
[ ]  ALTERNATOR .... CHECK
[ ]  MAGNETOS .... CHECK
NOTE: 150 RPM/75 RMP max difference
[ ]  ALTERNATE AIR .... CHECK
[ ]  THROTTLE .... 1000 RPM
[ ]  FLAPS .... 50%
[ ]  COMM/NAV RADIOS .... SET
[ ]  FLIGHT PLAN .... LOADED
[ ]  PITOT HEAT .... AS REQUIRED
[ ]  PARKING BRAKE .... RELEASE

Lineup
[ ]  FINAL .... CLEAR
[ ]  LANDING LIGHT .... ON
[ ]  FLAPS .... SET
[ ]  MIXTURE .... RICH
[ ]  FUEL PUMP .... BOOST
[ ]  TIME OFF .... NOTE

Climb
NOTE: Above 500 AGL
[ ]  FLAPS .... UP
[ ]  ENGINE INSTRUMENTS .... CHECK
[ ]  AIRSPEED .... 105 KIAS
NOTE: Above 1000 AGL
[ ]  FUEL PUMP .... OFF

Cruise
[ ]  CRUISE POWER .... SET
[ ]  MIXTURE .... LEAN
[ ]  ENGINE INSTRUMENTS .... CHECK
[ ]  EXTERNAL LIGHTS .... AS REQUIRED
[ ]  HEADING INDICATOR .... CHECK

Descent
[ ]  BRAKE PRESSURE .... CHECK
[ ]  HEADING INDICATOR .... CHECK
[ ]  ALTIMETER .... SET
[ ]  MIXTURE .... RICH
[ ]  FUEL PUMP .... BOOST
[ ]  FUEL TANK .... FULLEST
[ ]  CABIN HEAT/DEFROST .... AS REQUIRED

VFR Maneuvers
STALL
NOTE: 11"
STEEP TURNS
NOTE: 2100-2300 RPM
NOTE: 120 KIAS
SLOW FLIGHT
NOTE: 11"

Before Landing
[ ]  SEATS & BELTS .... SECURE
[ ]  MIXTURE .... RICH
[ ]  FUEL PUMP .... BOOST
[ ]  FLAPS .... AS REQUIRED
[ ]  LANDING LIGHT .... ON
[ ]  AUTO PILOT .... DISENGAGE

Precision/Non Precision Approach
PRECISION/NON PRECISION APPROACH
NOTE: ►Hold & PT
NOTE: 22" & 120 KIAS
NOTE: ►Pre landing
NOTE: 20" & 100 KIAS
NOTE: ►@ GS INT
NOTE: 17" 50% 100 KIAS
NOTE: ►@ MDA
NOTE: 24" & 100 KIAS

VFR Traffic Pattern
VFR TRAFFIC PATTERN
NOTE: ►Downwind
NOTE: 20" & 100 KIAS
NOTE: ►Abeam
NOTE: 12" 50% 90 KIAS        12" 0% 95 KIAS
NOTE: ►Base
NOTE: 12" 100% 85 KIAS       12" 0% 95 KIAS
NOTE: ►Final
NOTE: 12" 80 KIAS            12" 0% 90 KIAS

After Landing
[ ]  FUEL PUMP .... OFF
[ ]  THROTTLE .... 1000 RPM
[ ]  FLAPS .... UP
[ ]  TRANSPONDER .... STANDBY
[ ]  LIGHTS .... AS REQUIRED
[ ]  PITOT HEAT .... OFF

Engine Shutdown
[ ]  AVIONICS SWITCH .... OFF
[ ]  MIXTURE .... CUTOFF
[ ]  MAGNETOS .... OFF
[ ]  ALL LIGHTS .... OFF
[ ]  BAT & ALT MASTER SWITCH .... OFF
[ ]  CAPS SAFETY PIN .... INSERT
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