Cirrus SR20 — Stephen_Shields_SR20_CHECKLIST_v1.3 (Mar-06)
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "BEFORE TAKEOFF RUNUP" item count differs between passes (16 vs 18); verify nothing was dropped.
content_gap: Section "STARTING ENGINE" item count differs between passes (19 vs 23); verify nothing was dropped.

BEFORE STARTING ENGINE
[ ]  Preflight .... COMPLETED
[ ]  Place ignition keys on dash .... PLACE IGNITION KEYS ON DASH
[ ]  Hobbs Meter .... NOTE TIME IN LOGBOOK
[ ]  Emergency Equipment .... ON BOARD
[ ]  Passengers .... BRIEFED
[ ]  Seats, Seat Belts & Harnesses .... ADJUST & SECURE

STARTING ENGINE
WARNING: KEEP ALL PERSONNEL & STARTING CABLES FREE OF PROPELLER
[ ]  External Power (if applicable) .... CONNECT
[ ]  Brakes .... HOLD
[ ]  Battery Master Switches .... ON
Check voltage
[ ]  Strobe Lights .... ON
[ ]  Mixture .... FULL RICH
[ ]  Power Lever .... OPEN ¼ INCH
[ ]  Fuel Pump .... PRIME (only on cold first start), then BOOST
NOTE: NO BOOST REQUIRED IF ENGINE IS STILL WARM (off less than 60 min. in warm weather, less than 30 min. in cold weather)
[ ]  Propeller Area .... CLEAR
[ ]  Power Lever .... OPEN ¼ INCH
[ ]  Ignition Switch .... START
[ ]  Power Lever .... RETARD TO 1000 RPM
[ ]  Oil Pressure .... CHECK
[ ]  Alt Master Switches .... ON
[ ]  Avionics .... ON
[ ]  Engine Parameters .... MONITOR
[ ]  External Power (if applicable) .... DISCONNECT
[ ]  Ammeter .... CHECK

BEFORE TAKEOFF RUNUP
NOTE: COMING FROM e-checklist
[ ]  Boost Pump .... CONFIRM ON
[ ]  Power Level .... 1700 RPM
[ ]  Alternators .... CHECK
[ ]  Pitot Heat .... ON
[ ]  Avionics .... ON
[ ]  Navigation Lights .... ON
[ ]  Landing Light .... ON (3-5 seconds)
NOTE: May be left on if desired for safety
[ ]  ALT 1 & ALT .... CAUTION LIGHTS OUT & POSITIVE AMPS
[ ]  Voltage .... CHECK
[ ]  Pitot Heat .... OFF
Check for voltage drop
[ ]  Magnetos .... CHECK LH & RH
NOTE: RPM Drop ≤ 150, difference between magnetos ≤ 75 RPM
[ ]  Power Level .... DECREASE TO 1000 RPM
NOTE: RETURN TO e-checklist

SHUT DOWN
[ ]  Avionics Switch .... OFF
[ ]  Fuel Pump .... OFF
[ ]  Ignition Switch .... TOGGLE ON/OFF
[ ]  Mixture .... CUTOFF
[ ]  Magnetos .... OFF (remove keys)
[ ]  Bat-Alt Master Switches .... OFF (right to left)
[ ]  ELT .... TRANSMIT LIGHT OUT
[ ]  CAPS Handle .... INSERT PIN
[ ]  Hobbs Meter .... NOTE TIME IN LOGBOOK
[ ]  Flight Plan .... CLOSE
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