Cirrus SR22 — sr22_checklist_stephen_shirley
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full

Initial
[ ]  Weather & Den. Alt.
[ ]  Weight & Balance
[ ]  Performance Req.
[ ]  Flight Plan
[ ]  A.R.R.O.W. .... CHECK
[ ]  Avionics .... OFF
[ ]  Bat 2 Master .... ON
[ ]  Check Volts .... 23-25V
[ ]  Flap Light .... OFF
[ ]  Bat 1 Master .... ON
[ ]  Fuel Quantity
[ ]  Fullest Tank
[ ]  Flaps .... 100%, Light
[ ]  Check Flaps .... 100%
[ ]  Oil Annunciator .... ON
[ ]  Check Ann. Lights .... CHECK
[ ]  Check Volt .... 23-25V
[ ]  Masters .... OFF
[ ]  Alt. Static .... NORMAL
[ ]  Fire Extinguisher Egress Hammer
[ ]  CAPS pin .... IN
[ ]  Hobbs Time

Exterior Summary
[ ]  Check Fuel / Oil
[ ]  Caps/Drains/Vents
[ ]  Prop/Air Intake
[ ]  Exhaust System
[ ]  Surfaces & Controls
[ ]  Pitot/Static Ports
[ ]  Gear/Tires/Brakes
[ ]  Antennas
[ ]  Ties/Chocks/Doors
[ ]  Final Walk Around

Start
[ ]  Brief Passengers .... COMPLETE
[ ]  Remove CAPS pin .... REMOVE
[ ]  Masters .... ON
[ ]  Strobes .... ON
[ ]  Flaps .... UP
[ ]  Mixture .... RICH
[ ]  Power .... FORWARD
[ ]  PRIME .... 8 BUMPS, BOOST ON
[ ]  Power .... CLOSED
[ ]  Power .... 1/4" IF HOT
[ ]  Clear Propeller .... CLEAR
[ ]  Brakes .... HOLD
[ ]  Ignition .... START
AFTER EACH ATTEMPT:
[ ]  Power .... FORWARD
[ ]  Power .... CLOSED
[ ]  Power .... 1000 RPM
[ ]  Check Oil Pressure
[ ]  Monitor Engine
[ ]  Check Alternator 1
[ ]  Flaps .... UP
[ ]  Avionics .... ON
[ ]  GPS & Autopilot
[ ]  Frequencies
[ ]  ATIS/AWOS
[ ]  Altimeter

Taxi
[ ]  Seatbelts .... SECURE
[ ]  Cabin Heat/Defrost
[ ]  Lights .... AS REQUIRED
[ ]  Check Brakes .... CHECK
[ ]  Check HSI/Comp .... CHECK
[ ]  Check AI/TC .... CHECK

Run-Up
[ ]  Brakes .... HOLD
[ ]  Trim .... TAKEOFF
[ ]  Controls .... FREE & CORR
[ ]  Flaps .... 50% & CHECK
[ ]  Instruments .... CHECK
[ ]  Fuel .... FULLEST TANK
[ ]  Power .... 2000 RPM
[ ]  Check Prop. .... CHECK
[ ]  Power .... 1700 RPM
[ ]  Oil Pressure/Temp.
[ ]  Pitot Heat & Lights
[ ]  Check Alts/Volts .... 28
[ ]  Mags .... <150 DROP, <75 DIFF
[ ]  Power .... 1000 RPM
[ ]  Radios/Clearance
[ ]  Transponder Code
[ ]  Baro setting in Altimeter & S-A
[ ]  Initial altitude & alert in S-A

Taking Active
[ ]  Boost Pump .... ON
[ ]  Flaps .... 50%
[ ]  Mixture .... RICH

Takeoff
[ ]  Pitot Heat
[ ]  Flaps .... 50% & CHECK
[ ]  Lights
[ ]  Boost Pump .... ON
[ ]  Power .... FULL FORWARD
[ ]  Adjust Fuel Flow
[ ]  Engine Instruments
[ ]  Release Brakes .... RELEASE
[ ]  Rotate .... 70-73 KIAS
[ ]  Flaps up .... 80 KIAS
[ ]  Vx 80, Vy 100
[ ]  Normal 110-120

Climb
[ ]  Full Power
[ ]  Fuel Flow per list
[ ]  Engine Instruments
[ ]  Boost Pump .... OFF
[ ]  O2 .... ON AT 8000'

Cruise
[ ]  Set Power
[ ]  Lean as Required
[ ]  Engine Instruments
[ ]  Monitor Fuel Flow
[ ]  EGT 75 ROP~1350
[ ]  Oil temp~200

Descent
[ ]  Set Altimeter .... SET
[ ]  Fuel .... FULLEST TANK
[ ]  Mixture .... FULL RICH
[ ]  Marker Beacons
[ ]  Seatbelts .... SECURE

Before Landing
[ ]  Mixture .... FULL RICH
[ ]  Boost Pump .... ON
[ ]  Flaps .... AS REQUIRED
[ ]  Lights .... AS REQUIRED
[ ]  Autopilot .... OFF
[ ]  Downwind 100
[ ]  Base 90
[ ]  Short Final .... 80 KIAS
[ ]  Short Field .... 77 KIAS
[ ]  Active gentle flare

Clear Active
[ ]  Flaps .... UP
[ ]  Power .... 1000 RPM
[ ]  Pitot Heat .... OFF
[ ]  Trim .... TAKEOFF

Shutdown
[ ]  Record Flight Time
[ ]  Avionics .... OFF
[ ]  Boost Pump .... OFF
[ ]  Mixture .... LEAN/CUTOFF
[ ]  Ignition Switch .... OFF
[ ]  Masters .... OFF
[ ]  Lights .... OFF

Securing
[ ]  Check ELT
[ ]  CAPS pin .... REPLACE
[ ]  Hobbs Time
[ ]  Chocks .... IN
[ ]  Secure Doors
[ ]  Tie Downs/Covers
[ ]  Close Flight Plan

Reference Speeds
[ ]  VR Rotation - 70
[ ]  VX Best Angle – 80
[ ]  VY Best Rate – 100
[ ]  VS0 Stall w/flaps – 59
[ ]  VS Stall w/o flaps – 70
[ ]  Best Glide – 90
[ ]  VO Maximum Turbulence – 133
[ ]  VNO Maximum Cruise – 178
[ ]  VNE Never Exceed – 201
[ ]  VFE Flaps Extended – 104 top of white arc
[ ]  VFE ½ Flaps Ext. – 120
[ ]  Maximum X-Wind Demo – 20

Frequencies
[ ]  UNICOM: 122.7 122.8 122.95 123.0 123.05
[ ]  Multicom: 122.9
[ ]  Air-Air: 122.75 122.85
[ ]  Flight Service: 122.2 122.1 122.6 123.6
[ ]  Flight Watch: 122.0
[ ]  Guard: 121.5

Weights & Fluids
[ ]  MGTOW: 3400 lbs
[ ]  Empty Weight: 2290 lbs
[ ]  Maximum Baggage Cpt: 130 lbs
[ ]  Tire Inflation: Nose 40 +2/-0, Mains 62 +2/-0
[ ]  Oil: Exxon Elite 15W-50, Minimum 6 qts.

Power Loss Immediately After Takeoff  [EMERGENCY]
NO RESTART
[ ]  Best Glide [MEMORY] .... 88 KIAS (87 KIAS 2900 LBS)
[ ]  Mixture [MEMORY] .... CUTOFF
[ ]  Fuel Selector .... OFF
[ ]  Flaps .... DOWN/AS REQUIRED
[ ]  Masters & Ignition Switch .... OFF
[ ]  Power Lever .... IDLE
[ ]  Seatbelts .... SECURED

Power Loss In Flight  [EMERGENCY]
[ ]  Best Glide [MEMORY] .... 88 KIAS (87 KIAS 2900 LBS)
[ ]  Mixture .... FULL RICH
[ ]  Fuel Selector .... SWITCH TANKS
[ ]  Fuel Pump .... BOOST
[ ]  Ignition Switch .... CHECK, BOTH

Engine Airstart  [EMERGENCY]
[ ]  Battery Masters .... ON
[ ]  Power Lever .... 1/2" OPEN
[ ]  Mixture .... CUTOFF
[ ]  Fuel Selector .... SWITCH TANKS
[ ]  Ignition Switch .... BOTH
[ ]  Fuel Pump .... BOOST
[ ]  Alt. Masters .... OFF
[ ]  Starter .... ENGAGE (IF NOT WINDMILLING)
[ ]  Mixture .... SLOWLY INCREASE
[ ]  Power Lever .... SLOWLY INCREASE
[ ]  Alt. Masters .... ON

Forced Landing (Engine Out)  [EMERGENCY]
[ ]  Best Glide [MEMORY] .... 88 KIAS (87 KIAS 2900 LBS)
[ ]  Squawk .... 7700
[ ]  Declare Emergency .... GUARD 121.5
[ ]  Seatbelts .... SECURED
[ ]  ELT .... ON
[ ]  Power Lever .... IDLE
[ ]  Mixture .... CUTOFF
[ ]  Fuel Selector .... OFF
[ ]  Ignition .... OFF
[ ]  Boost Pump .... OFF
[ ]  Flaps .... AS NEEDED
[ ]  Master .... OFF

CAPS Deployment  [EMERGENCY]
[ ]  Minimum Possible Airspeed [MEMORY] .... 133 MAX DEMO'D
[ ]  Mixture .... CUTOFF
[ ]  Remove Cover .... REMOVE
[ ]  Remove Safety Pin .... REMOVE
[ ]  Pull Handle [MEMORY] .... DOWN
[ ]  Mixture .... CHECK/CUTOFF
[ ]  Fuel Selector .... OFF
[ ]  Masters .... OFF
[ ]  Ignition .... OFF
[ ]  Boost Pump .... OFF
[ ]  ELT .... ON
[ ]  Seatbelts .... SECURED
[ ]  Loose Items .... SECURED
[ ]  Cross Arms Across Chest
[ ]  Grasp Harness, Keep Torso Erect
[ ]  Evacuate Quickly

Smoke/Fume Elimination  [EMERGENCY]
[ ]  Heater .... OFF
[ ]  Air Vents .... OPEN, FULL COLD
[ ]  Land ASAP
[ ]  Cabin Doors .... UNLATCH (IF NECESSARY)

Engine Fire During Start  [EMERGENCY]
[ ]  Mixture [MEMORY] .... CUTOFF
[ ]  Fuel Selector [MEMORY] .... OFF
[ ]  Power Lever .... FORWARD
[ ]  Starter .... CRANK

Engine Fire In Flight  [EMERGENCY]
[ ]  Mixture [MEMORY] .... CUTOFF
[ ]  Power Lever .... IDLE
[ ]  Fuel Selector .... OFF
[ ]  Ignition .... OFF
[ ]  Perform Forced Landing Checklist

Wing Fire In Flight  [EMERGENCY]
[ ]  Pitot Heat .... OFF
[ ]  Navigation Lights .... OFF
[ ]  Strobes .... OFF
[ ]  Slip to keep flames away from tank
[ ]  Dive to blow out fire if practicable
[ ]  Land ASAP

Cabin Fire In Flight  [EMERGENCY]
[ ]  Masters .... OFF
[ ]  Heater .... OFF
[ ]  Air Vents .... CLOSED
[ ]  Fire Extinguisher .... ACTIVATE
WHEN FIRE EXTINGUISHED…
[ ]  Air Vents .... OPEN, FULL COLD
[ ]  Avionics .... OFF
[ ]  All other switches .... OFF
[ ]  Land ASAP
[ ]  Master Switches .... ON (ONLY IF REQUIRED)
[ ]  Avionics .... ON (ONLY IF REQUIRED)

Inadvertent Icing  [EMERGENCY]
[ ]  Pitot Heat .... ON
[ ]  Exit Icing Conditions
[ ]  Cabin Heat .... MAXIMUM
[ ]  Windshield Defrost .... FULL OPEN
[ ]  Alternate Induction Air .... ON
[ ]  Land Faster, Consider Reduced/No Flaps

Emergency Descent  [EMERGENCY]
[ ]  Flaps .... UP
[ ]  Power Lever .... IDLE
[ ]  Mixture .... FULL RICH
[ ]  Airspeed .... VNE (201 KIAS)
[ ]  Forward Slip .... IF NECESSARY
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