Cirrus SR22 — sr22_checklist_steve_kahn
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Climb out and level" item count differs between passes (2 vs 4); verify nothing was dropped.
content_gap: Section "Run-up / Pre-take-off" item count differs between passes (17 vs 18); verify nothing was dropped.

Pre-flight Inspection
[ ]  Fuel sump -- 5 drains
[ ]  Fuel tanks -- Check levels
[ ]  O-rings -- Inspect
[ ]  Oil level -- 6 - 8 quarts
[ ]  Tire pressure -- Nose 40; main 62 psi
[ ]  Wheel fairings -- Tight and clean
[ ]  Windshield -- Cleaned
[ ]  Control Surfaces -- Check
[ ]  Prop & spinner -- Check
[ ]  Chocks & ropes -- Remove
[ ]  Pitot cover & cowl plugs -- Off
[ ]  Baggage door -- Closed & locked
[ ]  Pitot heat -- Check
[ ]  Nav, Strobe, landing lights -- Check

Pre-start
[ ]  Circuit Breakers -- In
[ ]  CAPS pin -- Remove
[ ]  Doors locked/Seats -- Secure
[ ]  Seat belts, harnesses -- On
[ ]  Passenger Briefing -- Complete
[ ]  Bat #2 master -- Check 23-25V
[ ]  Flap position light -- Off
[ ]  All Bat-Alt Master switches -- On
[ ]  Strobe light -- On
[ ]  Brakes -- Test and set

Start
[ ]  Mixture -- Rich
[ ]  Throttle -- Full forward
[ ]  Prime -- 5 -10 seconds, then Boost
[ ]  Throttle -- Back to ¼ inch open
[ ]  Propeller area -- Clear
[ ]  Ignition switch -- Start (1000 RPM)
[ ]  Oil pressure -- Check
[ ]  Boost pump -- Off
[ ]  Fuel quantity -- Verify

Pre-taxi
[ ]  Avionics master -- On
[ ]  Ammeter -- Check Alt #1 & Alt #2
[ ]  MFS, Autopilot, GNS 430 -- Check/set
[ ]  ATIS -- Copy
[ ]  Altimeter -- Set
[ ]  Attitude indicator -- Set
[ ]  Parking brake -- Off
[ ]  Flaps -- Check and up
[ ]  Ground Clearance -- Okay

Run-up / Pre-take-off
[ ]  Flight instruments -- Monitor on taxi
[ ]  Flight controls -- Check, full range
[ ]  Elevator/Aileron Trim -- Set for take-off
[ ]  Flaps -- Set to 50%
[ ]  Fuel selector -- Fullest tank
[ ]  Boost pump -- On
[ ]  Throttle -- Increase to detent (2000 RPM)
[ ]  Bring throttle back -- 1700 RPM
[ ]  Load elec. system (w/ pitot & all lights)
[ ]  Check Amps/Volts – both alternators
[ ]  Mags -- 150 rpm max drop; 75 rpm diff.
[ ]  Throttle -- Return to 1000 rpm
[ ]  Transponder -- Set correct code
[ ]  GPS -- Activate flight plan or direct to
[ ]  Autopilot -- Set pre-select as required
[ ]  Pitot heat, lights -- As needed
[ ]  Tower -- Clearance for runway

Climb out and level
NOTE: Note -- Time
[ ]  Compass – Verify runway heading
[ ]  Rotate -- 70 Knots .... 70 KNOTS
[ ]  Flaps up -- 80 Knots .... 80 KNOTS
[ ]  Boost pump -- Off

Climb out and level
[ ]  Cruise alt -- Lean mixture
[ ]  Fuel -- Switch every 30 min; Boost on

Descent & landing
[ ]  ATIS -- Check
[ ]  Mixture -- Rich
[ ]  Auto pilot -- Off
[ ]  Landing lights -- On
[ ]  Flaps & speed -- 50% < 119 knots
[ ]  -100% < 104 knots

After landing
[ ]  Flaps -- Up
[ ]  Boost pump -- Off
[ ]  Flight plan -- Closed

Shutdown
[ ]  Avionics master -- Off
[ ]  Mixture -- Cutoff
[ ]  Magnetos -- Off
[ ]  Bat-Alt Master switches -- Off
[ ]  Lights, de-ice, pitot heat -- Off
[ ]  CAPS pin -- Insert
[ ]  Pitot cover, cowl plugs -- Install
[ ]  Canvass cover / Sun shields -- As needed
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