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BEFORE EXTERIOR
[ ]  GEAR CONTROL LEVER .... DOWN AND LATCHED
[ ]  TORQUE INDICATORS .... 100%
[ ]  DAVTRON CL0CK .... ZEROED
[ ]  ENGINE CONTROL SWITCHES .... ENG OFF
[ ]  OVERHEAD SWITCHES .... OFF OR NORMAL
IF GPU START IS TO BE MADE
[ ]  GROUND START SWITCH .... OFF/SER
[ ]  GPU .... CONNECTED AND ON
[ ]  GROUND START SWITCH .... GPU/PAR
[ ]  RIGHT VOLT/AMMETER .... PUSH FOR VOLTS
NOTE: (26-29 VOLTS LO VOLT LIGHT OUT)
[ ]  BATTERY SWITCH .... ON
[ ]  NAV LIGHTS (NIGHT FLIGHT) .... CHECK THEN OFF
[ ]  TORQUE INDICATORS .... ZERO
[ ]  GEAR POSITION LIGHTS .... 3 GREEN
[ ]  TRIM TABS (3) .... SET TO ZERO
[ ]  HYDRAULIC PRESSURES .... 470 PSI MINIMUM
[ ]  FLAPS .... DOWN
NOTE: FLAPS MUST BE UP FOR ACCURATE HYDRAULIC FLUID LEVEL CHECK AND SYSTEM PRESSURE SHOULD BE ZERO.
[ ]  OIL DOORS .... OPEN
[ ]  PARKING BRAKE .... AS REQUIRED
[ ]  FUEL QUANTITY .... CHECK
[ ]  BATTERY SWITCH .... OFF
[ ]  WINDSHIELD AND WINDOWS .... CHECK
[ ]  EMERGENCY EXIT .... SECURE
[ ]  CABIN COMPARTMENT .... SECURE
[ ]  BEFORE EXTERIOR CHECKLIST .... COMPLETE

EXTERIOR
CLOCKWISE
[ ]  DOOR BAYONET AND SEAL .... CHECK
[ ]  OAT PROBE AND UPPER WING .... CHECK
[ ]  LEFT WINDSHIELD/WIPER .... CHECK
[ ]  NOSE ACCESS .... SECURE
[ ]  LEFT PITOT HEAD .... CHECK
[ ]  LEFT RAM AIR INLET .... CLEAR
[ ]  LEFT LANDING LIGHT .... CHECK
[ ]  NOSE GEAR/DOORS .... CHECK
[ ]  RADOME .... CHECK
[ ]  RIGHT LANDING LIGHT .... CHECK
[ ]  RIGHT RAM AIR INLET .... CLEAR
[ ]  RIGHT PITOT HEAD .... CHECK
[ ]  RIGHT WINDSHIELD/WIPER .... CHECK
[ ]  EMERGENCY EXIT .... SECURE
[ ]  RIGHT INBOARD DEICE BOOT .... CHECK
[ ]  RIGHT WING FUEL SUMP .... DRAIN
[ ]  RIGHT ENGINE AND PROP .... CHECK
[ ]  RIGHT WING .... CHECK
[ ]  RIGHT ENGINE TAILPIPE .... CHECK
[ ]  RIGHT WHEEL WELL .... CHECK
[ ]  RIGHT STRUT, WHEEL AND BRAKE .... CHECK
[ ]  INBOARD FLAP AND HINGE .... CHECK
[ ]  AMBIENT AIR INLET .... CLEAR
[ ]  RIGHT SIDE EJECTOR TUBE .... CLEAR
[ ]  FREON AIR EVAP DRAIN .... CLEAR
[ ]  BATTERY VENT DRAIN .... CHECK
[ ]  ECU INTAKE PORT .... CLEAR
[ ]  RAM AIR INLET SCOOP .... CLEAR
[ ]  OXYGEN BOTTLE .... CHECK AND ON
[ ]  RIGHT STATIC PORTS .... CLEAR
[ ]  ANTENNAS .... CHECK
[ ]  DORSAL FIN .... CHECK
[ ]  VERTICAL AND HORIZONTAL DEICE BOOTS .... CHECK
[ ]  STATIC WICKS .... SECURE
[ ]  ELEVATORS AND TRIM TABS .... CHECK
[ ]  EXTERNAL RUDDER GUST LOCK .... REMOVED
[ ]  RUDDER AND TRIM TAB .... CHECK
[ ]  RUDDER HORN/HEATER .... CLEARANCE
[ ]  TAIL CONE .... CHECK
[ ]  FREON AIR INLET VENT .... CLEAR
[ ]  LEFT SIDE STATIC PORTS .... CLEAR
[ ]  ECU EXHAUST DUCT .... CLEAR
[ ]  FREON AIR EXHAUST .... CLEAR
[ ]  BATTERY VENT INLET .... CLEAR
[ ]  BAGGAGE COMPARTMENT .... CHECK
[ ]  FREON AIR EVAP DRAIN .... CLEAR
[ ]  LEFT INBOARD FLAP HINGE .... CHECK
[ ]  LEFT STRUT, WHEEL, BRAKE AND STRUT SWITCH .... CHECK
[ ]  LEFT WHEEL WELL .... CHECK
[ ]  LEFT TAILPIPE .... CHECK
[ ]  HYDRAULIC QUANTITY .... CHECK
[ ]  LEFT WING .... CHECK
[ ]  LEFT NACELLE, ENGINE AND PROP .... CHECK
[ ]  NITROGEN PRESSURE GAGE .... 425 TO 525 PSI
[ ]  LEFT WING FUEL SUMP .... DRAIN
[ ]  LEFT INBOARD DEICE BOOT .... CHECK
[ ]  EXTERIOR CHECKLIST .... COMPLETE

BEFORE STARTING ENGINES
[ ]  GEAR CONTROL LEVER .... DOWN AND LATCHED
[ ]  ENGINE CONTROL SWITCHES .... ENG OFF
[ ]  FUEL/HYD SWITCHES .... AS REQUIRED
[ ]  GND START SWITCH .... AS REQUIRED
IF GPU START IS TO BE MADE
[ ]  GND START SWITCH .... OFF/SER
[ ]  GPU .... CONNECTED AND ON
[ ]  GND START SWITCH .... GPU/PAR
[ ]  RIGHT VOLT/AMMETER .... PUSH FOR VOLTS
NOTE: (26-29 VOLTS LO VOLT LIGHT OUT)
[ ]  BATTERY SWITCH .... ON
[ ]  OVERHEAD SWITCHES .... SET FOR ENGINE START
[ ]  CABIN BUS .... AS REQUIRED
[ ]  TORQUE LIMITER SWITCHES .... OFF
[ ]  NTS SWITCHES .... TEST
[ ]  PANEL LIGHTS .... AS REQUIRED
[ ]  ANTI-COLLISION LIGHT .... ON
[ ]  BELTS/NO SMOKING SIGN .... ON
[ ]  AUTO START OVERRIDE .... AS REQUIRED
[ ]  CREW MIKE SELECTORS .... AS REQUIRED
[ ]  CREW OXYGEN MASKS .... FITTED, 100%, CHECK FLOW
[ ]  CIRCUIT BREAKER PANELS .... CHECK
[ ]  AURAL WARNING SYSTEMS .... CHECK
[ ]  ENVIRONMENTAL SYSTEM CONTROLS .... SET
[ ]  ENVIR MASTER SWITCH .... NORMAL
[ ]  CABIN DEPRESS SWITCH .... NORMAL
[ ]  TEMP CONTROL KNOB .... AS DESIRED
[ ]  AUTO/OVRD SWITCH .... OFF
[ ]  MAX FLO SWITCH .... OFF
[ ]  BLEED AIR VALVES .... BOTH CLOSED
[ ]  PRESSURIZATION SYSTEM CONTROLS .... SET
[ ]  CABIN RATE CONTROL .... 12 O'CLOCK
[ ]  CABIN ALTITUDE SELECTOR .... 1,000' AGL OR HIGHER
[ ]  CABIN DIFFERENTIAL .... ZERO
[ ]  CABIN ALTITUDE .... FIELD ELEVATION
[ ]  CABIN RATE OF CHANGE .... ZERO
[ ]  LO VOLT LIGHT .... ON WITHOUT GPU
[ ]  CREW AUDIO AND COMPASS PANELS .... SET AND SLAVE
[ ]  ANNUNCIATOR PANEL .... CHECK AND TEST
[ ]  FUEL TOTALIZER .... AS REQUIRED
[ ]  POWER LEVERS .... GND IDLE
[ ]  CONDITION LEVERS .... LO RPM
[ ]  OIL DOORS .... OPEN
[ ]  FLAPS .... UP, INDICATING UP
[ ]  HYD PRESS .... 470 PSI MINIMUM
[ ]  PROP SYNC .... OFF
[ ]  PARKING BRAKE .... AS REQUIRED
[ ]  FUEL QUANTITY .... CHECKED AND BALANCED
[ ]  ELT .... ARMED
[ ]  PASSENGER OXYGEN .... AS REQUIRED
[ ]  OXYGEN PRESSURE .... CHECK
[ ]  BATTERY SWITCH .... IF PAX NOT READY, OFF
[ ]  TAKEOFF DATA .... DETERMINED
[ ]  BEFORE STARTING ENGINES CHECKLIST .... COMPLETE

STARTING ENGINES
[ ]  EXTERNAL GUST LOCK .... STOWED
[ ]  PAX BRIEFING .... AS REQUIRED
[ ]  CABIN DOOR .... CLOSED, LOCKED
[ ]  INTERNAL CONTROL LOCK .... STOWED
[ ]  SEAT BELTS AND HARNESSES .... FASTENED
[ ]  BATTERY SWITCH .... ON
[ ]  DOOR SWITCH .... LOCK, DOOR LIGHT OUT
BATTERY START
[ ]  START MODE .... SELECTED
[ ]  PROPELLER .... CLEAR AND UNFEATHERED
[ ]  EGT .... BELOW 200°C
[ ]  ENGINE CONTROL SWITCH
[ ]  FUEL PUMP ON .... 15 PSI MINIMUM
[ ]  AIR START .... SET LEVER FOR NTS TEST
[ ]  GND START .... NTS LIGHT OUT WITHIN 1 SEC
[ ]  CONDITION LEVER .... READY FOR ABORT
[ ]  EGT AND RPM .... MONITOR
[ ]  OIL PRESSURE .... 40 PSI MIN AT 65% RPM
[ ]  FUEL PRESSURE .... GREEN ARC
[ ]  HYDRAULIC PRESSURE .... 900 TO 1075 PSI
[ ]  ANNUNCIATOR LIGHT .... OFF
[ ]  NTS SWITCH .... OFF
[ ]  TORQUE LIMITER SWITCH .... ON
[ ]  OPERATING ENGINE GENERATOR .... ON
[ ]  ANNUNCIATOR LIGHT .... OFF
[ ]  LO VOLT LIGHT .... OFF
[ ]  AMMETER .... 200 AMPS OR LESS
[ ]  GND START SWITCH .... GPU/PAR
NOTE: REPEAT ITEMS MARKED (**) FOR SECOND ENGINE START
[ ]  OTHER GENERATOR .... ON
[ ]  ANUNCIATOR LIGHT .... OFF
[ ]  LOAD SHARING AND VOLTAGE .... CHECK
GPU START
[ ]  PROPELLER .... CLEAR AND UNFEATHERED
[ ]  EGT .... BELOW 200°C
[ ]  ENGINE CONTROL SWITCH
[ ]  FUEL PUMP ON .... 15 PSI MINIMUM
[ ]  AIR START .... SET LEVER FOR NTS TEST
[ ]  GND START .... LIGHT OUT WITHIN 1 SEC.
[ ]  CONDITION LEVER .... READY FOR ABORT
[ ]  EGT AND RPM .... MONITOR
[ ]  OIL PRESSURE .... 40 PSI MIN AT 65% RPM
[ ]  FUEL PRESSURE .... GREEN ARC
[ ]  HYDRAULIC PRESSURE .... 900 TO 1075
[ ]  ANNUNCIATOR LIGHT .... OFF
[ ]  NTS SWITCH .... NORMAL
[ ]  TORQUE LIMIT SWITCH .... ON
NOTE: REPEAT ITEMS MARKED (**) FOR SECOND ENGINE START
[ ]  GND START SWITCH .... OFF/SER
[ ]  GPU .... DISCONNECTED AND REMOVED
[ ]  GND START SWITCH .... GPU/PAR
[ ]  BOTH GENERATORS .... ON
[ ]  ANNUNCIATOR LIGHTS .... OFF
[ ]  LO VOLT LIGHT .... OUT
[ ]  LOAD SHARING AND VOLTAGE .... CHECK
[ ]  STARTING ENGINES CHECKLIST .... COMPLETE

AFTER START/BEFORE TAXI
[ ]  CABIN BUS .... VERIFY ON
[ ]  RADIO SWITCHES .... ON
[ ]  BUS OFF LIGHTS .... OUT
[ ]  INVERTERS .... CHECKED AND ON
[ ]  AVIONICS SWITCHES .... ON
[ ]  BLEED AIR VALVES .... CHECK AND BOTH OPEN
[ ]  MAX FLO .... AS REQUIRED
[ ]  AUTO/OVRD SWITCH .... AS REQUIRED
[ ]  OIL TEMPERATURE .... GREEN ARC
[ ]  SRL SYSTEM .... CHECK
[ ]  SRL/ P/P SWITCHES .... NORMAL
[ ]  CONDITION LEVERS .... HIGH
[ ]  POWER LEVERS .... 100%
NOTE: OBSERVE RPM JUMP AT 80%
[ ]  EGT .... NOTE VALUE
[ ]  SRL/ P/P SWITCHES .... SRL OFF
[ ]  EGT .... VALUE WITHIN 10 C
[ ]  SRL/ P/P SWITCHES .... NORMAL
[ ]  NTS CHECK VALVE .... CHECK
[ ]  CONDITION LEVERS .... HI RPM
[ ]  POWER LEVERS .... FLT IDLE
[ ]  NTS SWITCH .... TEST
[ ]  NT LIGHTS .... ON
[ ]  NTS TEST LIGHTS .... REMAIN OFF
[ ]  NTS SWITCHES .... OFF
NOTE: TORQUE LIMITER TEST CAN BE PERFORMED AT THIS POINT
[ ]  OVERSPEED GOVERNOR .... CHECK
[ ]  POWER LEVERS (ONE AT A TIME) .... ADVANCE
[ ]  RPM .... 103 TO 105%
CAUTION: DO NOT EXCEED 106% RPM
[ ]  POWER LEVERS .... GND IDLE
[ ]  CONDITION LEVERS .... LO RPM
[ ]  PROPELLERS (ONE AT A TIME) .... UNLOCK
[ ]  POWER LEVERS .... SLIGHTLY INTO REVERSE
[ ]  TORQUE AND FUEL FLOW .... OBSERVE SLIGHT RISE
[ ]  POWER LEVERS .... GND IDLE
[ ]  GYRO PRESSURE .... CHECK
[ ]  HEADING INDICATORS .... CHECKED AND NO FLAGS
[ ]  ATIS AND CLEARANCE .... AS REQUIRED
[ ]  ALTIMETERS AND CLOCKS .... SET
[ ]  AFTER START/BEFORE TAXI CHECKLIST .... COMPLETE

TAXI/BEFORE TAKEOFF
[ ]  TAXI LIGHTS .... AS REQUIRED
[ ]  BRAKES .... CHECK
[ ]  FLIGHT INSTRUMENTS .... CHECKED
[ ]  YAW DAMPER .... CHECKED AND OFF
[ ]  TAXI CHECKLIST .... COMPLETE

BEFORE TAKEOFF
[ ]  FLIGHT CONTROLS .... FREE AND FULL TRAVEL
[ ]  ELECTRIC TRIM AND A/P .... CHECKED AND OFF
[ ]  TRIM TABS (3) .... SET FOR TAKEOFF
[ ]  CIRCUIT BREAKER PANELS .... CHECK
[ ]  MAX FLO SWITCH .... OFF
[ ]  FLAPS .... UP, INDICATING UP
[ ]  FUEL QUANTITY .... RECHECK
[ ]  FUEL INTERCONNECT VALVE .... CHECKED AND CLOSED
[ ]  LOW FUEL PUMPS .... CHECKED AND OFF
[ ]  ENGINE INSTRUMENTS .... CHECK
[ ]  RADIOS AND FLIGHT INSTRUMENTS .... CHECK AND SET
[ ]  ICE PROTECTION .... CHECKED AND OFF
[ ]  CREW BRIEFING .... ACCOMPLISH
[ ]  BEFORE TAKEOFF CHECKLIST .... COMPLETE

LINEUP/TAKEOFF
[ ]  WEATHER RADAR .... AS REQUIRED
[ ]  TRANSPONDER .... ON
[ ]  LANDING AND TAXI LIGHTS .... AS REQUIRED
[ ]  STROBE LIGHTS .... ON
[ ]  UNDERSPEED GOVERNOR .... CHECK
[ ]  CONDITION LEVERS .... HI RPM
[ ]  POWER LEVER .... GND IDLE
[ ]  ENGINE RPM .... 96.5 TO 97.5%
[ ]  POWER LEVERS .... REVERSE SLIGHTLY
[ ]  ENGINE RPM .... 96.5 TO 97.5%
[ ]  TORQUE/TEMP LIMITER TEST .... AS REQUIRED
[ ]  CONDITION LEVERS HIGH .... HI RPM
[ ]  POWER LEVERS .... OBTAIN 100% RPM
[ ]  TORQUE/TEMP LIMITER SWITCHES .... TEST
[ ]  FUEL FLOW AND RPM .... OBSERVE DROP
CAUTION: DO NOT ALLOW RPM TO GO BELOW 65%
[ ]  IGNITION OVERRIDE .... AS REQUIRED
[ ]  PITOT HEAT .... ON
[ ]  ICE PROTECTION .... AS REQUIRED
[ ]  ANNUNCIATOR PANEL .... CONSIDERED
[ ]  LINEUP CHECKLIST .... COMPLETE

TAKEOFF
[ ]  POWER LEVERS .... ADVANCE
[ ]  BETA LIGHTS .... OFF
[ ]  ENGINE RPM .... VERIFY 100%
[ ]  ENGINE INTRUMENTS .... MONITOR
[ ]  ROTATE .... 15° AT 100 KIAS

AFTER TAKEOFF/CLIMB
[ ]  GEAR .... UP AT 200' AGL
[ ]  OIL DOORS .... AS REQUIRED
[ ]  CLIMB POWER .... SET 650 EGT 90% TQ, AND 97 TO 99% RPM
[ ]  PROP SYNC .... ON
[ ]  CLIMB SPEED .... 135 KIAS AT SEA LEVEL DECREASING 1 KT/1,000'
[ ]  IGNITION OVERRIDE .... OFF
[ ]  BELTS/NO SMOKING SIGN .... AS REQUIRED
[ ]  PRESSURIZATION .... CHECK AND ADJUST RATE
[ ]  YAW DAMPER .... AS REQUIRED
[ ]  AFTER TAKEOFF CHECKLIST .... COMPLETE

PASSING 10,000 FEET
[ ]  PRESSURIZATION .... CHECK DIFF AND ALTITUDE
[ ]  LANDING AND TAXI LIGHTS .... OFF

PASSING FL 180
[ ]  ALTIMETERS .... 29.92
[ ]  WINDSHIELD HEAT .... ON
[ ]  OXYGEN SYSTEM .... CHECK
[ ]  PASSENGER OXYGEN .... AUTO
[ ]  OXYGEN PRESSURE .... CHECK
[ ]  CREW MASKS .... CHECK FLOW

CRUISE
[ ]  CRUISE POWER .... SET
[ ]  ANNUNCIATOR PANEL .... TEST PERIODICALLY
[ ]  ICE PROTECTION .... AS REQUIRED
[ ]  OXYGEN SYSTEM .... CHECK
[ ]  PRESSURIZATION .... CHECK
[ ]  LOW FUEL PUMPS .... CHECK AT 600 LBS

DESCENT
[ ]  BELTS SIGN .... ON
[ ]  ICE PROTECTION .... AS REQUIRED
[ ]  WINDSHIELD HEAT .... AS REQUIRED
[ ]  PRESSURIZATION CONTROLS .... SET FOR DESTINATION
[ ]  ATIS INFORMATION .... RECEIVED AND RECORDED
[ ]  LANDING DATA .... DETERMINED
[ ]  ALTIMETER .... SET PASSING FL 180

APPROACH
[ ]  ICE PROTECTION .... AS REQUIRED
[ ]  LANDING LIGHTS .... AS REQUIRED
[ ]  HYDRAULIC PRESURE .... CHECK
[ ]  PRESSURIZATION .... CHECK
[ ]  CREW BRIEFING .... ACCOMPLISH

BEFORE LANDING
[ ]  WINDSHIELD HEAT .... VERIFY OFF
[ ]  IGNITION OVERRIDE .... AS REQUIRED
[ ]  BELTS/NO SMOKING SIGN .... ON
[ ]  RADIO ALTIMETER .... CHECK AND SET
[ ]  CONDITION LEVERS .... HI RPM
[ ]  GEAR .... DOWN AND LOCKED
[ ]  FLAPS .... AS REQUIRED
[ ]  OIL DOORS .... OPEN
[ ]  PROP SYNC (TYPE I) .... OFF
[ ]  YAW DAMPER .... OFF
[ ]  MAX FLO SWITCH .... OFF

AFTER LANDING
[ ]  POWER LEVERS .... GND IDLE
[ ]  CONDITION LEVERS .... LO RPM
[ ]  ICE PROTECTION .... OFF
[ ]  IGNITION OVERRIDE .... OFF
[ ]  STROBE LIGHTS .... OFF
[ ]  LANDING AND TAXI LIGHTS .... AS REQUIRED
[ ]  TRANSPONDER AND WEATHER RADAR .... STANDBY
[ ]  FLAPS .... UP
[ ]  OIL DOORS .... VERIFY OPEN
[ ]  PROP SYNC .... OFF

SHUTDOWN
[ ]  PARKING BRAKE .... AS REQUIRED
[ ]  AUTO/OVRD SWITCH .... OFF
[ ]  AUXILLIARY EQUIPMENT .... OFF
[ ]  AVIONICS SWITCHES .... OFF
[ ]  INVERTER AND RADIO SWITCHES .... OFF
[ ]  GENERATORS .... OFF
[ ]  ENGINES .... SHUTDOWN
[ ]  POWER LEVERS .... GND IDLE
[ ]  ENGINE CONTROL SWITCHES .... ENG OFF
[ ]  POWER LEVERS .... FULL REVERSE AT 50% RPM
[ ]  DOOR SWITCH .... UNLOCK AFTER PROP STOPS

SECURING AIRPLANE
[ ]  OXYGEN SYSTEM .... OFF
[ ]  CREW MASKS .... DISARM AND DISCONNECT
[ ]  OIL DOORS .... CLOSED
[ ]  BATTERY SWITCH .... OFF
[ ]  GND START SWITCH .... OFF/SER
[ ]  PARKING BRAKE .... AS REQUIRED
[ ]  AIRPLANE .... SECURE
[ ]  RUDDER GUST LOCK .... INSTALL
[ ]  TIE DOWN AND CHOCKS .... AS REQUIRED
[ ]  EXTERNAL COVERS .... AS REQUIRED
[ ]  POST FLIGHT INSPECTION .... COMPLETE
[ ]  COURTESY LIGHT .... OBSERVE OFF

GO AROUND
[ ]  F/D GO AROUND MODE .... SELECTED
[ ]  POWER .... MAX ALLOWABLE
[ ]  AIRSPEED .... 100 KIAS
[ ]  FLAPS .... UP-135 KIAS AS FLAPS RETRACT
[ ]  GEAR .... UP WHEN POSITIVE CLIMB
[ ]  OIL DOORS .... AS REQUIRED
[ ]  IGNITION OVERRIDE .... OFF

TAXI BACK
[ ]  FLAPS .... UP
[ ]  TRIM .... 3 TABS SET FOR TAKEOFF
[ ]  RADAR .... STANDBY
[ ]  TRANSPONDER .... STANDBY
[ ]  ICE PROTECTION .... CHECK

QUICK TURN
[ ]  PROPS .... ON LOCKS
[ ]  GND START SWITCH .... PAR
[ ]  EGT .... BELOW 200 C
[ ]  ENGINE .... START
[ ]  GENERATOR .... ON
[ ]  TRIM .... 3 TABS SET FOR TAKEOFF
[ ]  FLAPS .... UP

AIRSPEEDS FOR SAFE OPERATION (KIAS)
CONDITIONS:
NOTE: TAKEOFF WEIGHT-----11,200 LBS
NOTE: LANDING WEIGHT-----10,550 LBS
NOTE: STANDARD DAY-----SEA LEVEL
NOTE: TE CLIMB TO 50 FEET(FLAPS UP/GEAR DOWN)-----102
NOTE: VX (CLEAN)-----95
NOTE: VY (CLEAN)-----135
NOTE: SE CLIMB TO 50 FEET (FLAPS UP/GEAR DOWN)-----98
NOTE: VXSE (CLEAN)-----102
NOTE: VYSE (CLEAN)-----120
NOTE: VSSE-----105
NOTE: VMO-----250
NOTE: VA (10325)-----139
NOTE: THRESHOLD SPEED (FULL FLAPS)-----100
NOTE: TRANSITION TO BALKED LANDING-----100
NOTE: MAX DEMONSTRATED CROSSWIND (TAKEOFF)-----30
NOTE: MAX DEMONSTRATED CROSSWIND (LANDING)-----27
NOTE: VMCA-----93
NOTE: MODERATE TURBULANCE PENETRATION-----180
NOTE: SEVERE/EXTREME TURBULANCE PENETRATION-----VA
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