Diamond DA40 Star — Jacob_Esparza_Diamond_Star_DA40_Pre-Flight_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Front Fuselage" item count differs between passes (9 vs 11); verify nothing was dropped.

Cabin Check
[ ]  Maintenance Check
[ ]  Weight and Balance .... COMPUTED
[ ]  Airplane Documents .... ARROW ON BOARD
[ ]  Ignition Key .... REMOVED
[ ]  Front and Rear canopy .... UNDAMAGED/CLEAN
[ ]  All Electrical Equipment .... OFF
[ ]  Circuit Breakers In
[ ]  Engine Control Levers .... CHECK CONDITION
[ ]  Throttle .... IDLE
[ ]  Mixture .... FULL LEAN
[ ]  Prop .... FULL FORWARD
[ ]  Master Switch (BAT) .... ON
[ ]  Annunciator Panel
[ ]  Fuel Quantity .... CHECK
[ ]  Lights .... ON/CHECK
[ ]  Master Switch (BAT) .... OFF
[ ]  Loose Items Secure
[ ]  Flight Controls .... FREE AND CORRECT
[ ]  Baggage .... SECURED AND STOWED

Left Main Landing Gear
[ ]  Landing Gear Strut
[ ]  Wheel Fairing
[ ]  Tire Pressure .... CHECK 36 P.S.I
[ ]  Tire Wear
[ ]  Tire, Wheel, Brake
[ ]  Brake Line
[ ]  Slip Marks
[ ]  Chocks .... REMOVED

Left Wing
[ ]  Wing Surface
[ ]  Step
[ ]  Lower Surface Air Intake
[ ]  Lower Surface Openings .... CHECK FOR FUEL
[ ]  Fuel Sump
[ ]  Stall Warning
[ ]  Tank Filler .... VISUALLY CHECK
[ ]  2 Stall Strips on Wing .... CHECK
[ ]  Pitot Tube .... CLEAN ORFICES OPEN
[ ]  Landing/Taxi Light
[ ]  Wing Tip
[ ]  Strobes and Position Lights
[ ]  Mooring .... CHECK CLEAR
[ ]  Aileron and Linkages
[ ]  Foreign Objects in Aileron Paddle .... REMOVE
[ ]  Flap and Linkages
[ ]  Flap Hinges and Safety Pin

Left Fuselage
[ ]  Canopy, left side .... CHECK
[ ]  Rear Cabin Door and Window
[ ]  Fuselage Skin
[ ]  Antennas

Empennage
[ ]  Stabilizers and control surfaces
[ ]  Hinges
[ ]  Elevator Trim Tab
[ ]  Rudder Trim Tab
[ ]  Mooring on fin .... CHECK CLEAR
[ ]  Tail Skid and lower fin

Right Fuselage
[ ]  Fuselage Skin
[ ]  Window
[ ]  Canopy, Right Side .... CHECK

Right Wing
[ ]  Flap and Linkage
[ ]  Flap hinges and safety pin
[ ]  Aileron and Linkages
[ ]  Aileron hinges and safety pin
[ ]  Foreign objects in aileron paddle .... REMOVE
[ ]  Wing tip
[ ]  Position and Strobe Lights
[ ]  Mooring .... CHECK CLEAR
[ ]  Wing Surface
[ ]  2 Stall Strips on Wing .... CHECK
[ ]  Tank Filler .... VISUALLY CHECK
[ ]  Lower Surface Openings .... CHECK FOR FUEL
[ ]  Fuel Sump
[ ]  Step

Right Main Landing Gear
[ ]  Landing Gear Strut
[ ]  Wheel Fairing
[ ]  Tire Inflation .... CHECK 36 PSI
[ ]  Tire Wear and Depth
[ ]  Tire Wheel Brake
[ ]  Brake Line .... CHECK FOR LEAKS
[ ]  Slip Marks
[ ]  Chocks .... REMOVE

Front Fuselage
[ ]  Oil Level .... MIN 4 QTS FOR VFR / MIN 6 QTS FOR IFR
[ ]  Cowling
[ ]  3 Air Intakes .... CLEAR
[ ]  Propeller .... MAX BLADE SHAKE 3 MM / MAX ANGULAR PLAY 2°
[ ]  Spinner and Screws
[ ]  Nose Gear
[ ]  Tire and Wheel
[ ]  Slip Marks
[ ]  Tire Wear and Depth

Front Fuselage (cont)
[ ]  Wheel Fairing
[ ]  Tow Bar .... REMOVED
[ ]  Tire Pressure .... CHECK 29 PSI
[ ]  Chocks .... REMOVE
[ ]  Exhaust

Underside
[ ]  Antennas (if fitted) .... CHECK
[ ]  Gascolator .... STRAIN
[ ]  Venting Pipes .... CHECK FOR BLOCKAGE
[ ]  Fuselage Underside .... CHECK FOR FLUIDS

Happy Flying!!!
NOTE: Happy Flying!!!
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