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Before Starting Engine
[ ]  Preflight Inspection .... Complete
[ ]  Rudder Pedals .... Adjusted/locked
[ ]  CRM/Passenger Brief .... Complete
[ ]  Safety Harnesses .... On/Fastened
[ ]  Baggage .... Check/secured
[ ]  Rear Door .... Closed/secured
[ ]  Door Lock .... Unlocked, key removed
[ ]  Front canopy .... Position 1 or 2
[ ]  Canopy Lock .... Unblocked
[ ]  Parking Brake .... Set
[ ]  Flight Controls .... Free
[ ]  Trim Wheel .... TO
[ ]  Throttle .... Idle
[ ]  RPM Lever .... HIGH RPM
[ ]  Mixture Control Lever .... Lean
[ ]  Friction device, throttle .... Adjusted
[ ]  Alternate Air .... Closed
[ ]  Alternate Static Valve .... Closed
[ ]  Avionics Master .... OFF
[ ]  Essential Bus Switch .... OFF
[ ]  Master Switch (BAT) .... ON
[ ]  Fuel Tank Selector .... Fullest Tank

Starting Engine (cold)
[ ]  Strobe Light .... ON
[ ]  Electrical Fuel Pump .... ON (check noise)
[ ]  Throttle .... 1.2” forward
[ ]  Mixture Control Lever .... Rich 3-5 sec, then LEAN
[ ]  Throttle .... IDLE
[ ]  Ignition Switch .... START
WHEN ENGINE STARTS:
[ ]  Mixture Control Lever .... Rapidly to RICH
[ ]  Oil Pressure .... Green within 15 Seconds
[ ]  Electric Fuel Pump .... OFF
[ ]  ALTernator Switch .... ON
[ ]  Ammeter .... Check
[ ]  Fuel Pressure .... Check No MSG
[ ]  Annunciator Section of PFD .... Check

Starting Engine (warm)
[ ]  Strobe Light .... ON
[ ]  Electrical Fuel Pump .... ON (check noise)
[ ]  Throttle .... 1.2” forward
[ ]  Mixture Control Lever .... Rich 1-3 sec, then LEAN
[ ]  Ignition Switch .... START
WHEN ENGINE STARTS:
[ ]  Mixture Control Lever .... Rapidly to RICH
[ ]  Oil Pressure .... Green within 15 Seconds
[ ]  Electric Fuel Pump .... OFF
[ ]  ALTernator Switch .... ON
[ ]  Ammeter .... Check
[ ]  Fuel Pressure .... Check No MSG
[ ]  Annunciator Section of PFD .... Check

Before Taxi Check
[ ]  Avionics Master .... ON
[ ]  PFD .... NO AUTOPILOT ANNUCIATIONS
[ ]  Autopilot Disconnect Tone .... NOTE
[ ]  Electrical Equipment .... On as required
[ ]  Flaps .... UP-T/O-LDG-T/O (indicator/visual check)
[ ]  Flood light .... On, Test as Req.
[ ]  Ammeter .... Check
[ ]  Fuel Tank Selector .... Change tanks, confirm engine runs 1 min @1500RPM
[ ]  Pitot Heating .... On, test (no annunciator)
[ ]  Pitot Heating .... OFF
[ ]  Lights .... Check
[ ]  Throttle .... Check 600-800 RPM
[ ]  ATIS/AWOS/ASOS .... Obtain
[ ]  Flight Instruments/avionics .... Set
[ ]  Altimeters .... Set (both)
[ ]  Clearance .... Obtain
[ ]  Fuel Totalizer .... Check, set
[ ]  Flight Plan .... Set, check

Taxi Check
[ ]  Brakes .... Test
[ ]  Flight Instruments .... Check

Run Up
[ ]  Parking Brake .... Set
[ ]  Rear Door .... Check closed/locked
[ ]  Front Canopy .... Closed, locked
[ ]  Safety Harnesses .... ON/Fastened
[ ]  Flight Controls .... Free, correct
[ ]  Trim .... Check T/O
[ ]  Fuel Tank Selector .... Fullest Tank
[ ]  Circuit Breakers .... IN
[ ]  Flaps .... Check T/O
[ ]  Engine Instruments .... Green Sector
[ ]  Door Warning Light .... Check ext.
[ ]  Fuel Pressure .... Check NO MSG
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture Control Lever .... RICH (below 5000’DA)
[ ]  Throttle .... 2000 RPM
[ ]  Magneto .... Check (175±50 RPM)
[ ]  RPM Lever .... Cycle 3x (max 500RPM)
[ ]  Throttle .... 1000 RPM
[ ]  Parking Brake .... Release
[ ]  Lights .... On as required

Engine Shut-Down
[ ]  Parking Brake .... Set
[ ]  Engine Instruments .... Check
[ ]  Avionics Master Switch .... OFF
[ ]  All Electrical Equipment .... OFF
[ ]  Throttle .... 1000 RPM
[ ]  Ignition Check .... OFF until RPM Drop; the BOTH
[ ]  Mixture Control Lever .... LEAN- shut engine off
[ ]  Ignition Switch .... OFF
[ ]  Master Switch .... OFF
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