Diamond DA40 Star — Sam_Dawson_DA40_InFlight_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "After Landing" item count differs between passes (8 vs 7); verify nothing was dropped.

BEFORE TAKEOFF (FINAL ITEMS)
[ ]  Heading .... Aligned w/ runway
[ ]  Altitude .... Correct
[ ]  Transponder .... ALT
[ ]  Taxi, Landing/Strobe Lights .... On
[ ]  Time .... Note

CLIMB CHECK
[ ]  Flaps .... UP
[ ]  Airspeed .... 80 KIAS
[ ]  RPM .... 2400 RPM
[ ]  Throttle .... MAX POWER
[ ]  Mixture .... RICH; above 5000’ hold EGT constant
[ ]  Engine Instruments .... In Green
[ ]  Trim .... As Required
[ ]  Electrical Fuel Pump .... ON at high Altitude

CRUISE CHECK
[ ]  Flaps .... UP
[ ]  Throttle .... Set
[ ]  RPM .... 1800-2400 RPM
[ ]  Mixture .... SET IAW p. 4A.3.10
[ ]  Trim .... As Required
[ ]  Fuel Tank Selector .... As Required
[ ]  Electrical Fuel Pump .... On at high altitude

DESCENT CHECK
[ ]  Mixture .... Adjust
[ ]  RPM .... 1800-2400
[ ]  Throttle .... As Required
[ ]  Electrical fuel pump .... ON at high altitude
[ ]  ATIS .... Obtain
[ ]  LIGHTS .... On
[ ]  Avionics .... Set
[ ]  Approach Briefing .... Complete
TURN-TIME-TWIST-TAP-THROTTLE-TALK
NOTE: Vr- 59, Vx-66, Vy-73, Vfe-108/91, VA-108/94, Vref-71/67, Glide-73, VNO-129, VNE- 178
NOTE: 22 January 2007

Approach Brief (bold items for VFR)
[ ]  Approach .... Type, Runway
[ ]  GPS .... Set
[ ]  Frequency .... Set, ID
[ ]  Final Approach Course
[ ]  FAF
[ ]  DH/MDA
[ ]  Approach Lights/PAPI/VASI .... Pilot activated?
[ ]  TDZE, HAT/HAA
[ ]  MAP- time, DME, GPS WP? .... Note if GPS WP or DME
[ ]  Missed Approach Procedure .... Review
[ ]  Notes .... Review
[ ]  Runway exit/taxi plan .... Review Direction
[ ]  Terrain .... Highest/MSA
[ ]  Before Landing Check .... To the line
[ ]  Min. Alt., MAP & Climb Out .... Complete

BEFORE LANDING CHECK
[ ]  Fuel Selector .... Fullest Tank
[ ]  Electrical Pump .... ON
[ ]  Safety Harness .... fastened
[ ]  Airspeed .... Reduce to flaps speed
[ ]  Flaps .... T/O (if desired)
[ ]  Trim .... As required
[ ]  Landing light .... As Required
----------------------------SHORT FINAL---------------------------------------
[ ]  Mixture .... Rich (below 5000’ DA)
[ ]  RPM .... HIGH RPM
[ ]  Airspeed .... Reduce to flap speed
[ ]  Flaps .... LDG
[ ]  Approach Speed .... 71/67/63/58

GO AROUND
[ ]  Throttle .... MAX PWR, Press GA, Verify GA/GA in PFD
[ ]  Airspeed .... 66 KIAS
[ ]  Flaps .... TO
[ ]  RPM Lever .... 2400
[ ]  Airspeed .... 73
[ ]  Flaps .... UP
[ ]  Electrical Pump .... OFF
[ ]  Altitude Pre-select .... SET
[ ]  GPS .... Set

After Landing
[ ]  Fuel Pump .... Off
[ ]  Transponder .... Confirm OFF
[ ]  Pitot Heat .... Off
[ ]  Avionics .... As required
[ ]  Lights .... As Required
[ ]  Flaps .... UP
TURN- TIME-TWIST-TAP-THROTTLE-TALK
NOTE: 22 January 2007
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