Fokker 100 — MAX_Fokker100-650_Check
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "TAKEOFF" item count differs between passes (18 vs 19); verify nothing was dropped.

BEFORE START
[ ]  Seat Belt - No SMKG .... ON
[ ]  Fuel Quantity .... CHECKED
[ ]  Altimetars .... SET
[ ]  Ship's Papers .... ON BOARD
[ ]  FMP .... SET
[ ]  L-R FMS .... SET
[ ]  MFDS/TRP .... SET
[ ]  Nav/Com .... SET
[ ]  Parking Brake .... SET
[ ]  L-R Windows And Doors .... CLOSED

CLEARED FOR ENGINE START
[ ]  ENG Anti-Icing .... Check OFF
[ ]  Beacon .... ON
[ ]  Engine Panel .... SET
[ ]  Fuel Pumps .... ON
[ ]  Windows And Probe Heat .... ON
[ ]  Bleed Press .... CHECK
[ ]  Thrust Levers .... FWD IDLE
[ ]  Start Engines

AFTER START
[ ]  Anti-Icing .... SET
[ ]  Engine Panel .... CHECKED
[ ]  Alert Lights .... OUT
[ ]  Flaps .... SET FOR TAKEOFF
[ ]  Fuel Levers .... CHECKED OPEN
[ ]  Trims .... SET
[ ]  Door Selector .... AUTOMATIC

DURING TAXI/BEFORE TAKEOFF
[ ]  Flight Instruments .... CHECKED
[ ]  FMP .... SET
[ ]  ABS .... RTO
[ ]  Brake Temperatures .... CHECKED
[ ]  TO Data And Breifing .... COMPLETED
[ ]  Flight Controls .... CHECKED
[ ]  Radar And Transponder .... AS REQUIRED

CLEARED FOR TAKEOFF
[ ]  APU .... AS REQUIRED
[ ]  TO Config .... CHECKED

TAKEOFF
[ ]  Brakes .... RELEASE
[ ]  Thrust Levers .... ADVANCE SMOOTHLY TO 40% N1
[ ]  Thrust Levers .... ADVANCE SMOOTHLY TO 100% N1
--OR--
[ ]  TO/GA Mode
Engage
[ ]  Engine Instruments .... MONITOR
[ ]  Airspeed 80 KIAS .... CALLOUT "80 KNOTS"
[ ]  Airspeed V1 .... CALLOUT "V1"
[ ]  Airspeed VR .... CALLOUT "ROTATE"
[ ]  Airspeed V2 .... CALLOUT "V2"
[ ]  Landing Gear .... UP (WHEN POSITIVE CLIMB ESTABLISHED)
[ ]  Airspeed .... 250 KIAS AT 3,000' AGL
MAINTAIN V2+20 KIAS
[ ]  Autopilot .... ENGAGE AT 1,000' AGL
[ ]  Flaps .... UP AT 210 KIAS
[ ]  Autothrottle .... OFF
[ ]  Thrust Levers .... 90% N1
[ ]  Airspeed .... 250 KIAS AT 3,000' AGL
[ ]  Landing Gear Lever .... Verify OFF

AFTER TAKEOFF
[ ]  MFDS .... CHECKED
[ ]  Altimeters .... SET

CLIMB
[ ]  Airspeed .... MAINTAIN 250 KIAS
[ ]  Landing Lights .... OFF ABOVE 10,000' MSL
[ ]  Airspeed .... 280 KIAS ABOVE 10,000' MSL
[ ]  Seat Belt .... OFF ABOVE 10,000' MSL

CRUISE
[ ]  Thrust Levers .... AS DESIRED
[ ]  Trim .... AS NECESSARY

BEFORE APPROACH/DESCENT
[ ]  Seat Belt .... ON BELOW 10,000' MSL
[ ]  Landing Alt .... CHECKED
[ ]  Ignition .... AS REQUIRED
[ ]  ABS .... AS REQUIRED
[ ]  MFDS .... CHECKED
[ ]  Altimeters .... SET
[ ]  Landing Data/Approach Briefing .... COMPLETED
[ ]  Airspeed .... <250 KIAS BELOW 10,000' MSL
[ ]  Landing Lights .... ON BELOW 10,000' MSL

APPROACH
[ ]  Airspeed .... AS DESIRED
[ ]  Thrust Levers .... AS DESIRED
[ ]  Flaps .... AS DESIRED
[ ]  Autopilot .... AS DESIRED

LANDING
[ ]  Landing Gear .... DOWN
[ ]  Flaps .... SET
[ ]  Lift Dampers .... ARMED
NOTE: (use Shift+T)

LANDING ROLL
[ ]  Thrust Levers .... IDLE
[ ]  Autopilot .... CHECK DISENGAGED
[ ]  Autothrottle .... CHECK OFF
[ ]  Lift Dumpers .... CHECK FULL UP
[ ]  Brake .... AS REQUIRED
[ ]  Thrust Levers .... REVERSE
[ ]  Thrust Levers .... IDLE AT 60 KIAS

TAXI-IN
[ ]  Lift Dumpers .... DOWN
[ ]  Flap Lever .... UP
[ ]  Pitot Heat .... OFF
[ ]  Landing Lights .... AS DESIRED
[ ]  Flight Director .... OFF
[ ]  Transponder .... AS REQUIRED

PARKING
[ ]  Parking Brake .... AS REQUIRED
[ ]  Door Selector .... MANUAL
[ ]  APU .... AVAILABLE
[ ]  Speed Brake And Lift Dumpers .... IN
[ ]  Flaps .... SET
[ ]  RADAR .... CHECK OFF
[ ]  Anti-Icing .... OFF
[ ]  Fuel Levers .... SHUT
[ ]  Flight Controls .... LOCKED
[ ]  Seat Belt .... OFF
[ ]  Exterior Lights .... CHECK
[ ]  Fuel Pumps .... OFF
[ ]  Air Conditioning .... SET
[ ]  EFIS .... OFF
[ ]  MFDS .... CHECKED

FINAL STOP
[ ]  APU .... OFF
[ ]  BATTERIES .... OFF
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