Fuji FA-200 — fuji_fa200_KARI_Checklist
NOT FOR FLIGHT — source fidelity: unreviewed | operational review: none | completeness: full
content_gap: Section "Engine Start (COLD)" item count differs between passes (23 vs 17); verify nothing was dropped.
content_gap: Section "Normal Operating Speeds at MTOW 2335lb" item count differs between passes (39 vs 22); verify nothing was dropped.

Normal Operating Speeds at MTOW 2335lb
TAKE OFF 15° FLAP (NORMAL)
[ ]  VR .... 48 kts
CLIMB OUT CLEAN BEST RATE
[ ]  VY .... 71 kts
CRUISE %POWER
[ ]  Keep engine temp below 200°C .... 50-70
[ ]  Max rpm .... 2700
LANDING BASE LEG 15° FLAP
[ ]  Landing Base Leg 15° Flap .... 78 kts
FINAL 35° FLAP
[ ]  Final 35° Flap .... 70 kts
THRESHOLD
[ ]  Threshold .... 65 kts
MAX CROSSWIND
[ ]  Max Crosswind .... 15 kts
STALLING 35° FLAPS
[ ]  Stalling 35° Flaps .... 50 kts
25° FLAPS
[ ]  VS1 .... 52 kts
CLEAN
[ ]  VSO .... 59 kts
NOTE: Warner operates @ 4-9 kts > stall
NOTE: Caution - Stall Speed increases sharply with bank angle
25° FLAP STALL SPEED @ 45° BANK
[ ]  25° Flap stall speed @ 45° bank .... 63 kts
CLEAN STALL SPEED @ 45° BANK
[ ]  Clean stall speed @ 45° bank .... 70 kts
MINIMUM WINDMILL GLIDE
[ ]  Minimum Windmill Glide .... 82 kts
25° OR 35° FLAPS EXTENDED
[ ]  VFE .... 103 kts
DESIGN MANEUVERING SPEED
[ ]  VA .... 116 kts
15° FLAPS EXTENDED - WHITE ARC
[ ]  VFO .... 121 kts
NORMAL OPERATIONS – GREEN ARC
[ ]  VNO .... 128 kts
NEVER EXCEED – RED LINE
[ ]  VNE .... 145 kts

Engine Failure During Takeoff Run  [EMERGENCY]
[ ]  Throttle .... IDLE
[ ]  Brakes .... APPLY
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF

Engine Failure Immediately After Takeoff  [EMERGENCY]
[ ]  Airspeed .... MAINTAIN MIN 85 kts
[ ]  Fuel Selector Valve .... SWITCH TANKS
[ ]  Electric Fuel Pump .... ON
[ ]  Mixture .... RICH
[ ]  Carburettor Heat .... ON

Engine Failure During Flight  [EMERGENCY]
[ ]  Airspeed .... MIN 85 kts
[ ]  Carburettor Heat .... ON
[ ]  Electric Fuel Pump .... ON
[ ]  Fuel Selector Valve .... SWITCH TANKS
[ ]  Mixture .... RICH
[ ]  Magnetos .... BOTH
[ ]  Primer .... IN & LOCKED
[ ]  Master Switch .... ON
NOTE: If engine failure was caused by fuel exhaustion, power will not be regained after tanks are switched until empty fuel lines are filled, which may require up to ten seconds.

Landing w/o Engine Power  [EMERGENCY]
[ ]  Airspeed .... MIN 85 kts ON FINALS
[ ]  Radio .... MAYDAY on 121.5 MHz
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Fuel Selector Valve .... OFF
[ ]  Magnetos .... OFF
[ ]  Master Switch .... OFF
[ ]  Door .... OPEN
NOTE: Touchdown should be made at lowest possible airspeed with full flaps.

Electrical Fire in Flight  [EMERGENCY]
[ ]  Master Switch .... OFF
[ ]  Vents .... OPEN
[ ]  Cabin Heat and Air .... OFF
[ ]  All Electrics .... OFF
[ ]  Master Switch .... ON
[ ]  Switch on Essential Eqpt .... ONE BY ONE
[ ]  Fire .... CHECK AFTER EACH ITEM
[ ]  Land .... AS SOON AS POSSIBLE

Engine Fire in Flight  [EMERGENCY]
[ ]  Fuel Selector Valve .... OFF
[ ]  Throttle .... CLOSED
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Cabin Heat and Air .... OFF
[ ]  Defroster .... OFF
[ ]  Forced Landing .... EXECUTE

Engine Fire During Start On Ground  [EMERGENCY]
[ ]  Cranking .... CONTINUE
IF ENGINE STARTS:
[ ]  Power .... 1800 RPM for a few minutes
[ ]  Engine .... SHUTDOWN & INSPECT
[ ]  a. Fuel Pump .... OFF
[ ]  b. Fuel Selector .... OFF
[ ]  c. Master Switch .... OFF
[ ]  d. Magnetos .... OFF
IF ENGINE FAILS TO START:
[ ]  Passengers .... EVACUATE
[ ]  Engine .... SECURE
[ ]  a. Fuel Pump .... OFF
[ ]  b. Mixture .... IDLE CUT-OFF
[ ]  c. Master Switch .... OFF
[ ]  d. Magnetos .... OFF
[ ]  e. Fuel Selector Valve .... OFF
[ ]  Fire .... EXTINGUISH

Cockpit
[ ]  Tech Log + Weight / Balance .... CHECK
[ ]  Tacho Hours .... CHECK & RECORD
[ ]  Transparencies .... CLEAN
[ ]  Control Locks .... REMOVE
[ ]  Fire Extinguisher .... SECURE / GREEN ARC
[ ]  First Aid Kit .... PRESENT / SECURE
[ ]  Master Switch .... ON
[ ]  Fuel Quantity Gauges .... CHECK
[ ]  Anti-Collision Beacon .... CHECK
[ ]  Landing / Taxi Lights .... CHECK
[ ]  Nav Lights .... CHECK
[ ]  Stall Warner .... CHECK
[ ]  All Lighting Switches .... OFF
[ ]  Master Switch .... OFF
[ ]  Magnetos .... OFF, KEYS REMOVED
[ ]  Flaps .... 40°

Port Wing
[ ]  Fuel Tank .... DIP, CAP SECURE
[ ]  Tank Drain .... DRAIN, SECURE
[ ]  Fuel Sample .... PROPER COLOR
[ ]  Gear, Spat .... SECURE / UNDAMAGED
[ ]  Tyre .... INFLATED – MARK ALIGNED
[ ]  Chocks .... REMOVED
[ ]  Wing Tip & Light .... UNDAMAGED
[ ]  Tiedown .... REMOVED
[ ]  Pitot Mast .... CLEAR / UNDAMAGED
[ ]  Aileron .... FREEDOM OF MOVEMENT
[ ]  Flap .... SECURE & UNDAMAGED

Empennage
[ ]  Aerials .... SECURE
[ ]  Static Vent (each side) .... CLEAR
[ ]  Stabilators .... FREEDOM OF MOVEMENT
[ ]  Rudder .... VISUAL CHECK ONLY
[ ]  Anti-Balance / Trim .... SECURE, DAMAGE
[ ]  Tail Cone & Light .... SECURE, UNDAMAGED
[ ]  Tie Down .... REMOVED

Starboard Wing
[ ]  Flap .... SECURE / UNDAMAGED
[ ]  Aileron .... FREEDOM OF MOVEMENT
[ ]  Wing Tip & Light .... UNDAMAGED
[ ]  Tiedown .... REMOVED
[ ]  Fuel Tank .... DIP, CAP SECURE
[ ]  Tank Drain .... DRAIN, SECURE
[ ]  Fuel Sample .... PROPER COLOR
[ ]  Gear, Spat .... SECURE / UNDAMAGED
[ ]  Tyre .... INFLATED – MARK ALIGNED
[ ]  Chocks .... REMOVED

Nose
[ ]  Engine Oil Level .... 6 Qts. MIN, 8 Qts MAX
[ ]  Engine Oil Dipstick .... SECURE
[ ]  Cowling .... SECURE, UNDAMAGED
[ ]  Prop / Spinner .... SECURE, UNDAMAGED
[ ]  Alternator Belt .... PROPER TENSION
[ ]  Nose Oleo .... NO LEAKS / NORMAL
[ ]  Spat / Tyre .... CONDITION / DAMAGE
[ ]  Tow Bar .... REMOVED & STOWED
[ ]  Chocks .... REMOVED
[ ]  Fuel Sump Drain .... DRAIN, SECURE

Before Starting Engine
[ ]  Preflight Inspection .... COMPLETE
[ ]  Flaps .... UP IN STAGES
[ ]  Canopy .... CLOSED / LOCKED
[ ]  Controls .... FULL & FREE MOVEMENT
[ ]  Elevator Trim .... FULL TRAVEL – NEUTRAL
[ ]  Fuel Selector Valve .... EMPTIEST TANK
[ ]  Seats, Harnesses .... ADJUSTED, LOCKED
[ ]  Radio, Electrical Equipment .... OFF
[ ]  Parking Brake .... SET
[ ]  Circuit Breakers .... CHECK
[ ]  Anti-Collision Beacon .... ON

Engine Start (COLD)
[ ]  Master Switch .... ON
[ ]  Mixture .... FULL RICH
[ ]  Fuel Pump .... ON
[ ]  Fuel Pressure .... CHECK
[ ]  Carburettor Heat .... FREE MOVEMENT - COLD
[ ]  Prime .... AS REQUIRED
[ ]  Throttle .... OPEN ¼ INCH
[ ]  Propeller .... CLEAR
[ ]  Magnetos .... START
[ ]  Starter Engaged Light .... OUT
[ ]  Oil Pressure .... CHECK 25 psi MIN
[ ]  Engine .... WARM UP 1200 RPM
[ ]  Brakes .... HOLDING
[ ]  Low Volts Light .... OUT
[ ]  Ammeter .... CHARGING
[ ]  Suction .... REGISTERING
[ ]  Radios .... COM 1 ON
[ ]  NAV 1 .... ON
[ ]  COM 2 .... ON
[ ]  DME .... ON
[ ]  Transponder .... STANDBY
[ ]  NAV 2 .... ON
[ ]  GPS .... ON

Before Taxi
[ ]  Radios .... CHECK VOLUME
[ ]  Gyros .... ERECTED
[ ]  DI .... ALIGN WITH COMPASS
[ ]  Altimeters .... SET QFE / QNH
[ ]  Nav Lights .... AS REQUIRED
[ ]  Taxi Light .... ON
[ ]  Radio Check / Taxi Clearance .... OBTAIN
[ ]  Parking Brake .... OFF

Taxi Checks
[ ]  Brakes / Nosewheel Steering .... TEST
[ ]  Compass .... SWINGING FREELY
[ ]  DI .... TURNING CORRECTLY
[ ]  AI .... MOVING CORRECTLY
[ ]  Turn / Slip .... MOVING CORRECTLY
[ ]  ASI .... REGISTERING
[ ]  Nav Aids .... REGISTERING

Power Checks
[ ]  Parking Brake .... SET
[ ]  Fuel Pump .... ON
[ ]  Fuel Pressure .... GREEN ARC
[ ]  Fuel Selector .... FULLEST TANK
[ ]  Fuel Pump .... OFF
[ ]  Fuel Pressure .... GREEN ARC
[ ]  Oil Temperature .... YELLOW ARC MIN
[ ]  Oil Pressure .... CHECK 25 psi MIN
[ ]  Area Behind .... CLEAR
[ ]  Throttle .... GENTLY INCREASE - 2000 RPM
[ ]  Carburettor Heat .... HOT, CHECK RPM, COLD
[ ]  Magnetos .... CHECK (150 RPM Max drop, 50 RPM diff.)
[ ]  Suction .... IN WHITE ARC
[ ]  Oil Temperature .... YELLOW ARC MIN
[ ]  Oil Pressure .... CHECK 25 psi MIN
[ ]  Throttle - Idle .... 500 – 700 RPM
[ ]  Throttle .... 1200 RPM SET

Pre-Takeoff
[ ]  Elevator Trim .... SET NEUTRAL
[ ]  Flaps .... 15° (NORMAL)
[ ]  Fuel Contents .... SUFFICIENT
[ ]  Carburettor Heat .... COLD
[ ]  Primer .... LOCKED
[ ]  Throttle Friction .... FINGER TIGHT
[ ]  Mixture .... FULL RICH
[ ]  Magnetos .... BOTH
[ ]  DI .... ALIGN WITH COMPASS
[ ]  Altimeters .... SET QFE / QNH
[ ]  Radio Aids .... TUNE / IDENT
[ ]  Engine Temps & Pressure .... NORMAL
[ ]  Fuel Pump .... ON
[ ]  Pitot Heater .... AS REQUIRED
[ ]  Nav Lights .... AS REQUIRED
[ ]  Flight Controls .... FULL & FREE
[ ]  Hatches and Harnesses .... SECURE
[ ]  Parking Brake .... OFF
[ ]  Transponder .... ON-ALT
[ ]  Departure Clearance .... OBTAIN

Normal Takeoff
[ ]  Flaps .... 15° (NORMAL)
[ ]  Carburettor Heat .... COLD
[ ]  Fuel Pump .... ON
[ ]  DI .... ALIGNED WITH RUNWAY
[ ]  Engine Temps & Pressure .... NORMAL
[ ]  Throttle .... FULL OPEN
[ ]  Rotate .... 55 kts
[ ]  Climb Speed .... 71 kts
[ ]  Flaps .... RETRACT 300ft MIN
[ ]  Top of Climb .... FREDAL CHECKS

Short Field / Obstacle Clearance
[ ]  Flaps .... 25° (Second Notch)
[ ]  Carburetor Heat .... COLD
[ ]  Fuel Pump .... ON
[ ]  Throttle .... FULL OPEN
[ ]  Rotate .... 55-60 kts
[ ]  Initial Climb Speed .... 71 kts

Climb
[ ]  Normal Climb .... 75 kts
[ ]  VY – Best Rate of Climb Speed .... 71 kts
[ ]  VX – Best Angle of Climb Speed .... 65 kts

Cruise
[ ]  Fuel Pump .... OFF
[ ]  Power .... 2200-2600 RPM
[ ]  Elevator Trim .... SET
[ ]  Taxi Light .... OFF
[ ]  Mixture .... LEAN (MAX 200°C EGT)
[ ]  Fuel Selector .... SWITCH AS NEEDED

Before Landing
[ ]  Parking Brake .... OFF
[ ]  Mixture .... FULL RICH
[ ]  Magnetos .... BOTH
[ ]  Fuel Pump .... ON
[ ]  Fuel Selector .... FULLEST TANK
[ ]  Engine Temps & Pressure .... NORMAL
[ ]  Carburettor Heat .... HOT
[ ]  Seats / Harnesses .... ADJUSTED / LOCKED
[ ]  Airspeed .... IN WHITE ARC
[ ]  Flaps .... AS REQUIRED
[ ]  Airspeed .... 80 kts
[ ]  Elevator Trim .... SET
[ ]  Landing Light .... ON AS REQUIRED

Finals Checks
[ ]  Carburettor Heat .... COLD
[ ]  Runway .... CLEAR
[ ]  Approach .... SPEED & ANGLE OK
[ ]  Permissions .... LANDING CLEARANCE

After Landing
[ ]  Flaps .... UP
[ ]  Fuel Pump .... OFF
[ ]  Landing Light .... OFF
[ ]  Carburettor Heat .... OFF
[ ]  Transponder .... OFF

Shut-Down, Securing Aeroplane
[ ]  Magnetos .... CHECK LEFT / RIGHT
[ ]  Electrical Equipment, Lights .... OFF
[ ]  COM 1/2, NAV 1/2, DME, Xpdr, GPS .... OFF
[ ]  Throttle .... IDLE
[ ]  Mixture .... IDLE CUT-OFF
[ ]  Ignition .... OFF
[ ]  Master Switch .... OFF
[ ]  Parking Brake .... SET (IF REQUIRED)
[ ]  Chocks/Tiedowns .... INSTALLED

Specifications
[ ]  Maximum Gross Weight .... 2335 lbs
[ ]  Basic Empty Weight .... 1575 lbs
[ ]  Payload With Full Fuel .... 448 lbs
[ ]  Fuel Flow @ 75% Power .... 8 gph
[ ]  Total Fuel Capacity .... 52 gal
[ ]  Fuel Octane .... 100LL (Blue)
[ ]  Oil Sump Capacity .... 8 qts
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